(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "74xx:74LS00" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 1.27 0))
      (property "Value" "74LS00" (at 0 -1.27 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls00" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "TTL nand 2-input" (at 0 0 0))
      (property "ki_description" "quad 2-input NAND gate" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SO14*" (at 0 0 0))
      (symbol "74LS00_1_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS00_1_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "1")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "2")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS00_2_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS00_2_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "4")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "5")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS00_3_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS00_3_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "10")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS00_4_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS00_4_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "12")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS00_5_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS00_5_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74LS05" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 1.27 0))
      (property "Value" "74LS05" (at 0 -1.27 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS05" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "TTL not inv OpenCol" (at 0 0 0))
      (property "ki_description" "Inverter Open Collect" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (at 0 0 0))
      (symbol "74LS05_1_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74LS05_2_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74LS05_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS05_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS05_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74LS05_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS05_7_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS05_7_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x40_Counter_Clockwise" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 1.27 50.8 0))
      (property "Value" "Conn_02x40_Counter_Clockwise" (at 1.27 -53.34 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x40, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (at 0 0 0))
      (symbol "Conn_02x40_Counter_Clockwise_1_1"
        (rectangle (start -1.27 -50.673) (end 0 -50.927)
          (fill (type none))
        )
        (rectangle (start -1.27 -48.133) (end 0 -48.387)
          (fill (type none))
        )
        (rectangle (start -1.27 -45.593) (end 0 -45.847)
          (fill (type none))
        )
        (rectangle (start -1.27 -43.053) (end 0 -43.307)
          (fill (type none))
        )
        (rectangle (start -1.27 -40.513) (end 0 -40.767)
          (fill (type none))
        )
        (rectangle (start -1.27 -37.973) (end 0 -38.227)
          (fill (type none))
        )
        (rectangle (start -1.27 -35.433) (end 0 -35.687)
          (fill (type none))
        )
        (rectangle (start -1.27 -32.893) (end 0 -33.147)
          (fill (type none))
        )
        (rectangle (start -1.27 -30.353) (end 0 -30.607)
          (fill (type none))
        )
        (rectangle (start -1.27 -27.813) (end 0 -28.067)
          (fill (type none))
        )
        (rectangle (start -1.27 -25.273) (end 0 -25.527)
          (fill (type none))
        )
        (rectangle (start -1.27 -22.733) (end 0 -22.987)
          (fill (type none))
        )
        (rectangle (start -1.27 -20.193) (end 0 -20.447)
          (fill (type none))
        )
        (rectangle (start -1.27 -17.653) (end 0 -17.907)
          (fill (type none))
        )
        (rectangle (start -1.27 -15.113) (end 0 -15.367)
          (fill (type none))
        )
        (rectangle (start -1.27 -12.573) (end 0 -12.827)
          (fill (type none))
        )
        (rectangle (start -1.27 -10.033) (end 0 -10.287)
          (fill (type none))
        )
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 10.287) (end 0 10.033)
          (fill (type none))
        )
        (rectangle (start -1.27 12.827) (end 0 12.573)
          (fill (type none))
        )
        (rectangle (start -1.27 15.367) (end 0 15.113)
          (fill (type none))
        )
        (rectangle (start -1.27 17.907) (end 0 17.653)
          (fill (type none))
        )
        (rectangle (start -1.27 20.447) (end 0 20.193)
          (fill (type none))
        )
        (rectangle (start -1.27 22.987) (end 0 22.733)
          (fill (type none))
        )
        (rectangle (start -1.27 25.527) (end 0 25.273)
          (fill (type none))
        )
        (rectangle (start -1.27 28.067) (end 0 27.813)
          (fill (type none))
        )
        (rectangle (start -1.27 30.607) (end 0 30.353)
          (fill (type none))
        )
        (rectangle (start -1.27 33.147) (end 0 32.893)
          (fill (type none))
        )
        (rectangle (start -1.27 35.687) (end 0 35.433)
          (fill (type none))
        )
        (rectangle (start -1.27 38.227) (end 0 37.973)
          (fill (type none))
        )
        (rectangle (start -1.27 40.767) (end 0 40.513)
          (fill (type none))
        )
        (rectangle (start -1.27 43.307) (end 0 43.053)
          (fill (type none))
        )
        (rectangle (start -1.27 45.847) (end 0 45.593)
          (fill (type none))
        )
        (rectangle (start -1.27 48.387) (end 0 48.133)
          (fill (type none))
        )
        (rectangle (start -1.27 49.53) (end 3.81 -52.07)
          (fill (type background))
        )
        (rectangle (start 3.81 -50.673) (end 2.54 -50.927)
          (fill (type none))
        )
        (rectangle (start 3.81 -48.133) (end 2.54 -48.387)
          (fill (type none))
        )
        (rectangle (start 3.81 -45.593) (end 2.54 -45.847)
          (fill (type none))
        )
        (rectangle (start 3.81 -43.053) (end 2.54 -43.307)
          (fill (type none))
        )
        (rectangle (start 3.81 -40.513) (end 2.54 -40.767)
          (fill (type none))
        )
        (rectangle (start 3.81 -37.973) (end 2.54 -38.227)
          (fill (type none))
        )
        (rectangle (start 3.81 -35.433) (end 2.54 -35.687)
          (fill (type none))
        )
        (rectangle (start 3.81 -32.893) (end 2.54 -33.147)
          (fill (type none))
        )
        (rectangle (start 3.81 -30.353) (end 2.54 -30.607)
          (fill (type none))
        )
        (rectangle (start 3.81 -27.813) (end 2.54 -28.067)
          (fill (type none))
        )
        (rectangle (start 3.81 -25.273) (end 2.54 -25.527)
          (fill (type none))
        )
        (rectangle (start 3.81 -22.733) (end 2.54 -22.987)
          (fill (type none))
        )
        (rectangle (start 3.81 -20.193) (end 2.54 -20.447)
          (fill (type none))
        )
        (rectangle (start 3.81 -17.653) (end 2.54 -17.907)
          (fill (type none))
        )
        (rectangle (start 3.81 -15.113) (end 2.54 -15.367)
          (fill (type none))
        )
        (rectangle (start 3.81 -12.573) (end 2.54 -12.827)
          (fill (type none))
        )
        (rectangle (start 3.81 -10.033) (end 2.54 -10.287)
          (fill (type none))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (rectangle (start 3.81 10.287) (end 2.54 10.033)
          (fill (type none))
        )
        (rectangle (start 3.81 12.827) (end 2.54 12.573)
          (fill (type none))
        )
        (rectangle (start 3.81 15.367) (end 2.54 15.113)
          (fill (type none))
        )
        (rectangle (start 3.81 17.907) (end 2.54 17.653)
          (fill (type none))
        )
        (rectangle (start 3.81 20.447) (end 2.54 20.193)
          (fill (type none))
        )
        (rectangle (start 3.81 22.987) (end 2.54 22.733)
          (fill (type none))
        )
        (rectangle (start 3.81 25.527) (end 2.54 25.273)
          (fill (type none))
        )
        (rectangle (start 3.81 28.067) (end 2.54 27.813)
          (fill (type none))
        )
        (rectangle (start 3.81 30.607) (end 2.54 30.353)
          (fill (type none))
        )
        (rectangle (start 3.81 33.147) (end 2.54 32.893)
          (fill (type none))
        )
        (rectangle (start 3.81 35.687) (end 2.54 35.433)
          (fill (type none))
        )
        (rectangle (start 3.81 38.227) (end 2.54 37.973)
          (fill (type none))
        )
        (rectangle (start 3.81 40.767) (end 2.54 40.513)
          (fill (type none))
        )
        (rectangle (start 3.81 43.307) (end 2.54 43.053)
          (fill (type none))
        )
        (rectangle (start 3.81 45.847) (end 2.54 45.593)
          (fill (type none))
        )
        (rectangle (start 3.81 48.387) (end 2.54 48.133)
          (fill (type none))
        )
        (pin passive line (at -5.08 48.26 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 25.4 0) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 22.86 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at -5.08 20.32 0) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 17.78 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at -5.08 15.24 0) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "Pin_15")
          (number "15")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "Pin_16")
          (number "16")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_17")
          (number "17")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_18")
          (number "18")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_19")
          (number "19")
        )
        (pin passive line (at -5.08 45.72 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_20")
          (number "20")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_21")
          (number "21")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_22")
          (number "22")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_23")
          (number "23")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_24")
          (number "24")
        )
        (pin passive line (at -5.08 -12.7 0) (length 3.81)
          (name "Pin_25")
          (number "25")
        )
        (pin passive line (at -5.08 -15.24 0) (length 3.81)
          (name "Pin_26")
          (number "26")
        )
        (pin passive line (at -5.08 -17.78 0) (length 3.81)
          (name "Pin_27")
          (number "27")
        )
        (pin passive line (at -5.08 -20.32 0) (length 3.81)
          (name "Pin_28")
          (number "28")
        )
        (pin passive line (at -5.08 -22.86 0) (length 3.81)
          (name "Pin_29")
          (number "29")
        )
        (pin passive line (at -5.08 43.18 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at -5.08 -25.4 0) (length 3.81)
          (name "Pin_30")
          (number "30")
        )
        (pin passive line (at -5.08 -27.94 0) (length 3.81)
          (name "Pin_31")
          (number "31")
        )
        (pin passive line (at -5.08 -30.48 0) (length 3.81)
          (name "Pin_32")
          (number "32")
        )
        (pin passive line (at -5.08 -33.02 0) (length 3.81)
          (name "Pin_33")
          (number "33")
        )
        (pin passive line (at -5.08 -35.56 0) (length 3.81)
          (name "Pin_34")
          (number "34")
        )
        (pin passive line (at -5.08 -38.1 0) (length 3.81)
          (name "Pin_35")
          (number "35")
        )
        (pin passive line (at -5.08 -40.64 0) (length 3.81)
          (name "Pin_36")
          (number "36")
        )
        (pin passive line (at -5.08 -43.18 0) (length 3.81)
          (name "Pin_37")
          (number "37")
        )
        (pin passive line (at -5.08 -45.72 0) (length 3.81)
          (name "Pin_38")
          (number "38")
        )
        (pin passive line (at -5.08 -48.26 0) (length 3.81)
          (name "Pin_39")
          (number "39")
        )
        (pin passive line (at -5.08 40.64 0) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 -50.8 0) (length 3.81)
          (name "Pin_40")
          (number "40")
        )
        (pin passive line (at 7.62 -50.8 180) (length 3.81)
          (name "Pin_41")
          (number "41")
        )
        (pin passive line (at 7.62 -48.26 180) (length 3.81)
          (name "Pin_42")
          (number "42")
        )
        (pin passive line (at 7.62 -45.72 180) (length 3.81)
          (name "Pin_43")
          (number "43")
        )
        (pin passive line (at 7.62 -43.18 180) (length 3.81)
          (name "Pin_44")
          (number "44")
        )
        (pin passive line (at 7.62 -40.64 180) (length 3.81)
          (name "Pin_45")
          (number "45")
        )
        (pin passive line (at 7.62 -38.1 180) (length 3.81)
          (name "Pin_46")
          (number "46")
        )
        (pin passive line (at 7.62 -35.56 180) (length 3.81)
          (name "Pin_47")
          (number "47")
        )
        (pin passive line (at 7.62 -33.02 180) (length 3.81)
          (name "Pin_48")
          (number "48")
        )
        (pin passive line (at 7.62 -30.48 180) (length 3.81)
          (name "Pin_49")
          (number "49")
        )
        (pin passive line (at -5.08 38.1 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 -27.94 180) (length 3.81)
          (name "Pin_50")
          (number "50")
        )
        (pin passive line (at 7.62 -25.4 180) (length 3.81)
          (name "Pin_51")
          (number "51")
        )
        (pin passive line (at 7.62 -22.86 180) (length 3.81)
          (name "Pin_52")
          (number "52")
        )
        (pin passive line (at 7.62 -20.32 180) (length 3.81)
          (name "Pin_53")
          (number "53")
        )
        (pin passive line (at 7.62 -17.78 180) (length 3.81)
          (name "Pin_54")
          (number "54")
        )
        (pin passive line (at 7.62 -15.24 180) (length 3.81)
          (name "Pin_55")
          (number "55")
        )
        (pin passive line (at 7.62 -12.7 180) (length 3.81)
          (name "Pin_56")
          (number "56")
        )
        (pin passive line (at 7.62 -10.16 180) (length 3.81)
          (name "Pin_57")
          (number "57")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_58")
          (number "58")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_59")
          (number "59")
        )
        (pin passive line (at -5.08 35.56 0) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_60")
          (number "60")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_61")
          (number "61")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_62")
          (number "62")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_63")
          (number "63")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_64")
          (number "64")
        )
        (pin passive line (at 7.62 10.16 180) (length 3.81)
          (name "Pin_65")
          (number "65")
        )
        (pin passive line (at 7.62 12.7 180) (length 3.81)
          (name "Pin_66")
          (number "66")
        )
        (pin passive line (at 7.62 15.24 180) (length 3.81)
          (name "Pin_67")
          (number "67")
        )
        (pin passive line (at 7.62 17.78 180) (length 3.81)
          (name "Pin_68")
          (number "68")
        )
        (pin passive line (at 7.62 20.32 180) (length 3.81)
          (name "Pin_69")
          (number "69")
        )
        (pin passive line (at -5.08 33.02 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 22.86 180) (length 3.81)
          (name "Pin_70")
          (number "70")
        )
        (pin passive line (at 7.62 25.4 180) (length 3.81)
          (name "Pin_71")
          (number "71")
        )
        (pin passive line (at 7.62 27.94 180) (length 3.81)
          (name "Pin_72")
          (number "72")
        )
        (pin passive line (at 7.62 30.48 180) (length 3.81)
          (name "Pin_73")
          (number "73")
        )
        (pin passive line (at 7.62 33.02 180) (length 3.81)
          (name "Pin_74")
          (number "74")
        )
        (pin passive line (at 7.62 35.56 180) (length 3.81)
          (name "Pin_75")
          (number "75")
        )
        (pin passive line (at 7.62 38.1 180) (length 3.81)
          (name "Pin_76")
          (number "76")
        )
        (pin passive line (at 7.62 40.64 180) (length 3.81)
          (name "Pin_77")
          (number "77")
        )
        (pin passive line (at 7.62 43.18 180) (length 3.81)
          (name "Pin_78")
          (number "78")
        )
        (pin passive line (at 7.62 45.72 180) (length 3.81)
          (name "Pin_79")
          (number "79")
        )
        (pin passive line (at -5.08 30.48 0) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at 7.62 48.26 180) (length 3.81)
          (name "Pin_80")
          (number "80")
        )
        (pin passive line (at -5.08 27.94 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Priority_Encoder:74HC148" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 12.7 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "74HC148_0_1"
        (rectangle (start -5.08 8.89) (end 5.08 -11.43)
          (fill (type background))
        )
        (text "74HC148" (at 0 10.16 0))
      )
      (symbol "74HC148_1_1"
        (pin input line (at -7.62 7.62 0) (length 2.54)
          (name "4")
          (number "1")
        )
        (pin input line (at 7.62 -7.62 180) (length 2.54)
          (name "0")
          (number "10")
        )
        (pin input line (at 7.62 -5.08 180) (length 2.54)
          (name "1")
          (number "11")
        )
        (pin input line (at 7.62 -2.54 180) (length 2.54)
          (name "2")
          (number "12")
        )
        (pin input line (at 7.62 0 180) (length 2.54)
          (name "3")
          (number "13")
        )
        (pin output line (at 7.62 2.54 180) (length 2.54)
          (name "GS")
          (number "14")
        )
        (pin output line (at 7.62 5.08 180) (length 2.54)
          (name "EO")
          (number "15")
        )
        (pin power_in line (at 7.62 7.62 180) (length 2.54)
          (name "Vcc")
          (number "16")
        )
        (pin input line (at -7.62 5.08 0) (length 2.54)
          (name "5")
          (number "2")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "6")
          (number "3")
        )
        (pin input line (at -7.62 0 0) (length 2.54)
          (name "7")
          (number "4")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "EI")
          (number "5")
        )
        (pin output line (at -7.62 -5.08 0) (length 2.54)
          (name "A2")
          (number "6")
        )
        (pin output line (at -7.62 -7.62 0) (length 2.54)
          (name "A1")
          (number "7")
        )
        (pin power_in line (at -7.62 -10.16 0) (length 2.54)
          (name "GND")
          (number "8")
        )
        (pin output line (at 7.62 -10.16 180) (length 2.54)
          (name "A0")
          (number "9")
        )
      )
    )
    (symbol "SRAM:AS6C62256-55PCN" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 20.32 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "AS6C62256-55PCN_0_1"
        (rectangle (start -7.62 16.51) (end 8.89 -19.05)
          (fill (type background))
        )
        (text "AS6C62256-55PCN" (at 0 17.78 0))
      )
      (symbol "AS6C62256-55PCN_1_1"
        (pin input line (at -10.16 15.24 0) (length 2.54)
          (name "A14")
          (number "1")
        )
        (pin input line (at -10.16 -7.62 0) (length 2.54)
          (name "A0")
          (number "10")
        )
        (pin bidirectional line (at -10.16 -10.16 0) (length 2.54)
          (name "DQ0")
          (number "11")
        )
        (pin bidirectional line (at -10.16 -12.7 0) (length 2.54)
          (name "DQ1")
          (number "12")
        )
        (pin bidirectional line (at -10.16 -15.24 0) (length 2.54)
          (name "DQ2")
          (number "13")
        )
        (pin power_in line (at -10.16 -17.78 0) (length 2.54)
          (name "Vss")
          (number "14")
        )
        (pin input line (at 11.43 -17.78 180) (length 2.54)
          (name "DQ3")
          (number "15")
        )
        (pin input line (at 11.43 -15.24 180) (length 2.54)
          (name "DQ4")
          (number "16")
        )
        (pin input line (at 11.43 -12.7 180) (length 2.54)
          (name "DQ5")
          (number "17")
        )
        (pin input line (at 11.43 -10.16 180) (length 2.54)
          (name "DQ6")
          (number "18")
        )
        (pin input line (at 11.43 -7.62 180) (length 2.54)
          (name "DQ7")
          (number "19")
        )
        (pin input line (at -10.16 12.7 0) (length 2.54)
          (name "A12")
          (number "2")
        )
        (pin input inverted (at 11.43 -5.08 180) (length 2.54)
          (name "CE#")
          (number "20")
        )
        (pin input line (at 11.43 -2.54 180) (length 2.54)
          (name "A10")
          (number "21")
        )
        (pin input inverted (at 11.43 0 180) (length 2.54)
          (name "OE#")
          (number "22")
        )
        (pin input line (at 11.43 2.54 180) (length 2.54)
          (name "A11")
          (number "23")
        )
        (pin input line (at 11.43 5.08 180) (length 2.54)
          (name "A9")
          (number "24")
        )
        (pin input line (at 11.43 7.62 180) (length 2.54)
          (name "A8")
          (number "25")
        )
        (pin input line (at 11.43 10.16 180) (length 2.54)
          (name "A13")
          (number "26")
        )
        (pin input inverted (at 11.43 12.7 180) (length 2.54)
          (name "WE#")
          (number "27")
        )
        (pin power_in line (at 11.43 15.24 180) (length 2.54)
          (name "Vcc")
          (number "28")
        )
        (pin input line (at -10.16 10.16 0) (length 2.54)
          (name "A7")
          (number "3")
        )
        (pin input line (at -10.16 7.62 0) (length 2.54)
          (name "A6")
          (number "4")
        )
        (pin input line (at -10.16 5.08 0) (length 2.54)
          (name "A5")
          (number "5")
        )
        (pin input line (at -10.16 2.54 0) (length 2.54)
          (name "A4")
          (number "6")
        )
        (pin input line (at -10.16 0 0) (length 2.54)
          (name "A3")
          (number "7")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "A2")
          (number "8")
        )
        (pin input line (at -10.16 -5.08 0) (length 2.54)
          (name "A1")
          (number "9")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 222.25 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 143.51) (diameter 0) (color 0 0 0 0))
  (junction (at 66.04 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 219.71 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 138.43) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 82.55) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 128.27) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 66.04 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 57.15) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 69.85) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 46.99) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 59.69) (diameter 0) (color 0 0 0 0))
  (junction (at 219.71 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 29.21 113.03) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 110.49) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 52.07) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 203.2 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 67.31) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 222.25 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 77.47) (diameter 0) (color 0 0 0 0))
  (junction (at 29.21 115.57) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 105.41) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 49.53) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 135.89) (diameter 0) (color 0 0 0 0))
  (junction (at 124.46 53.34) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 97.79) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 107.95) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 133.35) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 130.81) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 115.57) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 95.25) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 62.23) (diameter 0) (color 0 0 0 0))
  (junction (at 99.06 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 120.65) (diameter 0) (color 0 0 0 0))
  (junction (at 99.06 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 123.19) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 118.11) (diameter 0) (color 0 0 0 0))
  (junction (at 224.79 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 224.79 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 16.51 146.05) (diameter 0) (color 0 0 0 0))
  (bus_entry (at 209.55 106.68) (size 2.54 -2.54))
  (bus_entry (at 40.64 146.05) (size 2.54 -2.54))
  (bus_entry (at 40.64 54.61) (size 2.54 -2.54))
  (bus_entry (at 209.55 116.84) (size 2.54 -2.54))
  (bus_entry (at 190.5 96.52) (size 2.54 2.54))
  (bus_entry (at 40.64 133.35) (size 2.54 -2.54))
  (bus_entry (at 40.64 97.79) (size 2.54 -2.54))
  (bus_entry (at 209.55 109.22) (size 2.54 -2.54))
  (bus_entry (at 158.75 86.36) (size -2.54 2.54))
  (bus_entry (at 190.5 99.06) (size 2.54 -2.54))
  (bus_entry (at 190.5 91.44) (size 2.54 -2.54))
  (bus_entry (at 40.64 135.89) (size 2.54 -2.54))
  (bus_entry (at 40.64 57.15) (size 2.54 -2.54))
  (bus_entry (at 40.64 118.11) (size 2.54 -2.54))
  (bus_entry (at 158.75 96.52) (size -2.54 2.54))
  (bus_entry (at 40.64 120.65) (size 2.54 -2.54))
  (bus_entry (at 95.25 60.96) (size 2.54 -2.54))
  (bus_entry (at 40.64 138.43) (size 2.54 -2.54))
  (bus_entry (at 40.64 128.27) (size 2.54 -2.54))
  (bus_entry (at 40.64 123.19) (size 2.54 -2.54))
  (bus_entry (at 95.25 55.88) (size 2.54 -2.54))
  (bus_entry (at 40.64 102.87) (size 2.54 -2.54))
  (bus_entry (at 40.64 140.97) (size 2.54 -2.54))
  (bus_entry (at 134.62 43.18) (size 2.54 2.54))
  (bus_entry (at 132.08 43.18) (size 2.54 2.54))
  (bus_entry (at 209.55 111.76) (size 2.54 -2.54))
  (bus_entry (at 40.64 125.73) (size 2.54 -2.54))
  (bus_entry (at 209.55 114.3) (size 2.54 -2.54))
  (bus_entry (at 40.64 105.41) (size 2.54 -2.54))
  (bus_entry (at 95.25 63.5) (size 2.54 -2.54))
  (bus_entry (at 40.64 100.33) (size 2.54 -2.54))
  (bus_entry (at 158.75 104.14) (size -2.54 2.54))
  (bus_entry (at 209.55 104.14) (size 2.54 -2.54))
  (bus_entry (at 158.75 99.06) (size -2.54 2.54))
  (bus_entry (at 137.16 43.18) (size 2.54 2.54))
  (bus_entry (at 40.64 49.53) (size 2.54 -2.54))
  (bus_entry (at 40.64 107.95) (size 2.54 -2.54))
  (bus_entry (at 158.75 93.98) (size -2.54 2.54))
  (bus_entry (at 158.75 88.9) (size -2.54 2.54))
  (bus_entry (at 40.64 64.77) (size 2.54 -2.54))
  (bus_entry (at 40.64 130.81) (size 2.54 -2.54))
  (bus_entry (at 190.5 93.98) (size 2.54 -2.54))
  (bus_entry (at 40.64 92.71) (size 2.54 -2.54))
  (bus_entry (at 209.55 121.92) (size 2.54 -2.54))
  (bus_entry (at 209.55 119.38) (size 2.54 -2.54))
  (bus_entry (at 40.64 143.51) (size 2.54 -2.54))
  (bus_entry (at 40.64 62.23) (size 2.54 -2.54))
  (bus_entry (at 95.25 58.42) (size 2.54 -2.54))
  (bus_entry (at 158.75 101.6) (size -2.54 2.54))
  (bus_entry (at 40.64 46.99) (size 2.54 -2.54))
  (bus_entry (at 190.5 88.9) (size 2.54 -2.54))
  (bus_entry (at 158.75 91.44) (size -2.54 2.54))
  (bus_entry (at 40.64 95.25) (size 2.54 -2.54))
  (bus_entry (at 40.64 52.07) (size 2.54 -2.54))
  (bus_entry (at 40.64 59.69) (size 2.54 -2.54))
  (wire (pts (xy 60.96 44.45) (xy 60.96 41.91)))
  (wire (pts (xy 224.79 106.68) (xy 233.68 106.68)))
  (wire (pts (xy 134.62 60.96) (xy 134.62 45.72)))
  (bus (pts (xy 43.18 90.17) (xy 95.25 90.17)))
  (wire (pts (xy 111.76 80.01) (xy 99.06 80.01)))
  (bus (pts (xy 156.21 88.9) (xy 156.21 91.44)))
  (wire (pts (xy 97.79 58.42) (xy 107.95 58.42)))
  (wire (pts (xy 219.71 81.28) (xy 222.25 81.28)))
  (bus (pts (xy 43.18 115.57) (xy 43.18 118.11)))
  (wire (pts (xy 99.06 63.5) (xy 99.06 71.12)))
  (wire (pts (xy 224.79 97.79) (xy 224.79 106.68)))
  (bus (pts (xy 43.18 97.79) (xy 43.18 95.25)))
  (wire (pts (xy 163.83 111.76) (xy 166.37 111.76)))
  (wire (pts (xy 187.96 88.9) (xy 190.5 88.9)))
  (wire (pts (xy 158.75 86.36) (xy 166.37 86.36)))
  (wire (pts (xy 102.87 66.04) (xy 102.87 76.2)))
  (wire (pts (xy 132.08 53.34) (xy 132.08 68.58)))
  (bus (pts (xy 43.18 140.97) (xy 43.18 143.51)))
  (wire (pts (xy 29.21 140.97) (xy 40.64 140.97)))
  (wire (pts (xy 16.51 125.73) (xy 16.51 128.27)))
  (wire (pts (xy 161.29 109.22) (xy 166.37 109.22)))
  (bus (pts (xy 156.21 91.44) (xy 156.21 93.98)))
  (wire (pts (xy 105.41 68.58) (xy 105.41 73.66)))
  (wire (pts (xy 163.83 71.12) (xy 163.83 83.82)))
  (bus (pts (xy 95.25 55.88) (xy 95.25 43.18)))
  (wire (pts (xy 29.21 118.11) (xy 40.64 118.11)))
  (wire (pts (xy 16.51 107.95) (xy 16.51 110.49)))
  (wire (pts (xy 60.96 55.88) (xy 66.04 55.88)))
  (wire (pts (xy 16.51 113.03) (xy 16.51 115.57)))
  (bus (pts (xy 43.18 46.99) (xy 43.18 44.45)))
  (bus (pts (xy 193.04 68.58) (xy 156.21 68.58)))
  (bus (pts (xy 212.09 104.14) (xy 212.09 106.68)))
  (bus (pts (xy 43.18 133.35) (xy 43.18 135.89)))
  (bus (pts (xy 43.18 92.71) (xy 43.18 90.17)))
  (wire (pts (xy 16.51 54.61) (xy 16.51 57.15)))
  (bus (pts (xy 193.04 91.44) (xy 193.04 96.52)))
  (wire (pts (xy 187.96 93.98) (xy 190.5 93.98)))
  (wire (pts (xy 123.19 63.5) (xy 137.16 63.5)))
  (wire (pts (xy 163.83 83.82) (xy 166.37 83.82)))
  (wire (pts (xy 124.46 80.01) (xy 124.46 53.34)))
  (wire (pts (xy 209.55 121.92) (xy 158.75 121.92)))
  (wire (pts (xy 45.72 46.99) (xy 45.72 72.39)))
  (bus (pts (xy 134.62 43.18) (xy 137.16 43.18)))
  (wire (pts (xy 187.96 109.22) (xy 209.55 109.22)))
  (wire (pts (xy 29.21 130.81) (xy 40.64 130.81)))
  (wire (pts (xy 16.51 118.11) (xy 16.51 120.65)))
  (wire (pts (xy 105.41 73.66) (xy 190.5 73.66)))
  (wire (pts (xy 29.21 143.51) (xy 40.64 143.51)))
  (wire (pts (xy 119.38 80.01) (xy 124.46 80.01)))
  (wire (pts (xy 16.51 130.81) (xy 16.51 133.35)))
  (wire (pts (xy 200.66 58.42) (xy 200.66 101.6)))
  (bus (pts (xy 212.09 114.3) (xy 212.09 116.84)))
  (wire (pts (xy 207.01 83.82) (xy 203.2 83.82)))
  (wire (pts (xy 29.21 74.93) (xy 48.26 74.93)))
  (bus (pts (xy 156.21 99.06) (xy 156.21 101.6)))
  (wire (pts (xy 166.37 124.46) (xy 166.37 114.3)))
  (bus (pts (xy 156.21 96.52) (xy 156.21 99.06)))
  (wire (pts (xy 203.2 83.82) (xy 187.96 83.82)))
  (wire (pts (xy 29.21 92.71) (xy 40.64 92.71)))
  (wire (pts (xy 16.51 140.97) (xy 16.51 143.51)))
  (wire (pts (xy 97.79 60.96) (xy 107.95 60.96)))
  (wire (pts (xy 16.51 135.89) (xy 16.51 138.43)))
  (wire (pts (xy 16.51 100.33) (xy 16.51 102.87)))
  (bus (pts (xy 212.09 111.76) (xy 212.09 114.3)))
  (wire (pts (xy 222.25 81.28) (xy 224.79 81.28)))
  (wire (pts (xy 16.51 146.05) (xy 16.51 151.13)))
  (wire (pts (xy 16.51 82.55) (xy 16.51 85.09)))
  (wire (pts (xy 29.21 46.99) (xy 40.64 46.99)))
  (bus (pts (xy 156.21 93.98) (xy 156.21 96.52)))
  (wire (pts (xy 60.96 72.39) (xy 60.96 81.28)))
  (wire (pts (xy 60.96 41.91) (xy 76.2 41.91)))
  (wire (pts (xy 203.2 40.64) (xy 203.2 83.82)))
  (wire (pts (xy 29.21 52.07) (xy 40.64 52.07)))
  (wire (pts (xy 123.19 58.42) (xy 200.66 58.42)))
  (wire (pts (xy 16.51 67.31) (xy 16.51 69.85)))
  (wire (pts (xy 29.21 62.23) (xy 40.64 62.23)))
  (wire (pts (xy 29.21 72.39) (xy 45.72 72.39)))
  (wire (pts (xy 187.96 81.28) (xy 219.71 81.28)))
  (wire (pts (xy 219.71 97.79) (xy 219.71 106.68)))
  (wire (pts (xy 222.25 106.68) (xy 224.79 106.68)))
  (wire (pts (xy 219.71 81.28) (xy 219.71 90.17)))
  (bus (pts (xy 156.21 68.58) (xy 156.21 88.9)))
  (wire (pts (xy 16.51 90.17) (xy 16.51 92.71)))
  (wire (pts (xy 29.21 123.19) (xy 40.64 123.19)))
  (wire (pts (xy 187.96 111.76) (xy 209.55 111.76)))
  (wire (pts (xy 166.37 124.46) (xy 219.71 124.46)))
  (wire (pts (xy 29.21 120.65) (xy 40.64 120.65)))
  (bus (pts (xy 43.18 105.41) (xy 43.18 102.87)))
  (wire (pts (xy 224.79 81.28) (xy 224.79 90.17)))
  (wire (pts (xy 139.7 66.04) (xy 139.7 45.72)))
  (wire (pts (xy 16.51 87.63) (xy 16.51 90.17)))
  (wire (pts (xy 190.5 86.36) (xy 187.96 86.36)))
  (wire (pts (xy 29.21 113.03) (xy 29.21 115.57)))
  (wire (pts (xy 187.96 91.44) (xy 190.5 91.44)))
  (wire (pts (xy 29.21 133.35) (xy 40.64 133.35)))
  (wire (pts (xy 161.29 119.38) (xy 161.29 109.22)))
  (wire (pts (xy 29.21 49.53) (xy 40.64 49.53)))
  (wire (pts (xy 16.51 59.69) (xy 16.51 62.23)))
  (wire (pts (xy 29.21 125.73) (xy 40.64 125.73)))
  (bus (pts (xy 43.18 123.19) (xy 43.18 125.73)))
  (wire (pts (xy 16.51 95.25) (xy 16.51 97.79)))
  (wire (pts (xy 91.44 40.64) (xy 203.2 40.64)))
  (wire (pts (xy 187.96 114.3) (xy 209.55 114.3)))
  (wire (pts (xy 16.51 49.53) (xy 16.51 52.07)))
  (wire (pts (xy 158.75 88.9) (xy 166.37 88.9)))
  (bus (pts (xy 43.18 38.1) (xy 212.09 38.1)))
  (bus (pts (xy 43.18 111.76) (xy 43.18 115.57)))
  (bus (pts (xy 156.21 111.76) (xy 43.18 111.76)))
  (wire (pts (xy 16.51 115.57) (xy 16.51 118.11)))
  (wire (pts (xy 209.55 119.38) (xy 161.29 119.38)))
  (bus (pts (xy 43.18 102.87) (xy 43.18 100.33)))
  (wire (pts (xy 48.26 74.93) (xy 48.26 49.53)))
  (wire (pts (xy 123.19 60.96) (xy 134.62 60.96)))
  (wire (pts (xy 16.51 105.41) (xy 16.51 107.95)))
  (wire (pts (xy 200.66 101.6) (xy 187.96 101.6)))
  (bus (pts (xy 193.04 86.36) (xy 193.04 68.58)))
  (wire (pts (xy 219.71 106.68) (xy 222.25 106.68)))
  (wire (pts (xy 16.51 133.35) (xy 16.51 135.89)))
  (wire (pts (xy 66.04 55.88) (xy 69.85 55.88)))
  (wire (pts (xy 16.51 138.43) (xy 16.51 140.97)))
  (wire (pts (xy 29.21 128.27) (xy 40.64 128.27)))
  (wire (pts (xy 99.06 71.12) (xy 107.95 71.12)))
  (wire (pts (xy 97.79 55.88) (xy 107.95 55.88)))
  (wire (pts (xy 29.21 102.87) (xy 40.64 102.87)))
  (wire (pts (xy 158.75 99.06) (xy 166.37 99.06)))
  (bus (pts (xy 193.04 91.44) (xy 193.04 88.9)))
  (wire (pts (xy 16.51 92.71) (xy 16.51 95.25)))
  (wire (pts (xy 190.5 73.66) (xy 190.5 86.36)))
  (bus (pts (xy 43.18 135.89) (xy 43.18 138.43)))
  (bus (pts (xy 43.18 128.27) (xy 43.18 130.81)))
  (bus (pts (xy 43.18 44.45) (xy 43.18 38.1)))
  (wire (pts (xy 16.51 102.87) (xy 16.51 105.41)))
  (wire (pts (xy 16.51 72.39) (xy 16.51 74.93)))
  (wire (pts (xy 29.21 138.43) (xy 40.64 138.43)))
  (wire (pts (xy 29.21 54.61) (xy 40.64 54.61)))
  (wire (pts (xy 16.51 69.85) (xy 16.51 72.39)))
  (bus (pts (xy 43.18 120.65) (xy 43.18 123.19)))
  (bus (pts (xy 212.09 106.68) (xy 212.09 109.22)))
  (wire (pts (xy 16.51 52.07) (xy 16.51 54.61)))
  (wire (pts (xy 107.95 68.58) (xy 105.41 68.58)))
  (wire (pts (xy 48.26 49.53) (xy 76.2 49.53)))
  (wire (pts (xy 107.95 66.04) (xy 102.87 66.04)))
  (bus (pts (xy 156.21 101.6) (xy 156.21 104.14)))
  (bus (pts (xy 43.18 62.23) (xy 43.18 59.69)))
  (wire (pts (xy 16.51 143.51) (xy 16.51 146.05)))
  (bus (pts (xy 95.25 43.18) (xy 132.08 43.18)))
  (wire (pts (xy 29.21 105.41) (xy 40.64 105.41)))
  (wire (pts (xy 29.21 146.05) (xy 40.64 146.05)))
  (wire (pts (xy 123.19 53.34) (xy 124.46 53.34)))
  (wire (pts (xy 158.75 93.98) (xy 166.37 93.98)))
  (wire (pts (xy 29.21 110.49) (xy 29.21 113.03)))
  (bus (pts (xy 212.09 38.1) (xy 212.09 101.6)))
  (wire (pts (xy 158.75 91.44) (xy 166.37 91.44)))
  (wire (pts (xy 158.75 121.92) (xy 158.75 106.68)))
  (wire (pts (xy 29.21 115.57) (xy 31.75 115.57)))
  (bus (pts (xy 95.25 63.5) (xy 95.25 60.96)))
  (wire (pts (xy 16.51 57.15) (xy 16.51 59.69)))
  (wire (pts (xy 29.21 135.89) (xy 40.64 135.89)))
  (wire (pts (xy 16.51 64.77) (xy 16.51 67.31)))
  (bus (pts (xy 212.09 116.84) (xy 212.09 119.38)))
  (wire (pts (xy 158.75 101.6) (xy 166.37 101.6)))
  (wire (pts (xy 16.51 120.65) (xy 16.51 123.19)))
  (wire (pts (xy 29.21 59.69) (xy 40.64 59.69)))
  (wire (pts (xy 163.83 116.84) (xy 163.83 111.76)))
  (bus (pts (xy 156.21 106.68) (xy 156.21 111.76)))
  (wire (pts (xy 29.21 64.77) (xy 40.64 64.77)))
  (wire (pts (xy 99.06 71.12) (xy 99.06 80.01)))
  (wire (pts (xy 193.04 99.06) (xy 207.01 99.06)))
  (wire (pts (xy 132.08 68.58) (xy 123.19 68.58)))
  (wire (pts (xy 187.96 96.52) (xy 190.5 96.52)))
  (wire (pts (xy 29.21 95.25) (xy 40.64 95.25)))
  (wire (pts (xy 16.51 80.01) (xy 16.51 82.55)))
  (bus (pts (xy 43.18 57.15) (xy 43.18 54.61)))
  (wire (pts (xy 209.55 116.84) (xy 163.83 116.84)))
  (bus (pts (xy 43.18 49.53) (xy 43.18 46.99)))
  (bus (pts (xy 193.04 88.9) (xy 193.04 86.36)))
  (bus (pts (xy 43.18 130.81) (xy 43.18 133.35)))
  (wire (pts (xy 76.2 49.53) (xy 76.2 46.99)))
  (wire (pts (xy 29.21 100.33) (xy 40.64 100.33)))
  (wire (pts (xy 97.79 53.34) (xy 107.95 53.34)))
  (wire (pts (xy 16.51 77.47) (xy 16.51 80.01)))
  (wire (pts (xy 187.96 104.14) (xy 209.55 104.14)))
  (bus (pts (xy 43.18 54.61) (xy 43.18 52.07)))
  (bus (pts (xy 95.25 58.42) (xy 95.25 55.88)))
  (wire (pts (xy 224.79 81.28) (xy 233.68 81.28)))
  (wire (pts (xy 123.19 71.12) (xy 163.83 71.12)))
  (wire (pts (xy 16.51 97.79) (xy 16.51 100.33)))
  (wire (pts (xy 187.96 99.06) (xy 190.5 99.06)))
  (bus (pts (xy 43.18 138.43) (xy 43.18 140.97)))
  (wire (pts (xy 123.19 66.04) (xy 139.7 66.04)))
  (wire (pts (xy 16.51 128.27) (xy 16.51 130.81)))
  (wire (pts (xy 137.16 63.5) (xy 137.16 45.72)))
  (wire (pts (xy 102.87 76.2) (xy 166.37 76.2)))
  (wire (pts (xy 16.51 85.09) (xy 16.51 87.63)))
  (wire (pts (xy 124.46 50.8) (xy 124.46 53.34)))
  (bus (pts (xy 43.18 95.25) (xy 43.18 92.71)))
  (bus (pts (xy 43.18 118.11) (xy 43.18 120.65)))
  (wire (pts (xy 16.51 74.93) (xy 16.51 77.47)))
  (wire (pts (xy 66.04 81.28) (xy 69.85 81.28)))
  (bus (pts (xy 212.09 101.6) (xy 212.09 104.14)))
  (bus (pts (xy 132.08 43.18) (xy 134.62 43.18)))
  (wire (pts (xy 60.96 64.77) (xy 60.96 55.88)))
  (wire (pts (xy 16.51 62.23) (xy 16.51 64.77)))
  (wire (pts (xy 107.95 63.5) (xy 99.06 63.5)))
  (wire (pts (xy 60.96 81.28) (xy 66.04 81.28)))
  (wire (pts (xy 45.72 41.91) (xy 45.72 46.99)))
  (wire (pts (xy 29.21 107.95) (xy 40.64 107.95)))
  (bus (pts (xy 156.21 104.14) (xy 156.21 106.68)))
  (wire (pts (xy 16.51 46.99) (xy 16.51 49.53)))
  (wire (pts (xy 158.75 104.14) (xy 166.37 104.14)))
  (wire (pts (xy 158.75 106.68) (xy 166.37 106.68)))
  (wire (pts (xy 16.51 123.19) (xy 16.51 125.73)))
  (wire (pts (xy 166.37 76.2) (xy 166.37 81.28)))
  (bus (pts (xy 43.18 100.33) (xy 43.18 97.79)))
  (wire (pts (xy 16.51 110.49) (xy 16.51 113.03)))
  (bus (pts (xy 43.18 125.73) (xy 43.18 128.27)))
  (wire (pts (xy 29.21 57.15) (xy 40.64 57.15)))
  (wire (pts (xy 29.21 97.79) (xy 40.64 97.79)))
  (bus (pts (xy 95.25 63.5) (xy 95.25 90.17)))
  (wire (pts (xy 219.71 124.46) (xy 219.71 106.68)))
  (bus (pts (xy 43.18 59.69) (xy 43.18 57.15)))
  (bus (pts (xy 212.09 109.22) (xy 212.09 111.76)))
  (wire (pts (xy 158.75 96.52) (xy 166.37 96.52)))
  (wire (pts (xy 91.44 40.64) (xy 91.44 44.45)))
  (wire (pts (xy 187.96 106.68) (xy 209.55 106.68)))
  (bus (pts (xy 43.18 52.07) (xy 43.18 49.53)))
  (bus (pts (xy 95.25 60.96) (xy 95.25 58.42)))
  (label "BD6" (at 30.48 49.53 0) (fields_autoplaced))
  (label "BA9" (at 30.48 123.19 0) (fields_autoplaced))
  (label "BA5" (at 30.48 133.35 0) (fields_autoplaced))
  (label "BA2" (at 30.48 140.97 0) (fields_autoplaced))
  (label "{slash}SEL4" (at 30.48 100.33 0) (fields_autoplaced))
  (label "{slash}RES" (at 30.48 80.01 0) (fields_autoplaced))
  (label "BA7" (at 30.48 128.27 0) (fields_autoplaced))
  (label "BD0" (at 30.48 64.77 0) (fields_autoplaced))
  (label "BA8" (at 30.48 125.73 0) (fields_autoplaced))
  (label "BD4" (at 30.48 54.61 0) (fields_autoplaced))
  (label "{slash}SEL1" (at 30.48 107.95 0) (fields_autoplaced))
  (label "BA4" (at 30.48 135.89 0) (fields_autoplaced))
  (label "{slash}SEL9" (at 30.48 90.17 0) (fields_autoplaced))
  (label "{slash}SEL6" (at 30.48 95.25 0) (fields_autoplaced))
  (label "{slash}SEL2" (at 30.48 105.41 0) (fields_autoplaced))
  (label "{slash}SEL7" (at 30.48 92.71 0) (fields_autoplaced))
  (label "BD7" (at 30.48 46.99 0) (fields_autoplaced))
  (label "{slash}SEL3" (at 30.48 102.87 0) (fields_autoplaced))
  (label "BA0" (at 30.48 146.05 0) (fields_autoplaced))
  (label "{slash}SEL5" (at 30.48 97.79 0) (fields_autoplaced))
  (label "BA10" (at 30.48 120.65 0) (fields_autoplaced))
  (label "{slash}SEL10" (at 30.48 87.63 0) (fields_autoplaced))
  (label "{slash}IRQ" (at 30.48 77.47 0) (fields_autoplaced))
  (label "BD3" (at 30.48 57.15 0) (fields_autoplaced))
  (label "BA6" (at 30.48 130.81 0) (fields_autoplaced))
  (label "BD5" (at 30.48 52.07 0) (fields_autoplaced))
  (label "BA1" (at 30.48 143.51 0) (fields_autoplaced))
  (label "BD2" (at 30.48 59.69 0) (fields_autoplaced))
  (label "R{slash}W+Ē" (at 30.48 72.39 0) (fields_autoplaced))
  (label "BA3" (at 30.48 138.43 0) (fields_autoplaced))
  (label "{slash}SEL11" (at 30.48 85.09 0) (fields_autoplaced))
  (label "BØ2" (at 30.48 74.93 0) (fields_autoplaced))
  (label "BD1" (at 30.48 62.23 0) (fields_autoplaced))
  (label "BA11" (at 30.48 118.11 0) (fields_autoplaced))
  (symbol (lib_id "74xx:74LS05") (at 233.68 93.98 0) (unit 7)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U2" (at 240.03 93.345 0))
    (property "Value" "74LS05" (at 240.03 95.885 0))
    (property "Footprint" "" (at 233.68 93.98 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS05" (at 233.68 93.98 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Board0"
        (path
          (reference "U2") (unit 7)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 66.04 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 66.04 87.63 0))
    (property "Value" "GND" (at 66.04 86.36 0))
    (property "Footprint" "" (at 66.04 81.28 0))
    (property "Datasheet" "" (at 66.04 81.28 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 128.27 53.34 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 128.27 48.26 90))
    (property "Value" "10K" (at 128.27 50.8 90))
    (property "Footprint" "" (at 128.27 55.118 90))
    (property "Datasheet" "~" (at 128.27 53.34 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Board0"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 16.51 151.13 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 16.51 157.48 0))
    (property "Value" "GND" (at 16.51 156.21 0))
    (property "Footprint" "" (at 16.51 151.13 0))
    (property "Datasheet" "" (at 16.51 151.13 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "74xx:74LS05") (at 207.01 91.44 270) (unit 3)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U2" (at 215.9 91.44 0))
    (property "Value" "74LS05" (at 213.36 91.44 0))
    (property "Footprint" "" (at 207.01 91.44 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS05" (at 207.01 91.44 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Board0"
        (path
          (reference "U2") (unit 3)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 219.71 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C3" (at 219.71 91.44 0))
    (property "Value" ".1" (at 219.71 96.52 0))
    (property "Footprint" "" (at 220.6752 97.79 0))
    (property "Datasheet" "~" (at 219.71 93.98 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Board0"
        (path
          (reference "C3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Priority_Encoder:74HC148") (at 115.57 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U3" (at 115.57 48.26 0))
    (property "Value" "~" (at 115.57 60.96 0))
    (property "Footprint" "" (at 115.57 60.96 0))
    (property "Datasheet" "" (at 115.57 60.96 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Board0"
        (path
          (reference "U3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 124.46 50.8 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 124.46 54.61 0))
    (property "Value" "+5V" (at 124.46 46.99 0))
    (property "Footprint" "" (at 124.46 50.8 0))
    (property "Datasheet" "" (at 124.46 50.8 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "74xx:74LS00") (at 53.34 44.45 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U4" (at 53.3317 36.83 0))
    (property "Value" "74LS00" (at 53.3317 39.37 0))
    (property "Footprint" "" (at 53.34 44.45 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls00" (at 53.34 44.45 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Board0"
        (path
          (reference "U4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 60.96 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C4" (at 60.96 66.04 0))
    (property "Value" ".1" (at 60.96 71.12 0))
    (property "Footprint" "" (at 61.9252 72.39 0))
    (property "Datasheet" "~" (at 60.96 68.58 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Board0"
        (path
          (reference "C4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 222.25 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR08" (at 222.25 113.03 0))
    (property "Value" "GND" (at 222.25 111.76 0))
    (property "Footprint" "" (at 222.25 106.68 0))
    (property "Datasheet" "" (at 222.25 106.68 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "SRAM:AS6C62256-55PCN") (at 176.53 96.52 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 176.53 76.2 0))
    (property "Value" "~" (at 176.53 96.52 0))
    (property "Footprint" "" (at 176.53 96.52 0))
    (property "Datasheet" "" (at 176.53 96.52 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Board0"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 115.57 80.01 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C1" (at 114.3 78.74 90))
    (property "Value" ".1" (at 119.38 78.74 90))
    (property "Footprint" "" (at 119.38 79.0448 0))
    (property "Datasheet" "~" (at 115.57 80.01 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Board0"
        (path
          (reference "C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 99.06 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 99.06 86.36 0))
    (property "Value" "GND" (at 99.06 85.09 0))
    (property "Footprint" "" (at 99.06 80.01 0))
    (property "Datasheet" "" (at 99.06 80.01 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "74xx:74LS00") (at 83.82 44.45 0) (unit 2)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U4" (at 83.8117 36.83 0))
    (property "Value" "74LS00" (at 83.8117 39.37 0))
    (property "Footprint" "" (at 83.82 44.45 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls00" (at 83.82 44.45 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Board0"
        (path
          (reference "U4") (unit 2)
        )
      )
    )
  )
  (symbol (lib_id "74xx:74LS00") (at 69.85 68.58 0) (unit 5)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U4" (at 76.2 67.945 0))
    (property "Value" "74LS00" (at 76.2 70.485 0))
    (property "Footprint" "" (at 69.85 68.58 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74ls00" (at 69.85 68.58 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Board0"
        (path
          (reference "U4") (unit 5)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_02x40_Counter_Clockwise") (at 24.13 97.79 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J4" (at 22.86 44.45 0))
    (property "Value" "Conn_02x40_Counter_Clockwise" (at 22.86 44.45 0))
    (property "Footprint" "" (at 24.13 97.79 0))
    (property "Datasheet" "~" (at 24.13 97.79 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "50")
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "56")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "6")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "65")
    (pin "66")
    (pin "67")
    (pin "68")
    (pin "69")
    (pin "7")
    (pin "70")
    (pin "71")
    (pin "72")
    (pin "73")
    (pin "74")
    (pin "75")
    (pin "76")
    (pin "77")
    (pin "78")
    (pin "79")
    (pin "8")
    (pin "80")
    (pin "9")
    (instances
      (project "Board0"
        (path
          (reference "J4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 222.25 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 222.25 85.09 0))
    (property "Value" "+5V" (at 222.25 77.47 0))
    (property "Footprint" "" (at 222.25 81.28 0))
    (property "Datasheet" "" (at 222.25 81.28 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 66.04 55.88 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR06" (at 66.04 59.69 0))
    (property "Value" "+5V" (at 66.04 52.07 0))
    (property "Footprint" "" (at 66.04 55.88 0))
    (property "Datasheet" "" (at 66.04 55.88 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 31.75 115.57 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 31.75 119.38 0))
    (property "Value" "+5V" (at 31.75 111.76 0))
    (property "Footprint" "" (at 31.75 115.57 0))
    (property "Datasheet" "" (at 31.75 115.57 0))
    (pin "1")
    (instances
      (project "Board0"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 224.79 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C2" (at 224.79 91.44 0))
    (property "Value" ".1" (at 224.79 96.52 0))
    (property "Footprint" "" (at 225.7552 97.79 0))
    (property "Datasheet" "~" (at 224.79 93.98 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Board0"
        (path
          (reference "C2") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
