(kicad_sch (version 20211123) (generator eeschema)
  (paper "A0")
  (lib_symbols
    (symbol "74xx:74LS14" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "74LS14" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL not inverter" (id 5) (at 0 0 0))
      (property "ki_description" "Hex inverter schmitt trigger" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0))
      (symbol "74LS14_1_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74LS14_1_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_2_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74LS14_2_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS14_3_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS14_4_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74LS14_5_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS14_6_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_7_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS14_7_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74LS145" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 13.97 0))
      (property "Value" "74LS145" (id 1) (at -7.62 -16.51 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS145" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL DECOD10 OpenColl" (id 5) (at 0 0 0))
      (property "ki_description" "Decoder 1 to 10, Open Collector" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP?16*" (id 7) (at 0 0 0))
      (symbol "74LS145_1_0"
        (pin open_collector inverted (at 12.7 10.16 180) (length 5.08)
          (name "Q0")
          (number "1")
        )
        (pin open_collector inverted (at 12.7 -10.16 180) (length 5.08)
          (name "Q8")
          (number "10")
        )
        (pin open_collector inverted (at 12.7 -12.7 180) (length 5.08)
          (name "Q9")
          (number "11")
        )
        (pin input line (at -12.7 2.54 0) (length 5.08)
          (name "P3")
          (number "12")
        )
        (pin input line (at -12.7 5.08 0) (length 5.08)
          (name "P2")
          (number "13")
        )
        (pin input line (at -12.7 7.62 0) (length 5.08)
          (name "P1")
          (number "14")
        )
        (pin input line (at -12.7 10.16 0) (length 5.08)
          (name "P0")
          (number "15")
        )
        (pin power_in line (at 0 17.78 270) (length 5.08)
          (name "VCC")
          (number "16")
        )
        (pin open_collector inverted (at 12.7 7.62 180) (length 5.08)
          (name "Q1")
          (number "2")
        )
        (pin open_collector inverted (at 12.7 5.08 180) (length 5.08)
          (name "Q2")
          (number "3")
        )
        (pin open_collector inverted (at 12.7 2.54 180) (length 5.08)
          (name "Q3")
          (number "4")
        )
        (pin open_collector inverted (at 12.7 0 180) (length 5.08)
          (name "Q4")
          (number "5")
        )
        (pin open_collector inverted (at 12.7 -2.54 180) (length 5.08)
          (name "Q5")
          (number "6")
        )
        (pin open_collector inverted (at 12.7 -5.08 180) (length 5.08)
          (name "Q6")
          (number "7")
        )
        (pin power_in line (at 0 -20.32 90) (length 5.08)
          (name "GND")
          (number "8")
        )
        (pin open_collector inverted (at 12.7 -7.62 180) (length 5.08)
          (name "Q7")
          (number "9")
        )
      )
      (symbol "74LS145_1_1"
        (rectangle (start -7.62 12.7) (end 7.62 -15.24)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74LS151" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 19.05 0))
      (property "Value" "74LS151" (id 1) (at -7.62 -21.59 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS151" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL MUX8" (id 5) (at 0 0 0))
      (property "ki_description" "Multiplexer 8 to 1" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP?16*" (id 7) (at 0 0 0))
      (symbol "74LS151_1_0"
        (pin input line (at -12.7 7.62 0) (length 5.08)
          (name "I3")
          (number "1")
        )
        (pin input line (at -12.7 -10.16 0) (length 5.08)
          (name "S1")
          (number "10")
        )
        (pin input line (at -12.7 -7.62 0) (length 5.08)
          (name "S0")
          (number "11")
        )
        (pin input line (at -12.7 -2.54 0) (length 5.08)
          (name "I7")
          (number "12")
        )
        (pin input line (at -12.7 0 0) (length 5.08)
          (name "I6")
          (number "13")
        )
        (pin input line (at -12.7 2.54 0) (length 5.08)
          (name "I5")
          (number "14")
        )
        (pin input line (at -12.7 5.08 0) (length 5.08)
          (name "I4")
          (number "15")
        )
        (pin power_in line (at 0 22.86 270) (length 5.08)
          (name "VCC")
          (number "16")
        )
        (pin input line (at -12.7 10.16 0) (length 5.08)
          (name "I2")
          (number "2")
        )
        (pin input line (at -12.7 12.7 0) (length 5.08)
          (name "I1")
          (number "3")
        )
        (pin input line (at -12.7 15.24 0) (length 5.08)
          (name "I0")
          (number "4")
        )
        (pin output line (at 12.7 15.24 180) (length 5.08)
          (name "Z")
          (number "5")
        )
        (pin output line (at 12.7 12.7 180) (length 5.08)
          (name "~{Z}")
          (number "6")
        )
        (pin input line (at -12.7 -17.78 0) (length 5.08)
          (name "~{E}")
          (number "7")
        )
        (pin power_in line (at 0 -25.4 90) (length 5.08)
          (name "GND")
          (number "8")
        )
        (pin input line (at -12.7 -12.7 0) (length 5.08)
          (name "S2")
          (number "9")
        )
      )
      (symbol "74LS151_1_1"
        (rectangle (start -7.62 17.78) (end 7.62 -20.32)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74LS38" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "74LS38" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL Nand2 OpenCol Buffer" (id 5) (at 0 0 0))
      (property "ki_description" "Quad Buffer 2-input NAND Open collector" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0))
      (symbol "74LS38_1_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS38_1_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "1")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "2")
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS38_2_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS38_2_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "4")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "5")
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS38_3_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS38_3_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "10")
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS38_4_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS38_4_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "12")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS38_5_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS38_5_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "Connector:DIN-8" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 3.175 5.715 0))
      (property "Value" "DIN-8" (id 1) (at 2.032 -5.842 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "circular DIN connector" (id 4) (at 0 0 0))
      (property "ki_description" "8-pin DIN connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIN*" (id 6) (at 0 0 0))
      (symbol "DIN-8_0_1"
        (arc (start -5.08 0) (mid -3.8609 -3.3364) (end -0.762 -5.08)
          (fill (type none))
        )
        (circle (center -3.048 -0.762) (radius 0.508)
          (fill (type none))
        )
        (circle (center -2.54 2.032) (radius 0.508)
          (fill (type none))
        )
        (circle (center -1.524 -2.794) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 0)
            (xy -3.556 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.508)
            (xy 0 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 0)
            (xy 3.556 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -4.318 -2.54)
            (xy -2.032 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.54)
            (xy -4.318 2.54)
            (xy -3.048 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 4.318 -2.54)
            (xy 2.032 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 2.54)
            (xy 4.318 2.54)
            (xy 3.048 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 -4.953)
            (xy -0.762 -4.191)
            (xy 0.762 -4.191)
            (xy 0.762 -4.953)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 0 3.302) (radius 0.508)
          (fill (type none))
        )
        (arc (start 0.762 -5.08) (mid 3.8685 -3.343) (end 5.08 0)
          (fill (type none))
        )
        (circle (center 1.524 -2.794) (radius 0.508)
          (fill (type none))
        )
        (circle (center 2.54 2.032) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.048 -0.762) (radius 0.508)
          (fill (type none))
        )
        (arc (start 5.08 0) (mid 0 5.08) (end -5.08 0)
          (fill (type none))
        )
      )
      (symbol "DIN-8_1_1"
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at -7.62 2.54 0) (length 2.54)
          (name "~")
          (number "4")
        )
        (pin passive line (at 7.62 2.54 180) (length 2.54)
          (name "~")
          (number "5")
        )
        (pin passive line (at -7.62 -2.54 0) (length 2.54)
          (name "~")
          (number "6")
        )
        (pin passive line (at 7.62 -2.54 180) (length 2.54)
          (name "~")
          (number "7")
        )
        (pin passive line (at 0 -7.62 90) (length 2.54)
          (name "~")
          (number "8")
        )
      )
    )
    (symbol "Device:Buzzer" (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BZ" (id 0) (at 3.81 1.27 0))
      (property "Value" "Buzzer" (id 1) (at 3.81 -1.27 0))
      (property "Footprint" "" (id 2) (at -0.635 2.54 90))
      (property "Datasheet" "~" (id 3) (at -0.635 2.54 90))
      (property "ki_keywords" "quartz resonator ceramic" (id 4) (at 0 0 0))
      (property "ki_description" "Buzzer, polarized" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "*Buzzer*" (id 6) (at 0 0 0))
      (symbol "Buzzer_0_1"
        (arc (start 0 -3.175) (mid 3.175 0) (end 0 3.175)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.651 1.905)
            (xy -1.143 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.397 2.159)
            (xy -1.397 1.651)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 3.175)
            (xy 0 -3.175)
          )
          (fill (type none))
        )
      )
      (symbol "Buzzer_1_1"
        (pin passive line (at -2.54 2.54 0) (length 2.54)
          (name "-")
          (number "1")
        )
        (pin passive line (at -2.54 -2.54 0) (length 2.54)
          (name "+")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0))
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Network06" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RN" (id 0) (at -10.16 0 90))
      (property "Value" "R_Network06" (id 1) (at 7.62 0 90))
      (property "Footprint" "Resistor_THT:R_Array_SIP7" (id 2) (at 9.525 0 90))
      (property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "R network star-topology" (id 4) (at 0 0 0))
      (property "ki_description" "6 resistor network, star topology, bussed resistors, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R?Array?SIP*" (id 6) (at 0 0 0))
      (symbol "R_Network06_0_1"
        (rectangle (start -8.89 -3.175) (end 6.35 3.175)
          (fill (type background))
        )
        (rectangle (start -8.382 1.524) (end -6.858 -2.54)
          (fill (type none))
        )
        (circle (center -7.62 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -5.842 1.524) (end -4.318 -2.54)
          (fill (type none))
        )
        (circle (center -5.08 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -3.302 1.524) (end -1.778 -2.54)
          (fill (type none))
        )
        (circle (center -2.54 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -0.762 1.524) (end 0.762 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 -2.54)
            (xy -7.62 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 1.524)
            (xy -7.62 2.286)
            (xy -5.08 2.286)
            (xy -5.08 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.524)
            (xy -5.08 2.286)
            (xy -2.54 2.286)
            (xy -2.54 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.524)
            (xy -2.54 2.286)
            (xy 0 2.286)
            (xy 0 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.524)
            (xy 0 2.286)
            (xy 2.54 2.286)
            (xy 2.54 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.524)
            (xy 2.54 2.286)
            (xy 5.08 2.286)
            (xy 5.08 1.524)
          )
          (fill (type none))
        )
        (circle (center 0 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 1.778 1.524) (end 3.302 -2.54)
          (fill (type none))
        )
        (circle (center 2.54 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 4.318 1.524) (end 5.842 -2.54)
          (fill (type none))
        )
      )
      (symbol "R_Network06_1_1"
        (pin passive line (at -7.62 5.08 270) (length 2.54)
          (name "common")
          (number "1")
        )
        (pin passive line (at -7.62 -5.08 90) (length 1.27)
          (name "R1")
          (number "2")
        )
        (pin passive line (at -5.08 -5.08 90) (length 1.27)
          (name "R2")
          (number "3")
        )
        (pin passive line (at -2.54 -5.08 90) (length 1.27)
          (name "R3")
          (number "4")
        )
        (pin passive line (at 0 -5.08 90) (length 1.27)
          (name "R4")
          (number "5")
        )
        (pin passive line (at 2.54 -5.08 90) (length 1.27)
          (name "R5")
          (number "6")
        )
        (pin passive line (at 5.08 -5.08 90) (length 1.27)
          (name "R6")
          (number "7")
        )
      )
    )
    (symbol "MCU_Intel:8049" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -13.97 35.56 0))
      (property "Value" "8049" (id 1) (at 8.89 35.56 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "MCS-48 uC Microcontroller" (id 4) (at 0 0 0))
      (property "ki_description" "MCS-48 8-bit Microcontroller, 2KB Mask ROM, 128B RAM, DIP-40" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP* PDIP*" (id 6) (at 0 0 0))
      (symbol "8049_1_1"
        (rectangle (start -13.97 -34.29) (end 13.97 34.29)
          (fill (type background))
        )
        (pin input line (at -17.78 -25.4 0) (length 3.81)
          (name "T0")
          (number "1")
        )
        (pin output output_low (at 17.78 -12.7 180) (length 3.81)
          (name "~{WR}")
          (number "10")
        )
        (pin output line (at 17.78 -2.54 180) (length 3.81)
          (name "ALE")
          (number "11")
        )
        (pin bidirectional line (at 17.78 20.32 180) (length 3.81)
          (name "DB.0")
          (number "12")
        )
        (pin bidirectional line (at 17.78 17.78 180) (length 3.81)
          (name "DB.1")
          (number "13")
        )
        (pin bidirectional line (at 17.78 15.24 180) (length 3.81)
          (name "DB.2")
          (number "14")
        )
        (pin bidirectional line (at 17.78 12.7 180) (length 3.81)
          (name "DB.3")
          (number "15")
        )
        (pin bidirectional line (at 17.78 10.16 180) (length 3.81)
          (name "DB.4")
          (number "16")
        )
        (pin bidirectional line (at 17.78 7.62 180) (length 3.81)
          (name "DB.5")
          (number "17")
        )
        (pin bidirectional line (at 17.78 5.08 180) (length 3.81)
          (name "DB.6")
          (number "18")
        )
        (pin bidirectional line (at 17.78 2.54 180) (length 3.81)
          (name "DB.7")
          (number "19")
        )
        (pin input line (at 17.78 -25.4 180) (length 3.81)
          (name "X1")
          (number "2")
        )
        (pin power_in line (at 0 -38.1 90) (length 3.81)
          (name "GND")
          (number "20")
        )
        (pin bidirectional line (at -17.78 2.54 0) (length 3.81)
          (name "P2.0")
          (number "21")
        )
        (pin bidirectional line (at -17.78 0 0) (length 3.81)
          (name "P2.1")
          (number "22")
        )
        (pin bidirectional line (at -17.78 -2.54 0) (length 3.81)
          (name "P2.2")
          (number "23")
        )
        (pin bidirectional line (at -17.78 -5.08 0) (length 3.81)
          (name "P2.3")
          (number "24")
        )
        (pin output line (at -17.78 -20.32 0) (length 3.81)
          (name "PROG")
          (number "25")
        )
        (pin power_in line (at 17.78 30.48 180) (length 3.81)
          (name "VDD")
          (number "26")
        )
        (pin bidirectional line (at -17.78 25.4 0) (length 3.81)
          (name "P1.0")
          (number "27")
        )
        (pin bidirectional line (at -17.78 22.86 0) (length 3.81)
          (name "P1.1")
          (number "28")
        )
        (pin bidirectional line (at -17.78 20.32 0) (length 3.81)
          (name "P1.2")
          (number "29")
        )
        (pin output line (at 17.78 -30.48 180) (length 3.81)
          (name "X2")
          (number "3")
        )
        (pin bidirectional line (at -17.78 17.78 0) (length 3.81)
          (name "P1.3")
          (number "30")
        )
        (pin bidirectional line (at -17.78 15.24 0) (length 3.81)
          (name "P1.4")
          (number "31")
        )
        (pin bidirectional line (at -17.78 12.7 0) (length 3.81)
          (name "P1.5")
          (number "32")
        )
        (pin bidirectional line (at -17.78 10.16 0) (length 3.81)
          (name "P1.6")
          (number "33")
        )
        (pin bidirectional line (at -17.78 7.62 0) (length 3.81)
          (name "P1.7")
          (number "34")
        )
        (pin bidirectional line (at -17.78 -7.62 0) (length 3.81)
          (name "P2.4")
          (number "35")
        )
        (pin bidirectional line (at -17.78 -10.16 0) (length 3.81)
          (name "P2.5")
          (number "36")
        )
        (pin bidirectional line (at -17.78 -12.7 0) (length 3.81)
          (name "P2.6")
          (number "37")
        )
        (pin bidirectional line (at -17.78 -15.24 0) (length 3.81)
          (name "P2.7")
          (number "38")
        )
        (pin input line (at -17.78 -27.94 0) (length 3.81)
          (name "T1")
          (number "39")
        )
        (pin input inverted (at -17.78 30.48 0) (length 3.81)
          (name "~{RESET}")
          (number "4")
        )
        (pin power_in line (at 0 38.1 270) (length 3.81)
          (name "VCC")
          (number "40")
        )
        (pin input inverted (at 17.78 -17.78 180) (length 3.81)
          (name "~{SS}")
          (number "5")
        )
        (pin input inverted (at -17.78 -30.48 0) (length 3.81)
          (name "~{INT}")
          (number "6")
        )
        (pin input line (at 17.78 25.4 180) (length 3.81)
          (name "EA")
          (number "7")
        )
        (pin output output_low (at 17.78 -10.16 180) (length 3.81)
          (name "~{RD}")
          (number "8")
        )
        (pin output output_low (at 17.78 -7.62 180) (length 3.81)
          (name "~{PSEN}")
          (number "9")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 589.28 392.43) (diameter 0) (color 0 0 0 0))
  (junction (at 405.13 314.96) (diameter 0) (color 0 0 0 0))
  (junction (at 486.41 337.82) (diameter 0) (color 0 0 0 0))
  (junction (at 524.51 369.57) (diameter 0) (color 0 0 0 0))
  (junction (at 431.8 314.96) (diameter 0) (color 0 0 0 0))
  (junction (at 637.54 448.31) (diameter 0) (color 0 0 0 0))
  (junction (at 619.76 458.47) (diameter 0) (color 0 0 0 0))
  (junction (at 637.54 496.57) (diameter 0) (color 0 0 0 0))
  (junction (at 619.76 455.93) (diameter 0) (color 0 0 0 0))
  (junction (at 485.14 483.87) (diameter 0) (color 0 0 0 0))
  (junction (at 482.6 481.33) (diameter 0) (color 0 0 0 0))
  (junction (at 486.41 307.34) (diameter 0) (color 0 0 0 0))
  (junction (at 486.41 327.66) (diameter 0) (color 0 0 0 0))
  (junction (at 589.28 379.73) (diameter 0) (color 0 0 0 0))
  (junction (at 405.13 344.17) (diameter 0) (color 0 0 0 0))
  (junction (at 619.76 488.95) (diameter 0) (color 0 0 0 0))
  (no_connect (at 542.29 425.45))
  (no_connect (at 542.29 417.83))
  (no_connect (at 542.29 415.29))
  (no_connect (at 542.29 420.37))
  (no_connect (at 542.29 410.21))
  (no_connect (at 506.73 427.99))
  (no_connect (at 624.84 473.71))
  (no_connect (at 624.84 468.63))
  (no_connect (at 650.24 455.93))
  (wire (pts (xy 542.29 377.19) (xy 542.29 369.57)))
  (wire (pts (xy 568.96 340.36) (xy 568.96 415.29)))
  (wire (pts (xy 589.28 379.73) (xy 600.71 379.73)))
  (wire (pts (xy 397.51 271.78) (xy 487.68 271.78)))
  (wire (pts (xy 490.22 307.34) (xy 486.41 307.34)))
  (wire (pts (xy 405.13 309.88) (xy 405.13 314.96)))
  (wire (pts (xy 486.41 337.82) (xy 490.22 337.82)))
  (wire (pts (xy 574.04 397.51) (xy 574.04 402.59)))
  (wire (pts (xy 518.16 283.21) (xy 518.16 271.78)))
  (wire (pts (xy 447.04 356.87) (xy 447.04 358.14)))
  (wire (pts (xy 430.53 330.2) (xy 431.8 330.2)))
  (wire (pts (xy 431.8 359.41) (xy 405.13 359.41)))
  (wire (pts (xy 607.06 441.96) (xy 635 441.96)))
  (wire (pts (xy 415.29 387.35) (xy 415.29 354.33)))
  (wire (pts (xy 544.83 269.24) (xy 546.1 269.24)))
  (wire (pts (xy 584.2 392.43) (xy 584.2 394.97)))
  (wire (pts (xy 397.51 438.15) (xy 441.96 438.15)))
  (wire (pts (xy 544.83 431.8) (xy 547.37 431.8)))
  (wire (pts (xy 584.2 382.27) (xy 600.71 382.27)))
  (wire (pts (xy 609.6 466.09) (xy 624.84 466.09)))
  (wire (pts (xy 506.73 435.61) (xy 505.46 435.61)))
  (wire (pts (xy 492.76 532.13) (xy 504.19 532.13)))
  (wire (pts (xy 585.47 439.42) (xy 659.13 439.42)))
  (wire (pts (xy 576.58 394.97) (xy 576.58 397.51)))
  (wire (pts (xy 619.76 496.57) (xy 637.54 496.57)))
  (wire (pts (xy 397.51 438.15) (xy 397.51 271.78)))
  (wire (pts (xy 635 448.31) (xy 637.54 448.31)))
  (wire (pts (xy 589.28 392.43) (xy 600.71 392.43)))
  (wire (pts (xy 542.29 389.89) (xy 600.71 389.89)))
  (wire (pts (xy 544.83 439.42) (xy 547.37 439.42)))
  (wire (pts (xy 542.29 438.15) (xy 544.83 438.15)))
  (wire (pts (xy 584.2 394.97) (xy 600.71 394.97)))
  (wire (pts (xy 505.46 340.36) (xy 508 340.36)))
  (wire (pts (xy 659.13 439.42) (xy 659.13 458.47)))
  (wire (pts (xy 562.61 269.24) (xy 561.34 269.24)))
  (wire (pts (xy 482.6 481.33) (xy 504.19 481.33)))
  (wire (pts (xy 505.46 447.04) (xy 585.47 447.04)))
  (wire (pts (xy 571.5 410.21) (xy 600.71 410.21)))
  (wire (pts (xy 544.83 433.07) (xy 544.83 431.8)))
  (wire (pts (xy 542.29 382.27) (xy 547.37 382.27)))
  (wire (pts (xy 486.41 358.14) (xy 490.22 358.14)))
  (wire (pts (xy 581.66 387.35) (xy 600.71 387.35)))
  (wire (pts (xy 505.46 355.6) (xy 508 355.6)))
  (wire (pts (xy 542.29 369.57) (xy 524.51 369.57)))
  (wire (pts (xy 477.52 389.89) (xy 477.52 342.9)))
  (wire (pts (xy 476.25 269.24) (xy 487.68 269.24)))
  (wire (pts (xy 480.06 353.06) (xy 490.22 353.06)))
  (wire (pts (xy 576.58 397.51) (xy 600.71 397.51)))
  (wire (pts (xy 447.04 365.76) (xy 447.04 372.11)))
  (wire (pts (xy 574.04 402.59) (xy 600.71 402.59)))
  (wire (pts (xy 542.29 397.51) (xy 574.04 397.51)))
  (wire (pts (xy 405.13 359.41) (xy 405.13 344.17)))
  (wire (pts (xy 600.71 407.67) (xy 586.74 407.67)))
  (wire (pts (xy 497.84 420.37) (xy 497.84 466.09)))
  (wire (pts (xy 486.41 307.34) (xy 486.41 327.66)))
  (wire (pts (xy 487.68 486.41) (xy 487.68 410.21)))
  (wire (pts (xy 447.04 312.42) (xy 447.04 261.62)))
  (wire (pts (xy 568.96 415.29) (xy 600.71 415.29)))
  (wire (pts (xy 607.06 471.17) (xy 624.84 471.17)))
  (wire (pts (xy 542.29 394.97) (xy 576.58 394.97)))
  (wire (pts (xy 474.98 384.81) (xy 506.73 384.81)))
  (wire (pts (xy 490.22 412.75) (xy 506.73 412.75)))
  (wire (pts (xy 471.17 266.7) (xy 487.68 266.7)))
  (wire (pts (xy 617.22 458.47) (xy 619.76 458.47)))
  (wire (pts (xy 474.98 322.58) (xy 474.98 384.81)))
  (wire (pts (xy 452.12 341.63) (xy 452.12 283.21)))
  (wire (pts (xy 457.2 438.15) (xy 459.74 438.15)))
  (wire (pts (xy 485.14 407.67) (xy 506.73 407.67)))
  (wire (pts (xy 542.29 433.07) (xy 544.83 433.07)))
  (wire (pts (xy 449.58 327.66) (xy 449.58 274.32)))
  (wire (pts (xy 619.76 488.95) (xy 624.84 488.95)))
  (wire (pts (xy 542.29 402.59) (xy 571.5 402.59)))
  (wire (pts (xy 506.73 433.07) (xy 502.92 433.07)))
  (wire (pts (xy 589.28 417.83) (xy 600.71 417.83)))
  (wire (pts (xy 582.93 466.09) (xy 582.93 478.79)))
  (wire (pts (xy 506.73 420.37) (xy 497.84 420.37)))
  (wire (pts (xy 485.14 483.87) (xy 485.14 407.67)))
  (wire (pts (xy 586.74 407.67) (xy 586.74 309.88)))
  (wire (pts (xy 505.46 435.61) (xy 505.46 447.04)))
  (wire (pts (xy 447.04 327.66) (xy 449.58 327.66)))
  (wire (pts (xy 472.44 312.42) (xy 472.44 382.27)))
  (wire (pts (xy 415.29 387.35) (xy 506.73 387.35)))
  (wire (pts (xy 497.84 466.09) (xy 582.93 466.09)))
  (wire (pts (xy 614.68 461.01) (xy 624.84 461.01)))
  (wire (pts (xy 412.75 394.97) (xy 412.75 309.88)))
  (wire (pts (xy 586.74 309.88) (xy 515.62 309.88)))
  (wire (pts (xy 584.2 325.12) (xy 584.2 382.27)))
  (wire (pts (xy 485.14 529.59) (xy 504.19 529.59)))
  (wire (pts (xy 659.13 458.47) (xy 650.24 458.47)))
  (wire (pts (xy 502.92 266.7) (xy 518.16 266.7)))
  (wire (pts (xy 504.19 483.87) (xy 485.14 483.87)))
  (wire (pts (xy 515.62 325.12) (xy 584.2 325.12)))
  (wire (pts (xy 566.42 412.75) (xy 600.71 412.75)))
  (wire (pts (xy 635 441.96) (xy 635 448.31)))
  (wire (pts (xy 490.22 488.95) (xy 490.22 412.75)))
  (wire (pts (xy 607.06 452.12) (xy 607.06 471.17)))
  (wire (pts (xy 472.44 382.27) (xy 506.73 382.27)))
  (wire (pts (xy 447.04 341.63) (xy 452.12 341.63)))
  (wire (pts (xy 515.62 355.6) (xy 566.42 355.6)))
  (wire (pts (xy 486.41 337.82) (xy 486.41 358.14)))
  (wire (pts (xy 614.68 452.12) (xy 614.68 461.01)))
  (wire (pts (xy 508 309.88) (xy 505.46 309.88)))
  (wire (pts (xy 518.16 271.78) (xy 502.92 271.78)))
  (wire (pts (xy 582.93 478.79) (xy 624.84 478.79)))
  (wire (pts (xy 477.52 342.9) (xy 490.22 342.9)))
  (wire (pts (xy 542.29 400.05) (xy 600.71 400.05)))
  (wire (pts (xy 589.28 374.65) (xy 589.28 379.73)))
  (wire (pts (xy 490.22 322.58) (xy 474.98 322.58)))
  (wire (pts (xy 502.92 449.58) (xy 581.66 449.58)))
  (wire (pts (xy 518.16 266.7) (xy 518.16 265.43)))
  (wire (pts (xy 619.76 458.47) (xy 619.76 488.95)))
  (wire (pts (xy 482.6 481.33) (xy 482.6 527.05)))
  (wire (pts (xy 579.12 483.87) (xy 579.12 387.35)))
  (wire (pts (xy 506.73 389.89) (xy 477.52 389.89)))
  (wire (pts (xy 506.73 422.91) (xy 500.38 422.91)))
  (wire (pts (xy 585.47 447.04) (xy 585.47 439.42)))
  (wire (pts (xy 506.73 417.83) (xy 495.3 417.83)))
  (wire (pts (xy 482.6 527.05) (xy 504.19 527.05)))
  (wire (pts (xy 430.53 339.09) (xy 431.8 339.09)))
  (wire (pts (xy 485.14 483.87) (xy 485.14 529.59)))
  (wire (pts (xy 410.21 339.09) (xy 415.29 339.09)))
  (wire (pts (xy 502.92 433.07) (xy 502.92 449.58)))
  (wire (pts (xy 492.76 415.29) (xy 492.76 532.13)))
  (wire (pts (xy 506.73 360.68) (xy 562.61 360.68)))
  (wire (pts (xy 407.67 330.2) (xy 407.67 400.05)))
  (wire (pts (xy 589.28 392.43) (xy 589.28 417.83)))
  (wire (pts (xy 612.14 452.12) (xy 612.14 463.55)))
  (wire (pts (xy 431.8 314.96) (xy 405.13 314.96)))
  (wire (pts (xy 504.19 486.41) (xy 487.68 486.41)))
  (wire (pts (xy 619.76 455.93) (xy 624.84 455.93)))
  (wire (pts (xy 562.61 360.68) (xy 562.61 269.24)))
  (wire (pts (xy 412.75 309.88) (xy 431.8 309.88)))
  (wire (pts (xy 486.41 327.66) (xy 486.41 337.82)))
  (wire (pts (xy 431.8 314.96) (xy 431.8 325.12)))
  (wire (pts (xy 506.73 392.43) (xy 480.06 392.43)))
  (wire (pts (xy 515.62 340.36) (xy 568.96 340.36)))
  (wire (pts (xy 415.29 354.33) (xy 431.8 354.33)))
  (wire (pts (xy 447.04 261.62) (xy 495.3 261.62)))
  (wire (pts (xy 571.5 402.59) (xy 571.5 410.21)))
  (wire (pts (xy 506.73 397.51) (xy 410.21 397.51)))
  (wire (pts (xy 482.6 405.13) (xy 506.73 405.13)))
  (wire (pts (xy 500.38 422.91) (xy 500.38 463.55)))
  (wire (pts (xy 502.92 269.24) (xy 529.59 269.24)))
  (wire (pts (xy 612.14 463.55) (xy 624.84 463.55)))
  (wire (pts (xy 581.66 449.58) (xy 581.66 387.35)))
  (wire (pts (xy 474.98 438.15) (xy 506.73 438.15)))
  (wire (pts (xy 619.76 452.12) (xy 619.76 455.93)))
  (wire (pts (xy 405.13 314.96) (xy 405.13 344.17)))
  (wire (pts (xy 506.73 377.19) (xy 506.73 360.68)))
  (wire (pts (xy 619.76 455.93) (xy 619.76 458.47)))
  (wire (pts (xy 506.73 415.29) (xy 492.76 415.29)))
  (wire (pts (xy 407.67 330.2) (xy 415.29 330.2)))
  (wire (pts (xy 505.46 325.12) (xy 508 325.12)))
  (wire (pts (xy 542.29 387.35) (xy 579.12 387.35)))
  (wire (pts (xy 585.47 463.55) (xy 585.47 481.33)))
  (wire (pts (xy 624.84 483.87) (xy 579.12 483.87)))
  (wire (pts (xy 495.3 417.83) (xy 495.3 534.67)))
  (wire (pts (xy 504.19 488.95) (xy 490.22 488.95)))
  (wire (pts (xy 617.22 452.12) (xy 617.22 458.47)))
  (wire (pts (xy 589.28 379.73) (xy 589.28 392.43)))
  (wire (pts (xy 431.8 344.17) (xy 405.13 344.17)))
  (wire (pts (xy 544.83 438.15) (xy 544.83 439.42)))
  (wire (pts (xy 490.22 312.42) (xy 472.44 312.42)))
  (wire (pts (xy 500.38 463.55) (xy 585.47 463.55)))
  (wire (pts (xy 495.3 534.67) (xy 504.19 534.67)))
  (wire (pts (xy 486.41 327.66) (xy 490.22 327.66)))
  (wire (pts (xy 452.12 283.21) (xy 518.16 283.21)))
  (wire (pts (xy 585.47 481.33) (xy 624.84 481.33)))
  (wire (pts (xy 482.6 405.13) (xy 482.6 481.33)))
  (wire (pts (xy 542.29 405.13) (xy 600.71 405.13)))
  (wire (pts (xy 619.76 458.47) (xy 624.84 458.47)))
  (wire (pts (xy 487.68 410.21) (xy 506.73 410.21)))
  (wire (pts (xy 542.29 392.43) (xy 584.2 392.43)))
  (wire (pts (xy 410.21 339.09) (xy 410.21 397.51)))
  (wire (pts (xy 524.51 368.3) (xy 524.51 369.57)))
  (wire (pts (xy 609.6 452.12) (xy 609.6 466.09)))
  (wire (pts (xy 506.73 394.97) (xy 412.75 394.97)))
  (wire (pts (xy 480.06 392.43) (xy 480.06 353.06)))
  (wire (pts (xy 476.25 274.32) (xy 476.25 269.24)))
  (wire (pts (xy 619.76 488.95) (xy 619.76 496.57)))
  (wire (pts (xy 566.42 355.6) (xy 566.42 412.75)))
  (wire (pts (xy 449.58 274.32) (xy 476.25 274.32)))
  (wire (pts (xy 506.73 400.05) (xy 407.67 400.05)))
  (text "H" (at 530.86 532.13 0))
  (text "M" (at 530.86 499.11 0))
  (text "B" (at 530.86 547.37 0))
  (text "CN4-12" (at 593.09 407.67 0))
  (text "G" (at 530.86 534.67 0))
  (text "CN4-14" (at 593.09 412.75 0))
  (text "NUM LOCK" (at 516.89 339.09 0))
  (text "J" (at 530.86 527.05 0))
  (text "I" (at 530.86 529.59 0))
  (text "P" (at 530.86 491.49 0))
  (text "E" (at 530.86 539.75 0))
  (text "CN4-16" (at 593.09 417.83 0))
  (text "S" (at 530.86 483.87 0))
  (text "N" (at 530.86 496.57 0))
  (text "F" (at 530.86 537.21 0))
  (text "CN4-2" (at 593.09 382.27 0))
  (text "K" (at 530.86 504.19 0))
  (text "ALPHA/CAPS LOCK" (at 516.89 308.61 0))
  (text "O" (at 530.86 494.03 0))
  (text "A" (at 530.86 549.91 0))
  (text "Q" (at 530.86 488.95 0))
  (text "Data" (at 486.41 261.62 0))
  (text "CN4-6" (at 593.09 392.43 0))
  (text "Reset" (at 506.73 269.24 0))
  (text "CN4-15" (at 593.09 415.29 0))
  (text "T" (at 530.86 481.33 0))
  (text "D" (at 530.86 542.29 0))
  (text "ON LINE" (at 516.89 323.85 0))
  (text "L" (at 530.86 501.65 0))
  (text "R" (at 530.86 486.41 0))
  (text "CN4-1" (at 593.09 379.73 0))
  (text "C" (at 530.86 544.83 0))
  (text "Clock" (at 478.79 269.24 0))
  (text "HOLD" (at 516.89 354.33 0))
  (label "CN4-8" (at 593.09 397.51 0))
  (label "CN4-10" (at 593.09 402.59 0))
  (label "CN4-4" (at 593.09 387.35 0))
  (label "CN4-13" (at 593.09 410.21 0))
  (label "CN4-11" (at 593.09 405.13 0))
  (label "CN4-5" (at 593.09 389.89 0))
  (label "CN4-9" (at 593.09 400.05 0))
  (label "CN4-7" (at 593.09 394.97 0))
  (symbol (lib_id "74xx:74LS38") (at 439.42 341.63 0) (unit 3)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M5" (id 0) (at 439.42 332.74 0))
    (property "Value" "74LS38" (id 1) (at 439.42 335.28 0))
    (property "Footprint" "" (id 2) (at 439.42 341.63 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 439.42 341.63 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS38") (at 439.42 356.87 0) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M5" (id 0) (at 439.42 347.98 0))
    (property "Value" "74LS38" (id 1) (at 439.42 350.52 0))
    (property "Footprint" "" (id 2) (at 439.42 356.87 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 439.42 356.87 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS151") (at 637.54 471.17 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M7" (id 0) (at 639.5594 448.31 0))
    (property "Value" "74LS151" (id 1) (at 639.5594 450.85 0))
    (property "Footprint" "" (id 2) (at 637.54 471.17 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS151" (id 3) (at 637.54 471.17 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "74xx:74LS145") (at 516.89 537.21 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M3" (id 0) (at 518.9094 519.43 0))
    (property "Value" "74LS145" (id 1) (at 518.9094 521.97 0))
    (property "Footprint" "" (id 2) (at 516.89 537.21 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS145" (id 3) (at 516.89 537.21 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "74xx:74LS14") (at 467.36 438.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M4" (id 0) (at 467.36 429.26 0))
    (property "Value" "74LS14" (id 1) (at 467.36 431.8 0))
    (property "Footprint" "" (id 2) (at 467.36 438.15 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 467.36 438.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS38") (at 497.84 325.12 0) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 497.84 316.23 0))
    (property "Value" "74LS38" (id 1) (at 497.84 318.77 0))
    (property "Footprint" "" (id 2) (at 497.84 325.12 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 497.84 325.12 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:GND") (at 547.37 382.27 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 553.72 382.27 0))
    (property "Value" "GND" (id 1) (at 551.18 382.2699 90))
    (property "Footprint" "" (id 2) (at 547.37 382.27 0))
    (property "Datasheet" "" (id 3) (at 547.37 382.27 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 447.04 361.95 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 449.58 360.6799 0))
    (property "Value" "R" (id 1) (at 449.58 363.2199 0))
    (property "Footprint" "" (id 2) (at 448.818 361.95 90))
    (property "Datasheet" "~" (id 3) (at 447.04 361.95 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 486.41 307.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 486.41 311.15 0))
    (property "Value" "+5V" (id 1) (at 486.41 302.26 0))
    (property "Footprint" "" (id 2) (at 486.41 307.34 0))
    (property "Datasheet" "" (id 3) (at 486.41 307.34 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS14") (at 422.91 339.09 0) (unit 3)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M4" (id 0) (at 422.91 330.2 0))
    (property "Value" "74LS14" (id 1) (at 422.91 332.74 0))
    (property "Footprint" "" (id 2) (at 422.91 339.09 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 422.91 339.09 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS38") (at 497.84 355.6 0) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 497.84 346.71 0))
    (property "Value" "74LS38" (id 1) (at 497.84 349.25 0))
    (property "Footprint" "" (id 2) (at 497.84 355.6 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 497.84 355.6 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS145") (at 516.89 491.49 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M2" (id 0) (at 518.9094 473.71 0))
    (property "Value" "74LS145" (id 1) (at 518.9094 476.25 0))
    (property "Footprint" "" (id 2) (at 516.89 491.49 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS145" (id 3) (at 516.89 491.49 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Connector:DIN-8") (at 495.3 269.24 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J?" (id 0) (at 496.9511 259.08 0))
    (property "Value" "DIN-8" (id 1) (at 496.9511 261.62 0))
    (property "Footprint" "" (id 2) (at 495.3 269.24 0))
    (property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf" (id 3) (at 495.3 269.24 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "74xx:74LS38") (at 497.84 309.88 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 497.84 300.99 0))
    (property "Value" "74LS38" (id 1) (at 497.84 303.53 0))
    (property "Footprint" "" (id 2) (at 497.84 309.88 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 497.84 309.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS38") (at 497.84 340.36 0) (unit 3)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 497.84 331.47 0))
    (property "Value" "74LS38" (id 1) (at 497.84 334.01 0))
    (property "Footprint" "" (id 2) (at 497.84 340.36 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 497.84 340.36 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "Device:R_Network06") (at 614.68 447.04 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "RN?" (id 0) (at 622.3 446.0239 0))
    (property "Value" "R_Network06" (id 1) (at 622.3 448.5639 0))
    (property "Footprint" "Resistor_THT:R_Array_SIP7" (id 2) (at 624.205 447.04 90))
    (property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf" (id 3) (at 614.68 447.04 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
  )
  (symbol (lib_id "Device:R") (at 511.81 309.88 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 511.81 303.53 90))
    (property "Value" "R" (id 1) (at 511.81 306.07 90))
    (property "Footprint" "" (id 2) (at 511.81 308.102 90))
    (property "Datasheet" "~" (id 3) (at 511.81 309.88 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS14") (at 449.58 438.15 0) (unit 6)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M4" (id 0) (at 449.58 429.26 0))
    (property "Value" "74LS14" (id 1) (at 449.58 431.8 0))
    (property "Footprint" "" (id 2) (at 449.58 438.15 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 449.58 438.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:+5V") (at 637.54 448.31 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 637.54 452.12 0))
    (property "Value" "+5V" (id 1) (at 637.54 443.23 0))
    (property "Footprint" "" (id 2) (at 637.54 448.31 0))
    (property "Datasheet" "" (id 3) (at 637.54 448.31 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Buzzer") (at 449.58 374.65 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "BZ?" (id 0) (at 445.77 368.3 90))
    (property "Value" "Buzzer" (id 1) (at 445.77 370.84 90))
    (property "Footprint" "" (id 2) (at 452.12 374.015 90))
    (property "Datasheet" "~" (id 3) (at 452.12 374.015 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "MCU_Intel:8049") (at 524.51 407.67 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M1" (id 0) (at 526.5294 368.3 0))
    (property "Value" "8049" (id 1) (at 526.5294 370.84 0))
    (property "Footprint" "" (id 2) (at 524.51 402.59 0))
    (property "Datasheet" "" (id 3) (at 524.51 402.59 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:+5V") (at 452.12 372.11 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 452.12 375.92 0))
    (property "Value" "+5V" (id 1) (at 452.12 367.03 0))
    (property "Footprint" "" (id 2) (at 452.12 372.11 0))
    (property "Datasheet" "" (id 3) (at 452.12 372.11 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS38") (at 439.42 312.42 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M5" (id 0) (at 439.42 303.53 0))
    (property "Value" "74LS38" (id 1) (at 439.42 306.07 0))
    (property "Footprint" "" (id 2) (at 439.42 312.42 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 439.42 312.42 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS38") (at 439.42 327.66 0) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M5" (id 0) (at 439.42 318.77 0))
    (property "Value" "74LS38" (id 1) (at 439.42 321.31 0))
    (property "Footprint" "" (id 2) (at 439.42 327.66 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 439.42 327.66 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:+5V") (at 524.51 368.3 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 524.51 372.11 0))
    (property "Value" "+5V" (id 1) (at 524.51 363.22 0))
    (property "Footprint" "" (id 2) (at 524.51 368.3 0))
    (property "Datasheet" "" (id 3) (at 524.51 368.3 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 511.81 340.36 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 511.81 334.01 90))
    (property "Value" "R" (id 1) (at 511.81 336.55 90))
    (property "Footprint" "" (id 2) (at 511.81 338.582 90))
    (property "Datasheet" "~" (id 3) (at 511.81 340.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 471.17 266.7 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 464.82 266.7 0))
    (property "Value" "GND" (id 1) (at 472.44 266.6999 90))
    (property "Footprint" "" (id 2) (at 471.17 266.7 0))
    (property "Datasheet" "" (id 3) (at 471.17 266.7 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 405.13 309.88 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 405.13 313.69 0))
    (property "Value" "+5V" (id 1) (at 405.13 304.8 0))
    (property "Footprint" "" (id 2) (at 405.13 309.88 0))
    (property "Datasheet" "" (id 3) (at 405.13 309.88 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Crystal") (at 547.37 435.61 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Y?" (id 0) (at 551.18 434.3399 90))
    (property "Value" "Crystal" (id 1) (at 551.18 436.8799 90))
    (property "Footprint" "" (id 2) (at 547.37 435.61 0))
    (property "Datasheet" "~" (id 3) (at 547.37 435.61 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 511.81 355.6 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 511.81 349.25 90))
    (property "Value" "R" (id 1) (at 511.81 351.79 90))
    (property "Footprint" "" (id 2) (at 511.81 353.822 90))
    (property "Datasheet" "~" (id 3) (at 511.81 355.6 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 637.54 496.57 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 637.54 502.92 0))
    (property "Value" "GND" (id 1) (at 637.54 501.65 0))
    (property "Footprint" "" (id 2) (at 637.54 496.57 0))
    (property "Datasheet" "" (id 3) (at 637.54 496.57 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 518.16 265.43 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 518.16 269.24 0))
    (property "Value" "+5V" (id 1) (at 518.16 260.35 0))
    (property "Footprint" "" (id 2) (at 518.16 265.43 0))
    (property "Datasheet" "" (id 3) (at 518.16 265.43 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 589.28 374.65 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 589.28 378.46 0))
    (property "Value" "+5V" (id 1) (at 589.28 369.57 0))
    (property "Footprint" "" (id 2) (at 589.28 374.65 0))
    (property "Datasheet" "" (id 3) (at 589.28 374.65 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 511.81 325.12 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 511.81 318.77 90))
    (property "Value" "R" (id 1) (at 511.81 321.31 90))
    (property "Footprint" "" (id 2) (at 511.81 323.342 90))
    (property "Datasheet" "~" (id 3) (at 511.81 325.12 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS14") (at 537.21 269.24 0) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M4" (id 0) (at 537.21 260.35 0))
    (property "Value" "74LS14" (id 1) (at 537.21 262.89 0))
    (property "Footprint" "" (id 2) (at 537.21 269.24 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 537.21 269.24 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS14") (at 553.72 269.24 0) (unit 5)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M4" (id 0) (at 553.72 260.35 0))
    (property "Value" "74LS14" (id 1) (at 553.72 262.89 0))
    (property "Footprint" "" (id 2) (at 553.72 269.24 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 553.72 269.24 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS14") (at 422.91 330.2 0) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M4" (id 0) (at 422.91 321.31 0))
    (property "Value" "74LS14" (id 1) (at 422.91 323.85 0))
    (property "Footprint" "" (id 2) (at 422.91 330.2 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 422.91 330.2 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "BZ?") (unit 1) (value "Buzzer") (footprint "")
    )
    (path
      (reference "J?") (unit 1) (value "DIN-8") (footprint "")
    )
    (path
      (reference "M1") (unit 1) (value "8049") (footprint "")
    )
    (path
      (reference "M2") (unit 1) (value "74LS145") (footprint "")
    )
    (path
      (reference "M3") (unit 1) (value "74LS145") (footprint "")
    )
    (path
      (reference "M4") (unit 1) (value "74LS14") (footprint "")
    )
    (path
      (reference "M4") (unit 2) (value "74LS14") (footprint "")
    )
    (path
      (reference "M4") (unit 3) (value "74LS14") (footprint "")
    )
    (path
      (reference "M4") (unit 4) (value "74LS14") (footprint "")
    )
    (path
      (reference "M4") (unit 5) (value "74LS14") (footprint "")
    )
    (path
      (reference "M4") (unit 6) (value "74LS14") (footprint "")
    )
    (path
      (reference "M5") (unit 1) (value "74LS38") (footprint "")
    )
    (path
      (reference "M5") (unit 2) (value "74LS38") (footprint "")
    )
    (path
      (reference "M5") (unit 3) (value "74LS38") (footprint "")
    )
    (path
      (reference "M5") (unit 4) (value "74LS38") (footprint "")
    )
    (path
      (reference "M6") (unit 1) (value "74LS38") (footprint "")
    )
    (path
      (reference "M6") (unit 2) (value "74LS38") (footprint "")
    )
    (path
      (reference "M6") (unit 3) (value "74LS38") (footprint "")
    )
    (path
      (reference "M6") (unit 4) (value "74LS38") (footprint "")
    )
    (path
      (reference "M7") (unit 1) (value "74LS151") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "RN?") (unit 1) (value "R_Network06") (footprint "Resistor_THT:R_Array_SIP7")
    )
    (path
      (reference "Y?") (unit 1) (value "Crystal") (footprint "")
    )
  )
)
