(kicad_sch (version 20211123) (generator eeschema)
  (paper "A0")
  (lib_symbols
    (symbol "74xx_IEEE:7406" (pin_names (offset 0.762)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 3.81 7.62 0))
      (property "Value" "7406" (id 1) (at 6.35 -8.89 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "7406_0_0"
        (polyline
          (pts
            (xy -3.81 1.27)
            (xy -3.81 -1.27)
            (xy -2.54 0)
            (xy -3.81 1.27)
            (xy -3.81 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.048 1.016)
            (xy 4.064 2.032)
            (xy 2.54 3.556)
            (xy 1.016 2.032)
            (xy 2.032 1.016)
            (xy 1.016 1.016)
            (xy 4.064 1.016)
            (xy 4.064 1.016)
          )
          (fill (type none))
        )
      )
      (symbol "7406_0_1"
        (rectangle (start -6.35 6.35) (end 6.35 -6.35)
          (fill (type none))
        )
        (pin power_in line (at 0 6.35 270) (length 0) hide
          (name "Vcc")
          (number "14")
        )
        (pin power_in line (at 0 -6.35 90) (length 0) hide
          (name "Gnd")
          (number "7")
        )
      )
      (symbol "7406_1_1"
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "1")
        )
        (pin open_collector inverted (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "2")
        )
      )
      (symbol "7406_2_1"
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "3")
        )
        (pin open_collector inverted (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "4")
        )
      )
      (symbol "7406_3_1"
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "5")
        )
        (pin open_collector inverted (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "6")
        )
      )
      (symbol "7406_4_1"
        (pin open_collector inverted (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "8")
        )
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "9")
        )
      )
      (symbol "7406_5_1"
        (pin open_collector inverted (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "10")
        )
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "11")
        )
      )
      (symbol "7406_6_1"
        (pin open_collector inverted (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "12")
        )
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "13")
        )
      )
    )
    (symbol "Connector:Conn_01x02_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 2.54 0))
      (property "Value" "Conn_01x02_Male" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x02_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Connector:Conn_01x03_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 5.08 0))
      (property "Value" "Conn_01x03_Male" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x03_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
      )
    )
    (symbol "Connector:Conn_01x04_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 5.08 0))
      (property "Value" "Conn_01x04_Male" (id 1) (at 0 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x04_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
      )
    )
    (symbol "Connector:Conn_01x05_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 7.62 0))
      (property "Value" "Conn_01x05_Male" (id 1) (at 0 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x05_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 5.08)
            (xy 0.8636 5.08)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (rectangle (start 0.8636 5.207) (end 0 4.953)
          (fill (type outline))
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
      )
    )
    (symbol "Connector:Conn_01x08_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 10.16 0))
      (property "Value" "Conn_01x08_Male" (id 1) (at 0 -12.7 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x08_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -10.16)
            (xy 0.8636 -10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -7.62)
            (xy 0.8636 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 5.08)
            (xy 0.8636 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 7.62)
            (xy 0.8636 7.62)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -10.033) (end 0 -10.287)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -7.493) (end 0 -7.747)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (rectangle (start 0.8636 5.207) (end 0 4.953)
          (fill (type outline))
        )
        (rectangle (start 0.8636 7.747) (end 0 7.493)
          (fill (type outline))
        )
        (pin passive line (at 5.08 7.62 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at 5.08 -7.62 180) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 5.08 -10.16 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
      )
    )
    (symbol "Connector:DIN-5_180degree" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 3.175 5.715 0))
      (property "Value" "DIN-5_180degree" (id 1) (at 0 -6.35 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "circular DIN connector stereo audio" (id 4) (at 0 0 0))
      (property "ki_description" "5-pin DIN connector (5-pin DIN-5 stereo)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIN*" (id 6) (at 0 0 0))
      (symbol "DIN-5_180degree_0_1"
        (arc (start -5.08 0) (mid -3.8609 -3.3364) (end -0.762 -5.08)
          (fill (type none))
        )
        (circle (center -3.048 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center -2.286 2.286) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 0)
            (xy -3.556 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 0)
            (xy 3.556 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.54)
            (xy -4.318 2.54)
            (xy -2.794 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 2.54)
            (xy 4.318 2.54)
            (xy 2.794 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 -4.953)
            (xy -0.762 -4.191)
            (xy 0.762 -4.191)
            (xy 0.762 -4.953)
          )
          (fill (type none))
        )
        (circle (center 0 3.302) (radius 0.508)
          (fill (type none))
        )
        (arc (start 0.762 -5.08) (mid 3.8685 -3.343) (end 5.08 0)
          (fill (type none))
        )
        (circle (center 2.286 2.286) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.048 0) (radius 0.508)
          (fill (type none))
        )
        (arc (start 5.08 0) (mid 0 5.08) (end -5.08 0)
          (fill (type none))
        )
      )
      (symbol "DIN-5_180degree_1_1"
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at -7.62 2.54 0) (length 2.54)
          (name "~")
          (number "4")
        )
        (pin passive line (at 7.62 2.54 180) (length 2.54)
          (name "~")
          (number "5")
        )
      )
    )
    (symbol "Connector:TestPoint" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 6.858 0))
      (property "Value" "TestPoint" (id 1) (at 0 5.08 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_0_1"
        (circle (center 0 3.302) (radius 0.762)
          (fill (type none))
        )
      )
      (symbol "TestPoint_1_1"
        (pin passive line (at 0 0 90) (length 2.54)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x05_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 7.62 0))
      (property "Value" "Conn_02x05_Odd_Even" (id 1) (at 1.27 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x05_Odd_Even_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 6.35) (end 3.81 -6.35)
          (fill (type background))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Polarized_US" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_Polarized_US" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor, US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "C_Polarized_US_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.778)
            (xy -1.27 2.794)
          )
          (fill (type none))
        )
        (arc (start 2.032 -1.27) (mid 0 -0.5572) (end -2.032 -1.27)
          (fill (type none))
        )
      )
      (symbol "C_Polarized_US_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 3.302)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0))
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:L" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at -1.27 0 90))
      (property "Value" "L" (id 1) (at 1.905 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 6) (at 0 0 0))
      (symbol "L_0_1"
        (arc (start 0 -2.54) (mid 0.635 -1.905) (end 0 -1.27)
          (fill (type none))
        )
        (arc (start 0 -1.27) (mid 0.635 -0.635) (end 0 0)
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 0.635) (end 0 1.27)
          (fill (type none))
        )
        (arc (start 0 1.27) (mid 0.635 1.905) (end 0 2.54)
          (fill (type none))
        )
      )
      (symbol "L_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:Opamp_Dual" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 5.08 0))
      (property "Value" "Opamp_Dual" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "dual opamp" (id 5) (at 0 0 0))
      (property "ki_description" "Dual operational amplifier" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* MSOP*3x3mm*P0.65mm* SSOP*2.95x2.8mm*P0.65mm* TSSOP*3x3mm*P0.65mm* VSSOP*P0.5mm* TO?99*" (id 7) (at 0 0 0))
      (symbol "Opamp_Dual_1_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "2")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "3")
        )
      )
      (symbol "Opamp_Dual_2_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "5")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "6")
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "7")
        )
      )
      (symbol "Opamp_Dual_3_1"
        (pin power_in line (at -2.54 -7.62 90) (length 3.81)
          (name "V-")
          (number "4")
        )
        (pin power_in line (at -2.54 7.62 270) (length 3.81)
          (name "V+")
          (number "8")
        )
      )
    )
    (symbol "Device:Q_NPN_EBC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0))
      (property "Value" "Q_NPN_EBC" (id 1) (at 5.08 -1.27 0))
      (property "Footprint" "" (id 2) (at 5.08 2.54 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "transistor NPN" (id 4) (at 0 0 0))
      (property "ki_description" "NPN transistor, emitter/base/collector" (id 5) (at 0 0 0))
      (symbol "Q_NPN_EBC_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "Q_NPN_EBC_1_1"
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "1")
        )
        (pin passive line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "Device:Q_PNP_BCE" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0))
      (property "Value" "Q_PNP_BCE" (id 1) (at 5.08 -1.27 0))
      (property "Footprint" "" (id 2) (at 5.08 2.54 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "transistor PNP" (id 4) (at 0 0 0))
      (property "ki_description" "PNP transistor, base/collector/emitter" (id 5) (at 0 0 0))
      (symbol "Q_PNP_BCE_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 -1.778)
            (xy 1.778 -2.286)
            (xy 1.27 -1.27)
            (xy 2.286 -1.778)
            (xy 2.286 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "Q_PNP_BCE_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "3")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Network05" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RN" (id 0) (at -7.62 0 90))
      (property "Value" "R_Network05" (id 1) (at 7.62 0 90))
      (property "Footprint" "Resistor_THT:R_Array_SIP6" (id 2) (at 9.525 0 90))
      (property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "R network star-topology" (id 4) (at 0 0 0))
      (property "ki_description" "5 resistor network, star topology, bussed resistors, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R?Array?SIP*" (id 6) (at 0 0 0))
      (symbol "R_Network05_0_1"
        (rectangle (start -6.35 -3.175) (end 6.35 3.175)
          (fill (type background))
        )
        (rectangle (start -5.842 1.524) (end -4.318 -2.54)
          (fill (type none))
        )
        (circle (center -5.08 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -3.302 1.524) (end -1.778 -2.54)
          (fill (type none))
        )
        (circle (center -2.54 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -0.762 1.524) (end 0.762 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.524)
            (xy -5.08 2.286)
            (xy -2.54 2.286)
            (xy -2.54 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.524)
            (xy -2.54 2.286)
            (xy 0 2.286)
            (xy 0 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.524)
            (xy 0 2.286)
            (xy 2.54 2.286)
            (xy 2.54 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.524)
            (xy 2.54 2.286)
            (xy 5.08 2.286)
            (xy 5.08 1.524)
          )
          (fill (type none))
        )
        (circle (center 0 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 1.778 1.524) (end 3.302 -2.54)
          (fill (type none))
        )
        (circle (center 2.54 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 4.318 1.524) (end 5.842 -2.54)
          (fill (type none))
        )
      )
      (symbol "R_Network05_1_1"
        (pin passive line (at -5.08 5.08 270) (length 2.54)
          (name "common")
          (number "1")
        )
        (pin passive line (at -5.08 -5.08 90) (length 1.27)
          (name "R1")
          (number "2")
        )
        (pin passive line (at -2.54 -5.08 90) (length 1.27)
          (name "R2")
          (number "3")
        )
        (pin passive line (at 0 -5.08 90) (length 1.27)
          (name "R3")
          (number "4")
        )
        (pin passive line (at 2.54 -5.08 90) (length 1.27)
          (name "R4")
          (number "5")
        )
        (pin passive line (at 5.08 -5.08 90) (length 1.27)
          (name "R5")
          (number "6")
        )
      )
    )
    (symbol "Diode:1N4004" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "1N4004" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 0 -4.445 0))
      (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "400V 1A General Purpose Rectifier Diode, DO-41" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*DO?41*" (id 6) (at 0 0 0))
      (symbol "1N4004_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "1N4004_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Interface_UART:SN75176AP" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -4.318 8.89 0))
      (property "Value" "SN75176AP" (id 1) (at 1.016 8.89 0))
      (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (id 2) (at 0 -12.7 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75176a.pdf" (id 3) (at 40.64 -5.08 0))
      (property "ki_keywords" "Differential bus transceiver" (id 4) (at 0 0 0))
      (property "ki_description" "Differential RS-422/RS-485 bus transceiver, DIP-8" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0))
      (symbol "SN75176AP_0_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
      (symbol "SN75176AP_1_1"
        (pin output line (at -7.62 -5.08 0) (length 2.54)
          (name "R")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "~{RE}")
          (number "2")
        )
        (pin input line (at -7.62 5.08 0) (length 2.54)
          (name "DE")
          (number "3")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "D")
          (number "4")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "5")
        )
        (pin bidirectional line (at 7.62 -5.08 180) (length 2.54)
          (name "A")
          (number "6")
        )
        (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
          (name "B")
          (number "7")
        )
        (pin power_in line (at 0 10.16 270) (length 2.54)
          (name "VCC")
          (number "8")
        )
      )
    )
    (symbol "Jumper:Jumper_2_Bridged" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 1.905 0))
      (property "Value" "Jumper_2_Bridged" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "Jumper SPST" (id 4) (at 0 0 0))
      (property "ki_description" "Jumper, 2-pole, closed/bridged" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*" (id 6) (at 0 0 0))
      (symbol "Jumper_2_Bridged_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Bridged_0_1"
        (arc (start 1.524 0.254) (mid 0 0.762) (end -1.524 0.254)
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Bridged_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "Jumper:Jumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.794 0))
      (property "Value" "Jumper_2_Open" (id 1) (at 0 -2.286 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "Jumper SPST" (id 4) (at 0 0 0))
      (property "ki_description" "Jumper, 2-pole, open" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*" (id 6) (at 0 0 0))
      (symbol "Jumper_2_Open_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_0_1"
        (arc (start 1.524 1.27) (mid 0 1.778) (end -1.524 1.27)
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "MCU_Intel:8749" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -13.97 35.56 0))
      (property "Value" "8749" (id 1) (at 8.89 35.56 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "MCS-48 uC Microcontroller" (id 4) (at 0 0 0))
      (property "ki_description" "i8748, MCS-48 8-bit Microcontroller with Internal EPROM, 2KB EPROM, 128B RAM, DIP-40" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP* PDIP*" (id 6) (at 0 0 0))
      (symbol "8749_1_1"
        (rectangle (start -13.97 -34.29) (end 13.97 34.29)
          (fill (type background))
        )
        (pin input line (at -17.78 -25.4 0) (length 3.81)
          (name "T0")
          (number "1")
        )
        (pin output output_low (at 17.78 -12.7 180) (length 3.81)
          (name "~{WR}")
          (number "10")
        )
        (pin output line (at 17.78 -2.54 180) (length 3.81)
          (name "ALE")
          (number "11")
        )
        (pin bidirectional line (at 17.78 20.32 180) (length 3.81)
          (name "DB.0")
          (number "12")
        )
        (pin bidirectional line (at 17.78 17.78 180) (length 3.81)
          (name "DB.1")
          (number "13")
        )
        (pin bidirectional line (at 17.78 15.24 180) (length 3.81)
          (name "DB.2")
          (number "14")
        )
        (pin bidirectional line (at 17.78 12.7 180) (length 3.81)
          (name "DB.3")
          (number "15")
        )
        (pin bidirectional line (at 17.78 10.16 180) (length 3.81)
          (name "DB.4")
          (number "16")
        )
        (pin bidirectional line (at 17.78 7.62 180) (length 3.81)
          (name "DB.5")
          (number "17")
        )
        (pin bidirectional line (at 17.78 5.08 180) (length 3.81)
          (name "DB.6")
          (number "18")
        )
        (pin bidirectional line (at 17.78 2.54 180) (length 3.81)
          (name "DB.7")
          (number "19")
        )
        (pin input line (at 17.78 -25.4 180) (length 3.81)
          (name "X1")
          (number "2")
        )
        (pin power_in line (at 0 -38.1 90) (length 3.81)
          (name "GND")
          (number "20")
        )
        (pin bidirectional line (at -17.78 2.54 0) (length 3.81)
          (name "P2.0")
          (number "21")
        )
        (pin bidirectional line (at -17.78 0 0) (length 3.81)
          (name "P2.1")
          (number "22")
        )
        (pin bidirectional line (at -17.78 -2.54 0) (length 3.81)
          (name "P2.2")
          (number "23")
        )
        (pin bidirectional line (at -17.78 -5.08 0) (length 3.81)
          (name "P2.3")
          (number "24")
        )
        (pin output line (at -17.78 -20.32 0) (length 3.81)
          (name "PROG")
          (number "25")
        )
        (pin power_in line (at 17.78 30.48 180) (length 3.81)
          (name "Vpp/VDD")
          (number "26")
        )
        (pin bidirectional line (at -17.78 25.4 0) (length 3.81)
          (name "P1.0")
          (number "27")
        )
        (pin bidirectional line (at -17.78 22.86 0) (length 3.81)
          (name "P1.1")
          (number "28")
        )
        (pin bidirectional line (at -17.78 20.32 0) (length 3.81)
          (name "P1.2")
          (number "29")
        )
        (pin output line (at 17.78 -30.48 180) (length 3.81)
          (name "X2")
          (number "3")
        )
        (pin bidirectional line (at -17.78 17.78 0) (length 3.81)
          (name "P1.3")
          (number "30")
        )
        (pin bidirectional line (at -17.78 15.24 0) (length 3.81)
          (name "P1.4")
          (number "31")
        )
        (pin bidirectional line (at -17.78 12.7 0) (length 3.81)
          (name "P1.5")
          (number "32")
        )
        (pin bidirectional line (at -17.78 10.16 0) (length 3.81)
          (name "P1.6")
          (number "33")
        )
        (pin bidirectional line (at -17.78 7.62 0) (length 3.81)
          (name "P1.7")
          (number "34")
        )
        (pin bidirectional line (at -17.78 -7.62 0) (length 3.81)
          (name "P2.4")
          (number "35")
        )
        (pin bidirectional line (at -17.78 -10.16 0) (length 3.81)
          (name "P2.5")
          (number "36")
        )
        (pin bidirectional line (at -17.78 -12.7 0) (length 3.81)
          (name "P2.6")
          (number "37")
        )
        (pin bidirectional line (at -17.78 -15.24 0) (length 3.81)
          (name "P2.7")
          (number "38")
        )
        (pin input line (at -17.78 -27.94 0) (length 3.81)
          (name "T1")
          (number "39")
        )
        (pin input inverted (at -17.78 30.48 0) (length 3.81)
          (name "~{RESET}")
          (number "4")
        )
        (pin power_in line (at 0 38.1 270) (length 3.81)
          (name "VCC")
          (number "40")
        )
        (pin input inverted (at 17.78 -17.78 180) (length 3.81)
          (name "~{SS}")
          (number "5")
        )
        (pin input inverted (at -17.78 -30.48 0) (length 3.81)
          (name "~{INT}")
          (number "6")
        )
        (pin input line (at 17.78 25.4 180) (length 3.81)
          (name "EA")
          (number "7")
        )
        (pin output output_low (at 17.78 -10.16 180) (length 3.81)
          (name "~{RD}")
          (number "8")
        )
        (pin output output_low (at 17.78 -7.62 180) (length 3.81)
          (name "~{PSEN}")
          (number "9")
        )
      )
    )
    (symbol "Power_Supervisor:MC34064P" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -5.08 5.08 0))
      (property "Value" "MC34064P" (id 1) (at 5.08 5.08 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline" (id 2) (at 0 -12.7 0))
      (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF" (id 3) (at 0 0 0))
      (property "ki_keywords" "Power Supervisor" (id 4) (at 0 0 0))
      (property "ki_description" "Undervoltage Sensing Circuit, TO-92" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?92L?Inline*" (id 6) (at 0 0 0))
      (symbol "MC34064P_0_1"
        (rectangle (start -6.35 -5.08) (end 6.35 3.81)
          (fill (type background))
        )
      )
      (symbol "MC34064P_1_1"
        (pin open_collector line (at 8.89 1.27 180) (length 2.54)
          (name "~{RESET}")
          (number "1")
        )
        (pin input line (at -8.89 1.27 0) (length 2.54)
          (name "IN")
          (number "2")
        )
        (pin input line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "3")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 212.09 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 243.84 173.99) (diameter 0) (color 0 0 0 0))
  (junction (at 124.46 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 293.37 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 223.52 50.8) (diameter 0) (color 0 0 0 0))
  (junction (at 287.02 172.72) (diameter 0) (color 0 0 0 0))
  (junction (at 201.93 36.83) (diameter 0) (color 0 0 0 0))
  (junction (at 135.89 116.84) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 69.85) (diameter 0) (color 0 0 0 0))
  (junction (at 125.73 104.14) (diameter 0) (color 0 0 0 0))
  (junction (at 236.22 173.99) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 149.86) (diameter 0) (color 0 0 0 0))
  (junction (at 312.42 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 312.42 63.5) (diameter 0) (color 0 0 0 0))
  (junction (at 243.84 162.56) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 317.5 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 298.45 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 287.02 180.34) (diameter 0) (color 0 0 0 0))
  (junction (at 190.5 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 87.63 127) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 50.8) (diameter 0) (color 0 0 0 0))
  (junction (at 179.07 34.29) (diameter 0) (color 0 0 0 0))
  (junction (at 91.44 124.46) (diameter 0) (color 0 0 0 0))
  (junction (at 228.6 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 325.12 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 167.64 175.26) (diameter 0) (color 0 0 0 0))
  (junction (at 298.45 172.72) (diameter 0) (color 0 0 0 0))
  (junction (at 312.42 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 236.22 124.46) (diameter 0) (color 0 0 0 0))
  (junction (at 76.2 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 149.86) (diameter 0) (color 0 0 0 0))
  (junction (at 78.74 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 269.24 180.34) (diameter 0) (color 0 0 0 0))
  (junction (at 185.42 39.37) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 124.46) (diameter 0) (color 0 0 0 0))
  (junction (at 199.39 39.37) (diameter 0) (color 0 0 0 0))
  (junction (at 234.95 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 148.59 19.05) (diameter 0) (color 0 0 0 0))
  (junction (at 223.52 127) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 116.84) (diameter 0) (color 0 0 0 0))
  (junction (at 100.33 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 147.32 127) (diameter 0) (color 0 0 0 0))
  (junction (at 199.39 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 320.04 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 325.12 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 340.36 53.34) (diameter 0) (color 0 0 0 0))
  (junction (at 80.01 119.38) (diameter 0) (color 0 0 0 0))
  (junction (at 213.36 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 222.25 20.32) (diameter 0) (color 0 0 0 0))
  (junction (at 243.84 167.64) (diameter 0) (color 0 0 0 0))
  (junction (at 107.95 116.84) (diameter 0) (color 0 0 0 0))
  (junction (at 237.49 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 76.2 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 201.93 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 241.3 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 273.05 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 19.05) (diameter 0) (color 0 0 0 0))
  (junction (at 148.59 34.29) (diameter 0) (color 0 0 0 0))
  (junction (at 196.85 34.29) (diameter 0) (color 0 0 0 0))
  (junction (at 78.74 116.84) (diameter 0) (color 0 0 0 0))
  (junction (at 256.54 33.02) (diameter 0) (color 0 0 0 0))
  (junction (at 205.74 69.85) (diameter 0) (color 0 0 0 0))
  (junction (at 220.98 53.34) (diameter 0) (color 0 0 0 0))
  (junction (at 132.08 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 87.63 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 233.68 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 175.26) (diameter 0) (color 0 0 0 0))
  (junction (at 76.2 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 114.3) (diameter 0) (color 0 0 0 0))
  (junction (at 234.95 22.86) (diameter 0) (color 0 0 0 0))
  (junction (at 320.04 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 344.17 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 162.56) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 69.85) (diameter 0) (color 0 0 0 0))
  (junction (at 293.37 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 238.76 127) (diameter 0) (color 0 0 0 0))
  (junction (at 218.44 22.86) (diameter 0) (color 0 0 0 0))
  (junction (at 148.59 26.67) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 298.45 30.48) (diameter 0) (color 0 0 0 0))
  (junction (at 220.98 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 332.74 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 100.33 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 160.02 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 200.66 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 165.1 162.56) (diameter 0) (color 0 0 0 0))
  (junction (at 287.02 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 19.05) (diameter 0) (color 0 0 0 0))
  (junction (at 190.5 92.71) (diameter 0) (color 0 0 0 0))
  (no_connect (at 234.95 27.94))
  (no_connect (at 274.32 25.4))
  (no_connect (at 337.82 55.88))
  (no_connect (at 68.58 129.54))
  (no_connect (at 251.46 134.62))
  (no_connect (at 251.46 132.08))
  (no_connect (at 251.46 154.94))
  (no_connect (at 287.02 139.7))
  (no_connect (at 287.02 144.78))
  (no_connect (at 287.02 154.94))
  (no_connect (at 287.02 149.86))
  (no_connect (at 287.02 152.4))
  (no_connect (at 287.02 137.16))
  (no_connect (at 287.02 134.62))
  (no_connect (at 287.02 132.08))
  (no_connect (at 287.02 129.54))
  (no_connect (at 287.02 127))
  (no_connect (at 287.02 121.92))
  (no_connect (at 287.02 124.46))
  (no_connect (at 243.84 105.41))
  (wire (pts (xy 147.32 147.32) (xy 147.32 127)))
  (wire (pts (xy 185.42 39.37) (xy 199.39 39.37)))
  (wire (pts (xy 252.73 16.51) (xy 252.73 27.94)))
  (wire (pts (xy 251.46 139.7) (xy 208.28 139.7)))
  (wire (pts (xy 297.18 69.85) (xy 297.18 66.04)))
  (wire (pts (xy 213.36 111.76) (xy 251.46 111.76)))
  (wire (pts (xy 241.3 129.54) (xy 241.3 105.41)))
  (wire (pts (xy 223.52 127) (xy 223.52 185.42)))
  (wire (pts (xy 228.6 190.5) (xy 228.6 121.92)))
  (wire (pts (xy 148.59 26.67) (xy 143.51 26.67)))
  (wire (pts (xy 165.1 185.42) (xy 165.1 162.56)))
  (wire (pts (xy 223.52 50.8) (xy 223.52 127)))
  (wire (pts (xy 240.03 17.78) (xy 240.03 31.75)))
  (wire (pts (xy 325.12 69.85) (xy 317.5 69.85)))
  (wire (pts (xy 251.46 121.92) (xy 233.68 121.92)))
  (wire (pts (xy 181.61 36.83) (xy 201.93 36.83)))
  (wire (pts (xy 129.54 109.22) (xy 123.19 109.22)))
  (wire (pts (xy 293.37 38.1) (xy 298.45 38.1)))
  (wire (pts (xy 218.44 38.1) (xy 220.98 38.1)))
  (wire (pts (xy 135.89 109.22) (xy 135.89 104.14)))
  (wire (pts (xy 160.02 137.16) (xy 160.02 190.5)))
  (wire (pts (xy 287.02 180.34) (xy 298.45 180.34)))
  (wire (pts (xy 251.46 149.86) (xy 198.12 149.86)))
  (wire (pts (xy 203.2 157.48) (xy 203.2 127)))
  (wire (pts (xy 234.95 20.32) (xy 234.95 22.86)))
  (wire (pts (xy 157.48 39.37) (xy 185.42 39.37)))
  (wire (pts (xy 68.58 114.3) (xy 68.58 109.22)))
  (wire (pts (xy 208.28 69.85) (xy 208.28 85.09)))
  (wire (pts (xy 312.42 91.44) (xy 297.18 91.44)))
  (wire (pts (xy 218.44 16.51) (xy 252.73 16.51)))
  (wire (pts (xy 107.95 116.84) (xy 115.57 116.84)))
  (wire (pts (xy 297.18 91.44) (xy 297.18 87.63)))
  (wire (pts (xy 274.32 27.94) (xy 275.59 27.94)))
  (wire (pts (xy 185.42 50.8) (xy 185.42 53.34)))
  (wire (pts (xy 100.33 127) (xy 100.33 101.6)))
  (wire (pts (xy 293.37 20.32) (xy 293.37 30.48)))
  (wire (pts (xy 208.28 109.22) (xy 199.39 109.22)))
  (wire (pts (xy 213.36 44.45) (xy 240.03 44.45)))
  (wire (pts (xy 157.48 137.16) (xy 160.02 137.16)))
  (wire (pts (xy 198.12 20.32) (xy 196.85 20.32)))
  (wire (pts (xy 280.67 22.86) (xy 274.32 22.86)))
  (wire (pts (xy 236.22 170.18) (xy 251.46 170.18)))
  (wire (pts (xy 273.05 78.74) (xy 273.05 83.82)))
  (wire (pts (xy 205.74 77.47) (xy 205.74 81.28)))
  (wire (pts (xy 205.74 81.28) (xy 200.66 81.28)))
  (wire (pts (xy 250.19 25.4) (xy 250.19 44.45)))
  (wire (pts (xy 157.48 149.86) (xy 162.56 149.86)))
  (wire (pts (xy 91.44 137.16) (xy 91.44 124.46)))
  (wire (pts (xy 293.37 30.48) (xy 298.45 30.48)))
  (wire (pts (xy 251.46 172.72) (xy 251.46 173.99)))
  (wire (pts (xy 201.93 78.74) (xy 200.66 78.74)))
  (wire (pts (xy 256.54 38.1) (xy 256.54 33.02)))
  (wire (pts (xy 130.81 137.16) (xy 132.08 137.16)))
  (wire (pts (xy 344.17 76.2) (xy 344.17 77.47)))
  (wire (pts (xy 76.2 121.92) (xy 76.2 129.54)))
  (wire (pts (xy 247.65 25.4) (xy 250.19 25.4)))
  (wire (pts (xy 233.68 121.92) (xy 233.68 105.41)))
  (wire (pts (xy 312.42 30.48) (xy 320.04 30.48)))
  (wire (pts (xy 220.98 20.32) (xy 220.98 35.56)))
  (wire (pts (xy 105.41 119.38) (xy 105.41 139.7)))
  (wire (pts (xy 212.09 25.4) (xy 212.09 34.29)))
  (wire (pts (xy 223.52 185.42) (xy 165.1 185.42)))
  (wire (pts (xy 157.48 175.26) (xy 167.64 175.26)))
  (wire (pts (xy 287.02 172.72) (xy 290.83 172.72)))
  (wire (pts (xy 283.21 35.56) (xy 283.21 30.48)))
  (wire (pts (xy 355.6 96.52) (xy 344.17 96.52)))
  (wire (pts (xy 237.49 30.48) (xy 237.49 25.4)))
  (wire (pts (xy 78.74 109.22) (xy 83.82 109.22)))
  (wire (pts (xy 251.46 124.46) (xy 236.22 124.46)))
  (wire (pts (xy 243.84 162.56) (xy 251.46 162.56)))
  (wire (pts (xy 323.85 55.88) (xy 323.85 68.58)))
  (wire (pts (xy 256.54 33.02) (xy 280.67 33.02)))
  (wire (pts (xy 236.22 173.99) (xy 236.22 175.26)))
  (wire (pts (xy 132.08 101.6) (xy 130.81 101.6)))
  (wire (pts (xy 181.61 19.05) (xy 181.61 36.83)))
  (wire (pts (xy 273.05 83.82) (xy 279.4 83.82)))
  (wire (pts (xy 102.87 124.46) (xy 102.87 104.14)))
  (wire (pts (xy 91.44 116.84) (xy 107.95 116.84)))
  (wire (pts (xy 251.46 129.54) (xy 241.3 129.54)))
  (wire (pts (xy 144.78 124.46) (xy 144.78 144.78)))
  (wire (pts (xy 190.5 100.33) (xy 190.5 92.71)))
  (wire (pts (xy 124.46 139.7) (xy 135.89 139.7)))
  (wire (pts (xy 259.08 20.32) (xy 259.08 35.56)))
  (wire (pts (xy 179.07 55.88) (xy 228.6 55.88)))
  (wire (pts (xy 222.25 20.32) (xy 220.98 20.32)))
  (wire (pts (xy 68.58 144.78) (xy 76.2 144.78)))
  (wire (pts (xy 312.42 63.5) (xy 312.42 69.85)))
  (wire (pts (xy 144.78 124.46) (xy 205.74 124.46)))
  (wire (pts (xy 325.12 38.1) (xy 340.36 38.1)))
  (wire (pts (xy 198.12 20.32) (xy 198.12 16.51)))
  (wire (pts (xy 87.63 127) (xy 87.63 129.54)))
  (wire (pts (xy 160.02 190.5) (xy 228.6 190.5)))
  (wire (pts (xy 203.2 127) (xy 147.32 127)))
  (wire (pts (xy 201.93 25.4) (xy 196.85 25.4)))
  (wire (pts (xy 322.58 53.34) (xy 325.12 53.34)))
  (wire (pts (xy 149.86 182.88) (xy 149.86 175.26)))
  (wire (pts (xy 200.66 85.09) (xy 200.66 92.71)))
  (wire (pts (xy 247.65 31.75) (xy 247.65 30.48)))
  (wire (pts (xy 129.54 121.92) (xy 129.54 109.22)))
  (wire (pts (xy 332.74 76.2) (xy 344.17 76.2)))
  (wire (pts (xy 87.63 137.16) (xy 91.44 137.16)))
  (wire (pts (xy 317.5 78.74) (xy 317.5 76.2)))
  (wire (pts (xy 201.93 36.83) (xy 201.93 25.4)))
  (wire (pts (xy 123.19 139.7) (xy 124.46 139.7)))
  (wire (pts (xy 237.49 25.4) (xy 234.95 25.4)))
  (wire (pts (xy 218.44 22.86) (xy 218.44 16.51)))
  (wire (pts (xy 196.85 50.8) (xy 223.52 50.8)))
  (wire (pts (xy 198.12 162.56) (xy 195.58 162.56)))
  (wire (pts (xy 251.46 142.24) (xy 205.74 142.24)))
  (wire (pts (xy 129.54 121.92) (xy 208.28 121.92)))
  (wire (pts (xy 179.07 34.29) (xy 179.07 55.88)))
  (wire (pts (xy 322.58 55.88) (xy 323.85 55.88)))
  (wire (pts (xy 135.89 104.14) (xy 125.73 104.14)))
  (wire (pts (xy 96.52 106.68) (xy 96.52 93.98)))
  (wire (pts (xy 213.36 36.83) (xy 213.36 44.45)))
  (wire (pts (xy 256.54 33.02) (xy 256.54 22.86)))
  (wire (pts (xy 280.67 33.02) (xy 280.67 22.86)))
  (wire (pts (xy 149.86 58.42) (xy 149.86 69.85)))
  (wire (pts (xy 314.96 71.12) (xy 297.18 71.12)))
  (wire (pts (xy 196.85 40.64) (xy 196.85 34.29)))
  (wire (pts (xy 201.93 36.83) (xy 213.36 36.83)))
  (wire (pts (xy 322.58 58.42) (xy 322.58 63.5)))
  (wire (pts (xy 143.51 19.05) (xy 148.59 19.05)))
  (wire (pts (xy 275.59 27.94) (xy 275.59 66.04)))
  (wire (pts (xy 294.64 78.74) (xy 287.02 78.74)))
  (wire (pts (xy 125.73 104.14) (xy 123.19 104.14)))
  (wire (pts (xy 251.46 119.38) (xy 132.08 119.38)))
  (wire (pts (xy 243.84 162.56) (xy 243.84 167.64)))
  (wire (pts (xy 251.46 127) (xy 238.76 127)))
  (wire (pts (xy 132.08 116.84) (xy 132.08 101.6)))
  (wire (pts (xy 127 111.76) (xy 123.19 111.76)))
  (wire (pts (xy 223.52 50.8) (xy 223.52 35.56)))
  (wire (pts (xy 96.52 93.98) (xy 100.33 93.98)))
  (wire (pts (xy 185.42 39.37) (xy 185.42 40.64)))
  (wire (pts (xy 219.71 129.54) (xy 220.98 129.54)))
  (wire (pts (xy 312.42 86.36) (xy 312.42 85.09)))
  (wire (pts (xy 247.65 20.32) (xy 259.08 20.32)))
  (wire (pts (xy 251.46 157.48) (xy 203.2 157.48)))
  (wire (pts (xy 226.06 187.96) (xy 162.56 187.96)))
  (wire (pts (xy 322.58 63.5) (xy 312.42 63.5)))
  (wire (pts (xy 273.05 66.04) (xy 273.05 71.12)))
  (wire (pts (xy 323.85 68.58) (xy 314.96 68.58)))
  (wire (pts (xy 199.39 27.94) (xy 196.85 27.94)))
  (wire (pts (xy 355.6 58.42) (xy 355.6 96.52)))
  (wire (pts (xy 208.28 107.95) (xy 208.28 109.22)))
  (wire (pts (xy 80.01 119.38) (xy 105.41 119.38)))
  (wire (pts (xy 198.12 16.51) (xy 162.56 16.51)))
  (wire (pts (xy 162.56 34.29) (xy 148.59 34.29)))
  (wire (pts (xy 223.52 35.56) (xy 220.98 35.56)))
  (wire (pts (xy 210.82 46.99) (xy 226.06 46.99)))
  (wire (pts (xy 132.08 132.08) (xy 132.08 137.16)))
  (wire (pts (xy 256.54 22.86) (xy 247.65 22.86)))
  (wire (pts (xy 165.1 34.29) (xy 179.07 34.29)))
  (wire (pts (xy 218.44 22.86) (xy 222.25 22.86)))
  (wire (pts (xy 68.58 109.22) (xy 78.74 109.22)))
  (wire (pts (xy 218.44 38.1) (xy 218.44 22.86)))
  (wire (pts (xy 105.41 139.7) (xy 107.95 139.7)))
  (wire (pts (xy 228.6 121.92) (xy 233.68 121.92)))
  (wire (pts (xy 251.46 152.4) (xy 200.66 152.4)))
  (wire (pts (xy 177.8 62.23) (xy 177.8 60.96)))
  (wire (pts (xy 353.06 58.42) (xy 355.6 58.42)))
  (wire (pts (xy 312.42 86.36) (xy 312.42 91.44)))
  (wire (pts (xy 165.1 19.05) (xy 181.61 19.05)))
  (wire (pts (xy 287.02 167.64) (xy 298.45 167.64)))
  (wire (pts (xy 219.71 124.46) (xy 226.06 124.46)))
  (wire (pts (xy 228.6 55.88) (xy 228.6 121.92)))
  (wire (pts (xy 195.58 144.78) (xy 195.58 137.16)))
  (wire (pts (xy 111.76 132.08) (xy 115.57 132.08)))
  (wire (pts (xy 149.86 58.42) (xy 208.28 58.42)))
  (wire (pts (xy 167.64 137.16) (xy 160.02 137.16)))
  (wire (pts (xy 259.08 35.56) (xy 283.21 35.56)))
  (wire (pts (xy 297.18 60.96) (xy 294.64 60.96)))
  (wire (pts (xy 198.12 149.86) (xy 198.12 162.56)))
  (wire (pts (xy 157.48 26.67) (xy 157.48 39.37)))
  (wire (pts (xy 275.59 66.04) (xy 273.05 66.04)))
  (wire (pts (xy 111.76 96.52) (xy 115.57 96.52)))
  (wire (pts (xy 149.86 149.86) (xy 149.86 162.56)))
  (wire (pts (xy 325.12 53.34) (xy 325.12 69.85)))
  (wire (pts (xy 208.28 68.58) (xy 208.28 69.85)))
  (wire (pts (xy 76.2 144.78) (xy 87.63 144.78)))
  (wire (pts (xy 157.48 162.56) (xy 165.1 162.56)))
  (wire (pts (xy 236.22 124.46) (xy 236.22 105.41)))
  (wire (pts (xy 340.36 38.1) (xy 340.36 53.34)))
  (wire (pts (xy 237.49 33.02) (xy 237.49 30.48)))
  (wire (pts (xy 298.45 38.1) (xy 320.04 38.1)))
  (wire (pts (xy 154.94 50.8) (xy 149.86 50.8)))
  (wire (pts (xy 212.09 25.4) (xy 222.25 25.4)))
  (wire (pts (xy 147.32 127) (xy 127 127)))
  (wire (pts (xy 320.04 86.36) (xy 320.04 82.55)))
  (wire (pts (xy 222.25 17.78) (xy 240.03 17.78)))
  (wire (pts (xy 167.64 182.88) (xy 167.64 175.26)))
  (wire (pts (xy 68.58 114.3) (xy 71.12 114.3)))
  (wire (pts (xy 223.52 127) (xy 238.76 127)))
  (wire (pts (xy 280.67 78.74) (xy 287.02 78.74)))
  (wire (pts (xy 179.07 34.29) (xy 196.85 34.29)))
  (wire (pts (xy 107.95 121.92) (xy 107.95 137.16)))
  (wire (pts (xy 210.82 46.99) (xy 210.82 39.37)))
  (wire (pts (xy 200.66 152.4) (xy 200.66 175.26)))
  (wire (pts (xy 96.52 114.3) (xy 96.52 121.92)))
  (wire (pts (xy 317.5 69.85) (xy 317.5 76.2)))
  (wire (pts (xy 344.17 96.52) (xy 344.17 87.63)))
  (wire (pts (xy 132.08 132.08) (xy 135.89 132.08)))
  (wire (pts (xy 195.58 147.32) (xy 195.58 149.86)))
  (wire (pts (xy 313.69 76.2) (xy 317.5 76.2)))
  (wire (pts (xy 234.95 30.48) (xy 237.49 30.48)))
  (wire (pts (xy 252.73 27.94) (xy 247.65 27.94)))
  (wire (pts (xy 269.24 180.34) (xy 287.02 180.34)))
  (wire (pts (xy 100.33 101.6) (xy 107.95 101.6)))
  (wire (pts (xy 226.06 124.46) (xy 236.22 124.46)))
  (wire (pts (xy 251.46 147.32) (xy 195.58 147.32)))
  (wire (pts (xy 236.22 170.18) (xy 236.22 173.99)))
  (wire (pts (xy 237.49 33.02) (xy 256.54 33.02)))
  (wire (pts (xy 317.5 78.74) (xy 327.66 78.74)))
  (wire (pts (xy 314.96 68.58) (xy 314.96 71.12)))
  (wire (pts (xy 68.58 116.84) (xy 78.74 116.84)))
  (wire (pts (xy 190.5 109.22) (xy 199.39 109.22)))
  (wire (pts (xy 148.59 19.05) (xy 162.56 19.05)))
  (wire (pts (xy 222.25 20.32) (xy 222.25 17.78)))
  (wire (pts (xy 251.46 116.84) (xy 135.89 116.84)))
  (wire (pts (xy 190.5 107.95) (xy 190.5 109.22)))
  (wire (pts (xy 293.37 38.1) (xy 256.54 38.1)))
  (wire (pts (xy 68.58 132.08) (xy 68.58 144.78)))
  (wire (pts (xy 199.39 39.37) (xy 210.82 39.37)))
  (wire (pts (xy 212.09 34.29) (xy 208.28 34.29)))
  (wire (pts (xy 76.2 137.16) (xy 80.01 137.16)))
  (wire (pts (xy 149.86 162.56) (xy 149.86 175.26)))
  (wire (pts (xy 208.28 92.71) (xy 208.28 100.33)))
  (wire (pts (xy 243.84 167.64) (xy 243.84 173.99)))
  (wire (pts (xy 107.95 152.4) (xy 115.57 152.4)))
  (wire (pts (xy 205.74 69.85) (xy 208.28 69.85)))
  (wire (pts (xy 220.98 129.54) (xy 241.3 129.54)))
  (wire (pts (xy 298.45 30.48) (xy 304.8 30.48)))
  (wire (pts (xy 337.82 58.42) (xy 345.44 58.42)))
  (wire (pts (xy 135.89 116.84) (xy 132.08 116.84)))
  (wire (pts (xy 80.01 137.16) (xy 80.01 119.38)))
  (wire (pts (xy 220.98 129.54) (xy 220.98 182.88)))
  (wire (pts (xy 340.36 53.34) (xy 337.82 53.34)))
  (wire (pts (xy 87.63 127) (xy 100.33 127)))
  (wire (pts (xy 154.94 60.96) (xy 154.94 50.8)))
  (wire (pts (xy 208.28 34.29) (xy 208.28 58.42)))
  (wire (pts (xy 238.76 127) (xy 238.76 105.41)))
  (wire (pts (xy 68.58 119.38) (xy 80.01 119.38)))
  (wire (pts (xy 96.52 121.92) (xy 107.95 121.92)))
  (wire (pts (xy 320.04 30.48) (xy 325.12 30.48)))
  (wire (pts (xy 78.74 116.84) (xy 83.82 116.84)))
  (wire (pts (xy 162.56 16.51) (xy 162.56 19.05)))
  (wire (pts (xy 220.98 53.34) (xy 220.98 129.54)))
  (wire (pts (xy 274.32 20.32) (xy 283.21 20.32)))
  (wire (pts (xy 149.86 137.16) (xy 149.86 149.86)))
  (wire (pts (xy 294.64 60.96) (xy 294.64 78.74)))
  (wire (pts (xy 68.58 124.46) (xy 91.44 124.46)))
  (wire (pts (xy 320.04 38.1) (xy 325.12 38.1)))
  (wire (pts (xy 68.58 127) (xy 87.63 127)))
  (wire (pts (xy 123.19 147.32) (xy 147.32 147.32)))
  (wire (pts (xy 320.04 82.55) (xy 336.55 82.55)))
  (wire (pts (xy 240.03 31.75) (xy 247.65 31.75)))
  (wire (pts (xy 127 127) (xy 127 111.76)))
  (wire (pts (xy 132.08 119.38) (xy 132.08 132.08)))
  (wire (pts (xy 297.18 71.12) (xy 297.18 82.55)))
  (wire (pts (xy 144.78 144.78) (xy 123.19 144.78)))
  (wire (pts (xy 312.42 69.85) (xy 297.18 69.85)))
  (wire (pts (xy 196.85 34.29) (xy 196.85 30.48)))
  (wire (pts (xy 327.66 86.36) (xy 327.66 78.74)))
  (wire (pts (xy 208.28 85.09) (xy 208.28 92.71)))
  (wire (pts (xy 220.98 182.88) (xy 167.64 182.88)))
  (wire (pts (xy 162.56 149.86) (xy 162.56 187.96)))
  (wire (pts (xy 162.56 149.86) (xy 167.64 149.86)))
  (wire (pts (xy 185.42 53.34) (xy 220.98 53.34)))
  (wire (pts (xy 226.06 46.99) (xy 226.06 124.46)))
  (wire (pts (xy 213.36 44.45) (xy 213.36 111.76)))
  (wire (pts (xy 220.98 38.1) (xy 220.98 53.34)))
  (wire (pts (xy 219.71 121.92) (xy 228.6 121.92)))
  (wire (pts (xy 177.8 60.96) (xy 154.94 60.96)))
  (wire (pts (xy 208.28 139.7) (xy 208.28 121.92)))
  (wire (pts (xy 148.59 34.29) (xy 148.59 26.67)))
  (wire (pts (xy 76.2 121.92) (xy 96.52 121.92)))
  (wire (pts (xy 200.66 175.26) (xy 195.58 175.26)))
  (wire (pts (xy 190.5 92.71) (xy 200.66 92.71)))
  (wire (pts (xy 234.95 22.86) (xy 234.95 25.4)))
  (wire (pts (xy 327.66 96.52) (xy 344.17 96.52)))
  (wire (pts (xy 251.46 144.78) (xy 195.58 144.78)))
  (wire (pts (xy 205.74 142.24) (xy 205.74 124.46)))
  (wire (pts (xy 219.71 127) (xy 223.52 127)))
  (wire (pts (xy 298.45 167.64) (xy 298.45 172.72)))
  (wire (pts (xy 199.39 22.86) (xy 196.85 22.86)))
  (wire (pts (xy 102.87 104.14) (xy 107.95 104.14)))
  (wire (pts (xy 226.06 124.46) (xy 226.06 187.96)))
  (wire (pts (xy 199.39 39.37) (xy 199.39 27.94)))
  (wire (pts (xy 68.58 121.92) (xy 76.2 121.92)))
  (wire (pts (xy 165.1 162.56) (xy 167.64 162.56)))
  (wire (pts (xy 91.44 124.46) (xy 102.87 124.46)))
  (text "Reset" (at 167.64 16.51 0))
  (text "Clock" (at 167.64 34.29 0))
  (text "Data" (at 167.64 39.37 0))
  (text "[" (at 314.96 58.42 0))
  (symbol (lib_id "Device:R") (at 240.03 173.99 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R19" (id 0) (at 240.03 171.45 90))
    (property "Value" "4.7k" (id 1) (at 240.03 173.99 90))
    (property "Footprint" "" (id 2) (at 240.03 172.212 90))
    (property "Datasheet" "~" (id 3) (at 240.03 173.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx_IEEE:7406") (at 181.61 175.26 180) (unit 6)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 181.61 171.45 0))
    (property "Value" "7406" (id 1) (at 181.61 173.99 0))
    (property "Footprint" "" (id 2) (at 181.61 175.26 0))
    (property "Datasheet" "" (id 3) (at 181.61 175.26 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "Device:R") (at 280.67 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R4" (id 0) (at 283.21 73.6599 0))
    (property "Value" "10k" (id 1) (at 283.21 76.1999 0))
    (property "Footprint" "" (id 2) (at 278.892 74.93 90))
    (property "Datasheet" "~" (id 3) (at 280.67 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 287.02 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 287.02 123.19 0))
    (property "Value" "GND" (id 1) (at 289.56 116.84 0))
    (property "Footprint" "" (id 2) (at 287.02 116.84 0))
    (property "Datasheet" "" (id 3) (at 287.02 116.84 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 100.33 97.79 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R15" (id 0) (at 102.87 97.79 90))
    (property "Value" "1k" (id 1) (at 100.33 97.79 90))
    (property "Footprint" "" (id 2) (at 102.108 97.79 90))
    (property "Datasheet" "~" (id 3) (at 100.33 97.79 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:Conn_01x05_Male") (at 242.57 25.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J51" (id 0) (at 245.11 15.24 0))
    (property "Value" "Kbd_Hdr" (id 1) (at 245.11 17.78 0))
    (property "Footprint" "" (id 2) (at 242.57 25.4 0))
    (property "Datasheet" "~" (id 3) (at 242.57 25.4 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:Conn_01x04_Male") (at 269.24 22.86 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J54" (id 0) (at 269.875 15.24 0))
    (property "Value" "+5V & Spk" (id 1) (at 269.875 17.78 0))
    (property "Footprint" "" (id 2) (at 269.24 22.86 0))
    (property "Datasheet" "~" (id 3) (at 269.24 22.86 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "power:GND") (at 71.12 114.3 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 71.12 120.65 0))
    (property "Value" "GND" (id 1) (at 71.12 113.03 0))
    (property "Footprint" "" (id 2) (at 71.12 114.3 0))
    (property "Datasheet" "" (id 3) (at 71.12 114.3 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 269.24 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 269.24 107.95 0))
    (property "Value" "+5V" (id 1) (at 269.24 99.06 0))
    (property "Footprint" "" (id 2) (at 269.24 104.14 0))
    (property "Datasheet" "" (id 3) (at 269.24 104.14 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 153.67 162.56 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C15" (id 0) (at 154.94 165.1 0))
    (property "Value" "33pF" (id 1) (at 152.4 165.1 0))
    (property "Footprint" "" (id 2) (at 149.86 163.5252 0))
    (property "Datasheet" "~" (id 3) (at 153.67 162.56 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "MCU_Intel:8749") (at 269.24 142.24 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U3" (id 0) (at 271.2594 102.87 0))
    (property "Value" "8749" (id 1) (at 271.2594 105.41 0))
    (property "Footprint" "" (id 2) (at 269.24 137.16 0))
    (property "Datasheet" "" (id 3) (at 269.24 137.16 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 208.28 104.14 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C18" (id 0) (at 213.36 102.87 0))
    (property "Value" "6V 27" (id 1) (at 210.82 105.41 0))
    (property "Footprint" "" (id 2) (at 208.28 104.14 0))
    (property "Datasheet" "~" (id 3) (at 208.28 104.14 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 332.74 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 332.74 80.01 0))
    (property "Value" "+5V" (id 1) (at 332.74 71.12 0))
    (property "Footprint" "" (id 2) (at 332.74 76.2 0))
    (property "Datasheet" "" (id 3) (at 332.74 76.2 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 190.5 104.14 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C19" (id 0) (at 182.88 102.87 0))
    (property "Value" ".1" (id 1) (at 182.88 105.41 0))
    (property "Footprint" "" (id 2) (at 191.4652 107.95 0))
    (property "Datasheet" "~" (id 3) (at 190.5 104.14 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Jumper:Jumper_2_Bridged") (at 288.29 20.32 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "JB1_B" (id 0) (at 288.29 13.97 0))
    (property "Value" "B" (id 1) (at 288.29 16.51 0))
    (property "Footprint" "" (id 2) (at 288.29 20.32 0))
    (property "Datasheet" "~" (id 3) (at 288.29 20.32 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 219.71 121.92 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP1" (id 0) (at 210.82 121.92 90))
    (property "Value" "1" (id 1) (at 214.63 121.92 90))
    (property "Footprint" "" (id 2) (at 219.71 116.84 0))
    (property "Datasheet" "~" (id 3) (at 219.71 116.84 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:Conn_01x03_Male") (at 332.74 55.88 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J56" (id 0) (at 333.375 48.26 0))
    (property "Value" "Speaker" (id 1) (at 333.375 50.8 0))
    (property "Footprint" "" (id 2) (at 332.74 55.88 0))
    (property "Datasheet" "~" (id 3) (at 332.74 55.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Connector:TestPoint") (at 219.71 127 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP3" (id 0) (at 210.82 127 90))
    (property "Value" "3" (id 1) (at 214.63 127 90))
    (property "Footprint" "" (id 2) (at 219.71 121.92 0))
    (property "Datasheet" "~" (id 3) (at 219.71 121.92 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 111.76 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 111.76 102.87 0))
    (property "Value" "GND" (id 1) (at 111.76 95.25 0))
    (property "Footprint" "" (id 2) (at 111.76 96.52 0))
    (property "Datasheet" "" (id 3) (at 111.76 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 127 101.6 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 127 99.06 90))
    (property "Value" "1k" (id 1) (at 127 101.6 90))
    (property "Footprint" "" (id 2) (at 127 99.822 90))
    (property "Datasheet" "~" (id 3) (at 127 101.6 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Opamp_Dual") (at 325.12 78.74 270) (unit 3)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U5" (id 0) (at 325.12 71.12 90))
    (property "Value" "Opamp_Dual" (id 1) (at 325.12 73.66 90))
    (property "Footprint" "" (id 2) (at 325.12 78.74 0))
    (property "Datasheet" "~" (id 3) (at 325.12 78.74 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "4")
    (pin "8")
  )
  (symbol (lib_id "power:GND") (at 199.39 22.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 199.39 29.21 0))
    (property "Value" "GND" (id 1) (at 201.93 22.86 0))
    (property "Footprint" "" (id 2) (at 199.39 22.86 0))
    (property "Datasheet" "" (id 3) (at 199.39 22.86 0))
    (pin "1")
  )
  (symbol (lib_id "74xx_IEEE:7406") (at 191.77 69.85 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 191.77 66.04 0))
    (property "Value" "7406" (id 1) (at 191.77 68.58 0))
    (property "Footprint" "" (id 2) (at 191.77 69.85 0))
    (property "Datasheet" "" (id 3) (at 191.77 69.85 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "power:+5V") (at 107.95 116.84 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 107.95 120.65 0))
    (property "Value" "+5V" (id 1) (at 107.95 111.76 0))
    (property "Footprint" "" (id 2) (at 107.95 116.84 0))
    (property "Datasheet" "" (id 3) (at 107.95 116.84 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 316.23 86.36 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 316.23 83.82 90))
    (property "Value" "47" (id 1) (at 316.23 86.36 90))
    (property "Footprint" "" (id 2) (at 316.23 84.582 90))
    (property "Datasheet" "~" (id 3) (at 316.23 86.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 287.02 160.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 287.02 163.83 0))
    (property "Value" "+5V" (id 1) (at 289.56 160.02 0))
    (property "Footprint" "" (id 2) (at 287.02 160.02 0))
    (property "Datasheet" "" (id 3) (at 287.02 160.02 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:Conn_01x05_Male") (at 191.77 25.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J58" (id 0) (at 192.405 15.24 0))
    (property "Value" "Keyboard" (id 1) (at 193.04 17.78 0))
    (property "Footprint" "" (id 2) (at 191.77 25.4 0))
    (property "Datasheet" "~" (id 3) (at 191.77 25.4 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 269.24 180.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 269.24 186.69 0))
    (property "Value" "GND" (id 1) (at 269.24 185.42 0))
    (property "Footprint" "" (id 2) (at 269.24 180.34 0))
    (property "Datasheet" "" (id 3) (at 269.24 180.34 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 204.47 92.71 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 204.47 90.17 90))
    (property "Value" "10k" (id 1) (at 204.47 92.71 90))
    (property "Footprint" "" (id 2) (at 204.47 90.932 90))
    (property "Datasheet" "~" (id 3) (at 204.47 92.71 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Jumper:Jumper_2_Open") (at 208.28 63.5 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JB1_I" (id 0) (at 200.66 62.23 90))
    (property "Value" "I" (id 1) (at 205.74 64.77 90))
    (property "Footprint" "" (id 2) (at 208.28 63.5 0))
    (property "Datasheet" "~" (id 3) (at 208.28 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 273.05 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R3" (id 0) (at 275.59 73.6599 0))
    (property "Value" "1k" (id 1) (at 275.59 76.1999 0))
    (property "Footprint" "" (id 2) (at 271.272 74.93 90))
    (property "Datasheet" "~" (id 3) (at 273.05 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 153.67 137.16 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C17" (id 0) (at 154.94 139.7 0))
    (property "Value" "33pF" (id 1) (at 152.4 139.7 0))
    (property "Footprint" "" (id 2) (at 149.86 138.1252 0))
    (property "Datasheet" "~" (id 3) (at 153.67 137.16 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 219.71 124.46 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP2" (id 0) (at 210.82 124.46 90))
    (property "Value" "2" (id 1) (at 214.63 124.46 90))
    (property "Footprint" "" (id 2) (at 219.71 119.38 0))
    (property "Datasheet" "~" (id 3) (at 219.71 119.38 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 247.65 173.99 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R10" (id 0) (at 247.65 171.45 90))
    (property "Value" "4.7k" (id 1) (at 247.65 173.99 90))
    (property "Footprint" "" (id 2) (at 247.65 172.212 90))
    (property "Datasheet" "~" (id 3) (at 247.65 173.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 340.36 53.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 340.36 59.69 0))
    (property "Value" "GND" (id 1) (at 342.9 53.34 0))
    (property "Footprint" "" (id 2) (at 340.36 53.34 0))
    (property "Datasheet" "" (id 3) (at 340.36 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 293.37 34.29 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C11" (id 0) (at 285.75 33.02 0))
    (property "Value" ".1" (id 1) (at 285.75 35.56 0))
    (property "Footprint" "" (id 2) (at 294.3352 38.1 0))
    (property "Datasheet" "~" (id 3) (at 293.37 34.29 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 87.63 133.35 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R12" (id 0) (at 90.17 133.35 90))
    (property "Value" "470" (id 1) (at 87.63 133.35 90))
    (property "Footprint" "" (id 2) (at 89.408 133.35 90))
    (property "Datasheet" "~" (id 3) (at 87.63 133.35 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 76.2 140.97 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R17" (id 0) (at 78.74 140.97 90))
    (property "Value" "1k" (id 1) (at 76.2 140.97 90))
    (property "Footprint" "" (id 2) (at 77.978 140.97 90))
    (property "Datasheet" "~" (id 3) (at 76.2 140.97 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 68.58 144.78 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 68.58 151.13 0))
    (property "Value" "GND" (id 1) (at 68.58 148.59 0))
    (property "Footprint" "" (id 2) (at 68.58 144.78 0))
    (property "Datasheet" "" (id 3) (at 68.58 144.78 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 135.89 135.89 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 138.43 134.62 0))
    (property "Value" "33pF" (id 1) (at 138.43 137.16 0))
    (property "Footprint" "" (id 2) (at 136.8552 139.7 0))
    (property "Datasheet" "~" (id 3) (at 135.89 135.89 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Interface_UART:SN75176AP") (at 115.57 142.24 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U2" (id 0) (at 116.0906 129.54 0))
    (property "Value" "SN75176AP" (id 1) (at 116.0906 132.08 0))
    (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (id 2) (at 115.57 129.54 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75176a.pdf" (id 3) (at 74.93 137.16 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:R") (at 205.74 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R18" (id 0) (at 203.2 73.66 90))
    (property "Value" "100" (id 1) (at 205.74 73.66 90))
    (property "Footprint" "" (id 2) (at 203.962 73.66 90))
    (property "Datasheet" "~" (id 3) (at 205.74 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 148.59 34.29 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 148.59 40.64 0))
    (property "Value" "GND" (id 1) (at 148.59 38.1 0))
    (property "Footprint" "" (id 2) (at 148.59 34.29 0))
    (property "Datasheet" "" (id 3) (at 148.59 34.29 0))
    (pin "1")
  )
  (symbol (lib_id "Power_Supervisor:MC34064P") (at 199.39 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U?" (id 0) (at 199.39 93.98 0))
    (property "Value" "MC34064P" (id 1) (at 199.39 96.52 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline" (id 2) (at 199.39 114.3 0))
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34064-D.PDF" (id 3) (at 199.39 101.6 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:L") (at 308.61 30.48 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L2" (id 0) (at 308.61 24.13 90))
    (property "Value" "L" (id 1) (at 308.61 26.67 90))
    (property "Footprint" "" (id 2) (at 308.61 30.48 0))
    (property "Datasheet" "~" (id 3) (at 308.61 30.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 143.51 22.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C9" (id 0) (at 135.89 21.59 0))
    (property "Value" ".1" (id 1) (at 135.89 24.13 0))
    (property "Footprint" "" (id 2) (at 144.4752 26.67 0))
    (property "Datasheet" "~" (id 3) (at 143.51 22.86 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 87.63 140.97 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R14" (id 0) (at 90.17 140.97 90))
    (property "Value" "1k" (id 1) (at 87.63 140.97 90))
    (property "Footprint" "" (id 2) (at 89.408 140.97 90))
    (property "Datasheet" "~" (id 3) (at 87.63 140.97 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 320.04 34.29 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C13" (id 0) (at 312.42 33.02 0))
    (property "Value" ".1" (id 1) (at 312.42 35.56 0))
    (property "Footprint" "" (id 2) (at 321.0052 38.1 0))
    (property "Datasheet" "~" (id 3) (at 320.04 34.29 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 149.86 182.88 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 149.86 189.23 0))
    (property "Value" "GND" (id 1) (at 149.86 187.96 0))
    (property "Footprint" "" (id 2) (at 149.86 182.88 0))
    (property "Datasheet" "" (id 3) (at 149.86 182.88 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Network05") (at 238.76 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "RP1" (id 0) (at 246.38 99.3139 0))
    (property "Value" "4.7k" (id 1) (at 246.38 101.8539 0))
    (property "Footprint" "Resistor_THT:R_Array_SIP6" (id 2) (at 248.285 100.33 90))
    (property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf" (id 3) (at 238.76 100.33 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "Diode:1N4004") (at 204.47 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "CR1" (id 0) (at 204.47 82.55 0))
    (property "Value" "1N4004" (id 1) (at 204.47 87.63 0))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 204.47 89.535 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 204.47 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 149.86 50.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 149.86 54.61 0))
    (property "Value" "+5V" (id 1) (at 149.86 46.99 0))
    (property "Footprint" "" (id 2) (at 149.86 50.8 0))
    (property "Datasheet" "" (id 3) (at 149.86 50.8 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:DIN-5_180degree") (at 165.1 26.67 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J50" (id 0) (at 171.45 25.3998 90))
    (property "Value" "Keyboard" (id 1) (at 171.45 27.9398 90))
    (property "Footprint" "" (id 2) (at 165.1 26.67 0))
    (property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf" (id 3) (at 165.1 26.67 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:Opamp_Dual") (at 304.8 63.5 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U5" (id 0) (at 304.8 53.34 0))
    (property "Value" "Opamp_Dual" (id 1) (at 304.8 55.88 0))
    (property "Footprint" "" (id 2) (at 304.8 63.5 0))
    (property "Datasheet" "~" (id 3) (at 304.8 63.5 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "4")
    (pin "8")
  )
  (symbol (lib_id "Device:C") (at 153.67 149.86 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C16" (id 0) (at 154.94 152.4 0))
    (property "Value" "33pF" (id 1) (at 152.4 152.4 0))
    (property "Footprint" "" (id 2) (at 149.86 150.8252 0))
    (property "Datasheet" "~" (id 3) (at 153.67 149.86 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Jumper:Jumper_2_Open") (at 288.29 30.48 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "JB1_A" (id 0) (at 288.29 24.13 0))
    (property "Value" "A" (id 1) (at 288.29 26.67 0))
    (property "Footprint" "" (id 2) (at 288.29 30.48 0))
    (property "Datasheet" "~" (id 3) (at 288.29 30.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 125.73 104.14 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 125.73 110.49 0))
    (property "Value" "GND" (id 1) (at 128.27 106.68 0))
    (property "Footprint" "" (id 2) (at 125.73 104.14 0))
    (property "Datasheet" "" (id 3) (at 125.73 104.14 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 127 137.16 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 127 134.62 90))
    (property "Value" "1k" (id 1) (at 127 137.16 90))
    (property "Footprint" "" (id 2) (at 127 135.382 90))
    (property "Datasheet" "~" (id 3) (at 127 137.16 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 298.45 34.29 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C10" (id 0) (at 302.26 32.3849 0))
    (property "Value" "20V 10" (id 1) (at 302.26 34.9249 0))
    (property "Footprint" "" (id 2) (at 298.45 34.29 0))
    (property "Datasheet" "~" (id 3) (at 298.45 34.29 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:Conn_01x08_Male") (at 63.5 121.92 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J53" (id 0) (at 64.135 109.22 0))
    (property "Value" "Remote" (id 1) (at 64.135 111.76 0))
    (property "Footprint" "" (id 2) (at 63.5 121.92 0))
    (property "Datasheet" "~" (id 3) (at 63.5 121.92 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Jumper:Jumper_2_Open") (at 185.42 45.72 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "JB1_H" (id 0) (at 187.96 44.4499 90))
    (property "Value" "H" (id 1) (at 187.96 46.9899 90))
    (property "Footprint" "" (id 2) (at 185.42 45.72 0))
    (property "Datasheet" "~" (id 3) (at 185.42 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 316.23 91.44 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 316.23 88.9 90))
    (property "Value" "47" (id 1) (at 316.23 91.44 90))
    (property "Footprint" "" (id 2) (at 316.23 89.662 90))
    (property "Datasheet" "~" (id 3) (at 316.23 91.44 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 287.02 111.76 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 287.02 115.57 0))
    (property "Value" "+5V" (id 1) (at 289.56 111.76 0))
    (property "Footprint" "" (id 2) (at 287.02 111.76 0))
    (property "Datasheet" "" (id 3) (at 287.02 111.76 0))
    (pin "1")
  )
  (symbol (lib_id "74xx_IEEE:7406") (at 181.61 137.16 180) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 181.61 133.35 0))
    (property "Value" "7406" (id 1) (at 181.61 135.89 0))
    (property "Footprint" "" (id 2) (at 181.61 137.16 0))
    (property "Datasheet" "" (id 3) (at 181.61 137.16 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "Connector:Conn_01x02_Male") (at 195.58 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J57" (id 0) (at 191.77 78.74 0))
    (property "Value" "Reset_Btn" (id 1) (at 189.23 81.28 0))
    (property "Footprint" "" (id 2) (at 195.58 78.74 0))
    (property "Datasheet" "~" (id 3) (at 195.58 78.74 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 298.45 176.53 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 300.99 175.26 0))
    (property "Value" "33pF" (id 1) (at 300.99 177.8 0))
    (property "Footprint" "" (id 2) (at 299.4152 180.34 0))
    (property "Datasheet" "~" (id 3) (at 298.45 176.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Jumper:Jumper_2_Bridged") (at 207.01 25.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JB1_D" (id 0) (at 207.01 27.94 0))
    (property "Value" "D" (id 1) (at 207.01 30.48 0))
    (property "Footprint" "" (id 2) (at 207.01 25.4 0))
    (property "Datasheet" "~" (id 3) (at 207.01 25.4 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 325.12 30.48 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 325.12 34.29 0))
    (property "Value" "+5V" (id 1) (at 325.12 25.4 0))
    (property "Footprint" "" (id 2) (at 325.12 30.48 0))
    (property "Datasheet" "" (id 3) (at 325.12 30.48 0))
    (pin "1")
  )
  (symbol (lib_id "Jumper:Jumper_2_Bridged") (at 236.22 180.34 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "JB1_E" (id 0) (at 237.49 179.0699 90))
    (property "Value" "E" (id 1) (at 237.49 181.6099 90))
    (property "Footprint" "" (id 2) (at 236.22 180.34 0))
    (property "Datasheet" "~" (id 3) (at 236.22 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 243.84 162.56 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 243.84 166.37 0))
    (property "Value" "+5V" (id 1) (at 241.3 162.56 0))
    (property "Footprint" "" (id 2) (at 243.84 162.56 0))
    (property "Datasheet" "" (id 3) (at 243.84 162.56 0))
    (pin "1")
  )
  (symbol (lib_id "Jumper:Jumper_2_Open") (at 245.11 44.45 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "JB1_C" (id 0) (at 245.11 38.1 0))
    (property "Value" "C" (id 1) (at 245.11 40.64 0))
    (property "Footprint" "" (id 2) (at 245.11 44.45 0))
    (property "Datasheet" "~" (id 3) (at 245.11 44.45 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 236.22 185.42 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 236.22 191.77 0))
    (property "Value" "GND" (id 1) (at 236.22 190.5 0))
    (property "Footprint" "" (id 2) (at 236.22 185.42 0))
    (property "Datasheet" "" (id 3) (at 236.22 185.42 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 76.2 133.35 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R13" (id 0) (at 78.74 133.35 90))
    (property "Value" "470" (id 1) (at 76.2 133.35 90))
    (property "Footprint" "" (id 2) (at 77.978 133.35 90))
    (property "Datasheet" "~" (id 3) (at 76.2 133.35 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Q_NPN_EBC") (at 284.48 83.82 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q3" (id 0) (at 289.56 82.5499 0))
    (property "Value" "2N6427" (id 1) (at 289.56 85.0899 0))
    (property "Footprint" "" (id 2) (at 289.56 81.28 0))
    (property "Datasheet" "~" (id 3) (at 284.48 83.82 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:GND") (at 313.69 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 313.69 82.55 0))
    (property "Value" "GND" (id 1) (at 313.69 80.01 0))
    (property "Footprint" "" (id 2) (at 313.69 76.2 0))
    (property "Datasheet" "" (id 3) (at 313.69 76.2 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 100.33 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 100.33 97.79 0))
    (property "Value" "+5V" (id 1) (at 100.33 88.9 0))
    (property "Footprint" "" (id 2) (at 100.33 93.98 0))
    (property "Datasheet" "" (id 3) (at 100.33 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 325.12 34.29 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C12" (id 0) (at 328.93 32.3849 0))
    (property "Value" "20V 10" (id 1) (at 328.93 34.9249 0))
    (property "Footprint" "" (id 2) (at 325.12 34.29 0))
    (property "Datasheet" "~" (id 3) (at 325.12 34.29 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 190.5 92.71 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 190.5 96.52 0))
    (property "Value" "+5V" (id 1) (at 190.5 88.9 0))
    (property "Footprint" "" (id 2) (at 190.5 92.71 0))
    (property "Datasheet" "" (id 3) (at 190.5 92.71 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_PNP_BCE") (at 325.12 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q2" (id 0) (at 330.2 90.1699 0))
    (property "Value" "2N2907" (id 1) (at 330.2 92.7099 0))
    (property "Footprint" "" (id 2) (at 330.2 88.9 0))
    (property "Datasheet" "~" (id 3) (at 325.12 91.44 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "74xx_IEEE:7406") (at 163.83 69.85 180) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 163.83 66.04 0))
    (property "Value" "7406" (id 1) (at 163.83 68.58 0))
    (property "Footprint" "" (id 2) (at 163.83 69.85 0))
    (property "Datasheet" "" (id 3) (at 163.83 69.85 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "Connector:Conn_01x03_Male") (at 317.5 55.88 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J55" (id 0) (at 318.135 48.26 0))
    (property "Value" "Volume" (id 1) (at 318.135 50.8 0))
    (property "Footprint" "" (id 2) (at 317.5 55.88 0))
    (property "Datasheet" "~" (id 3) (at 317.5 55.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 148.59 22.86 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C8" (id 0) (at 152.4 20.9549 0))
    (property "Value" "20V 10" (id 1) (at 152.4 23.4949 0))
    (property "Footprint" "" (id 2) (at 148.59 22.86 0))
    (property "Datasheet" "~" (id 3) (at 148.59 22.86 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 233.68 95.25 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 233.68 99.06 0))
    (property "Value" "+5V" (id 1) (at 233.68 90.17 0))
    (property "Footprint" "" (id 2) (at 233.68 95.25 0))
    (property "Datasheet" "" (id 3) (at 233.68 95.25 0))
    (pin "1")
  )
  (symbol (lib_id "Interface_UART:SN75176AP") (at 115.57 106.68 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 116.0906 93.98 0))
    (property "Value" "SN75176AP" (id 1) (at 116.0906 96.52 0))
    (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (id 2) (at 115.57 93.98 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75176a.pdf" (id 3) (at 74.93 101.6 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Connector:TestPoint") (at 219.71 129.54 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP4" (id 0) (at 210.82 129.54 90))
    (property "Value" "4" (id 1) (at 214.63 129.54 90))
    (property "Footprint" "" (id 2) (at 219.71 124.46 0))
    (property "Datasheet" "~" (id 3) (at 219.71 124.46 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 201.93 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 201.93 85.09 0))
    (property "Value" "GND" (id 1) (at 201.93 77.47 0))
    (property "Footprint" "" (id 2) (at 201.93 78.74 0))
    (property "Datasheet" "" (id 3) (at 201.93 78.74 0))
    (pin "1")
  )
  (symbol (lib_id "74xx_IEEE:7406") (at 181.61 162.56 180) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 181.61 158.75 0))
    (property "Value" "7406" (id 1) (at 181.61 161.29 0))
    (property "Footprint" "" (id 2) (at 181.61 162.56 0))
    (property "Datasheet" "" (id 3) (at 181.61 162.56 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "Device:C") (at 287.02 176.53 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 289.56 175.26 0))
    (property "Value" "33pF" (id 1) (at 289.56 177.8 0))
    (property "Footprint" "" (id 2) (at 287.9852 180.34 0))
    (property "Datasheet" "~" (id 3) (at 287.02 176.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 247.65 167.64 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R20" (id 0) (at 247.65 165.1 90))
    (property "Value" "4.7k" (id 1) (at 247.65 167.64 90))
    (property "Footprint" "" (id 2) (at 247.65 165.862 90))
    (property "Datasheet" "~" (id 3) (at 247.65 167.64 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 276.86 71.12 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R11" (id 0) (at 276.86 68.58 90))
    (property "Value" "10k" (id 1) (at 276.86 71.12 90))
    (property "Footprint" "" (id 2) (at 276.86 69.342 90))
    (property "Datasheet" "~" (id 3) (at 276.86 71.12 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L") (at 87.63 116.84 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L3" (id 0) (at 86.36 118.11 90))
    (property "Value" "L" (id 1) (at 88.9 118.11 90))
    (property "Footprint" "" (id 2) (at 87.63 116.84 0))
    (property "Datasheet" "~" (id 3) (at 87.63 116.84 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Crystal") (at 294.64 172.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "X1" (id 0) (at 294.64 166.37 0))
    (property "Value" "11.3184" (id 1) (at 293.37 168.91 0))
    (property "Footprint" "" (id 2) (at 294.64 172.72 0))
    (property "Datasheet" "~" (id 3) (at 294.64 172.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Q_NPN_EBC") (at 341.63 82.55 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q1" (id 0) (at 346.71 81.2799 0))
    (property "Value" "2N2222" (id 1) (at 346.71 83.8199 0))
    (property "Footprint" "" (id 2) (at 346.71 80.01 0))
    (property "Datasheet" "~" (id 3) (at 341.63 82.55 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R") (at 149.86 54.61 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R9" (id 0) (at 152.4 54.61 90))
    (property "Value" "1k" (id 1) (at 149.86 54.61 90))
    (property "Footprint" "" (id 2) (at 151.638 54.61 90))
    (property "Datasheet" "~" (id 3) (at 149.86 54.61 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx_IEEE:7406") (at 181.61 149.86 180) (unit 5)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 181.61 146.05 0))
    (property "Value" "7406" (id 1) (at 181.61 148.59 0))
    (property "Footprint" "" (id 2) (at 181.61 149.86 0))
    (property "Datasheet" "" (id 3) (at 181.61 149.86 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x05_Odd_Even") (at 227.33 25.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J52" (id 0) (at 228.6 15.24 0))
    (property "Value" "Kbd_Hdr" (id 1) (at 228.6 33.02 0))
    (property "Footprint" "" (id 2) (at 227.33 25.4 0))
    (property "Datasheet" "~" (id 3) (at 227.33 25.4 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:+5V") (at 135.89 19.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 135.89 22.86 0))
    (property "Value" "+5V" (id 1) (at 135.89 15.24 0))
    (property "Footprint" "" (id 2) (at 135.89 19.05 0))
    (property "Datasheet" "" (id 3) (at 135.89 19.05 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 153.67 175.26 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C14" (id 0) (at 154.94 177.8 0))
    (property "Value" "33pF" (id 1) (at 152.4 177.8 0))
    (property "Footprint" "" (id 2) (at 149.86 176.2252 0))
    (property "Datasheet" "~" (id 3) (at 153.67 175.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 96.52 110.49 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R16" (id 0) (at 99.06 110.49 90))
    (property "Value" "1k" (id 1) (at 96.52 110.49 90))
    (property "Footprint" "" (id 2) (at 98.298 110.49 90))
    (property "Datasheet" "~" (id 3) (at 96.52 110.49 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 83.82 113.03 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C1" (id 0) (at 87.63 112.3949 0))
    (property "Value" "20V 10" (id 1) (at 87.63 114.9349 0))
    (property "Footprint" "" (id 2) (at 83.82 113.03 0))
    (property "Datasheet" "~" (id 3) (at 83.82 113.03 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Opamp_Dual") (at 304.8 85.09 0) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U5" (id 0) (at 304.8 74.93 0))
    (property "Value" "Opamp_Dual" (id 1) (at 304.8 77.47 0))
    (property "Footprint" "" (id 2) (at 304.8 85.09 0))
    (property "Datasheet" "~" (id 3) (at 304.8 85.09 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "4")
    (pin "8")
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 349.25 58.42 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C7" (id 0) (at 349.885 50.8 90))
    (property "Value" "35V 100" (id 1) (at 349.885 53.34 90))
    (property "Footprint" "" (id 2) (at 349.25 58.42 0))
    (property "Datasheet" "~" (id 3) (at 349.25 58.42 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 78.74 113.03 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 73.66 111.76 0))
    (property "Value" ".1" (id 1) (at 73.66 114.3 0))
    (property "Footprint" "" (id 2) (at 79.7052 116.84 0))
    (property "Datasheet" "~" (id 3) (at 78.74 113.03 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L") (at 139.7 19.05 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L1" (id 0) (at 139.7 13.97 90))
    (property "Value" "L" (id 1) (at 139.7 16.51 90))
    (property "Footprint" "" (id 2) (at 139.7 19.05 0))
    (property "Datasheet" "~" (id 3) (at 139.7 19.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 107.95 152.4 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 107.95 156.21 0))
    (property "Value" "+5V" (id 1) (at 107.95 147.32 0))
    (property "Footprint" "" (id 2) (at 107.95 152.4 0))
    (property "Datasheet" "" (id 3) (at 107.95 152.4 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 177.8 66.04 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R8" (id 0) (at 175.26 66.04 90))
    (property "Value" "4.7k" (id 1) (at 177.8 66.04 90))
    (property "Footprint" "" (id 2) (at 176.022 66.04 90))
    (property "Datasheet" "~" (id 3) (at 177.8 66.04 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 199.39 109.22 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 199.39 115.57 0))
    (property "Value" "GND" (id 1) (at 199.39 113.03 0))
    (property "Footprint" "" (id 2) (at 199.39 109.22 0))
    (property "Datasheet" "" (id 3) (at 199.39 109.22 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 135.89 113.03 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 138.43 111.76 0))
    (property "Value" "33pF" (id 1) (at 138.43 114.3 0))
    (property "Footprint" "" (id 2) (at 136.8552 116.84 0))
    (property "Datasheet" "~" (id 3) (at 135.89 113.03 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 124.46 139.7 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 124.46 146.05 0))
    (property "Value" "GND" (id 1) (at 127 142.24 0))
    (property "Footprint" "" (id 2) (at 124.46 139.7 0))
    (property "Datasheet" "" (id 3) (at 124.46 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "Jumper:Jumper_2_Open") (at 196.85 45.72 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "JB1_G" (id 0) (at 199.39 44.4499 90))
    (property "Value" "G" (id 1) (at 199.39 46.9899 90))
    (property "Footprint" "" (id 2) (at 196.85 45.72 0))
    (property "Datasheet" "~" (id 3) (at 196.85 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 111.76 132.08 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 111.76 138.43 0))
    (property "Value" "GND" (id 1) (at 111.76 130.81 0))
    (property "Footprint" "" (id 2) (at 111.76 132.08 0))
    (property "Datasheet" "" (id 3) (at 111.76 132.08 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 287.02 88.9 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 287.02 95.25 0))
    (property "Value" "GND" (id 1) (at 287.02 93.98 0))
    (property "Footprint" "" (id 2) (at 287.02 88.9 0))
    (property "Datasheet" "" (id 3) (at 287.02 88.9 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "20V 10") (footprint "")
    )
    (path
      (reference "C2") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C3") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C4") (unit 1) (value ".1") (footprint "")
    )
    (path
      (reference "C5") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C6") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C7") (unit 1) (value "35V 100") (footprint "")
    )
    (path
      (reference "C8") (unit 1) (value "20V 10") (footprint "")
    )
    (path
      (reference "C9") (unit 1) (value ".1") (footprint "")
    )
    (path
      (reference "C10") (unit 1) (value "20V 10") (footprint "")
    )
    (path
      (reference "C11") (unit 1) (value ".1") (footprint "")
    )
    (path
      (reference "C12") (unit 1) (value "20V 10") (footprint "")
    )
    (path
      (reference "C13") (unit 1) (value ".1") (footprint "")
    )
    (path
      (reference "C14") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C15") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C16") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C17") (unit 1) (value "33pF") (footprint "")
    )
    (path
      (reference "C18") (unit 1) (value "6V 27") (footprint "")
    )
    (path
      (reference "C19") (unit 1) (value ".1") (footprint "")
    )
    (path
      (reference "CR1") (unit 1) (value "1N4004") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "J50") (unit 1) (value "Keyboard") (footprint "")
    )
    (path
      (reference "J51") (unit 1) (value "Kbd_Hdr") (footprint "")
    )
    (path
      (reference "J52") (unit 1) (value "Kbd_Hdr") (footprint "")
    )
    (path
      (reference "J53") (unit 1) (value "Remote") (footprint "")
    )
    (path
      (reference "J54") (unit 1) (value "+5V & Spk") (footprint "")
    )
    (path
      (reference "J55") (unit 1) (value "Volume") (footprint "")
    )
    (path
      (reference "J56") (unit 1) (value "Speaker") (footprint "")
    )
    (path
      (reference "J57") (unit 1) (value "Reset_Btn") (footprint "")
    )
    (path
      (reference "J58") (unit 1) (value "Keyboard") (footprint "")
    )
    (path
      (reference "JB1_A") (unit 1) (value "A") (footprint "")
    )
    (path
      (reference "JB1_B") (unit 1) (value "B") (footprint "")
    )
    (path
      (reference "JB1_C") (unit 1) (value "C") (footprint "")
    )
    (path
      (reference "JB1_D") (unit 1) (value "D") (footprint "")
    )
    (path
      (reference "JB1_E") (unit 1) (value "E") (footprint "")
    )
    (path
      (reference "JB1_G") (unit 1) (value "G") (footprint "")
    )
    (path
      (reference "JB1_H") (unit 1) (value "H") (footprint "")
    )
    (path
      (reference "JB1_I") (unit 1) (value "I") (footprint "")
    )
    (path
      (reference "L1") (unit 1) (value "L") (footprint "")
    )
    (path
      (reference "L2") (unit 1) (value "L") (footprint "")
    )
    (path
      (reference "L3") (unit 1) (value "L") (footprint "")
    )
    (path
      (reference "Q1") (unit 1) (value "2N2222") (footprint "")
    )
    (path
      (reference "Q2") (unit 1) (value "2N2907") (footprint "")
    )
    (path
      (reference "Q3") (unit 1) (value "2N6427") (footprint "")
    )
    (path
      (reference "R1") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R2") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R3") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R4") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R5") (unit 1) (value "47") (footprint "")
    )
    (path
      (reference "R6") (unit 1) (value "47") (footprint "")
    )
    (path
      (reference "R7") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R8") (unit 1) (value "4.7k") (footprint "")
    )
    (path
      (reference "R9") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R10") (unit 1) (value "4.7k") (footprint "")
    )
    (path
      (reference "R11") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R12") (unit 1) (value "470") (footprint "")
    )
    (path
      (reference "R13") (unit 1) (value "470") (footprint "")
    )
    (path
      (reference "R14") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R15") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R16") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R17") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R18") (unit 1) (value "100") (footprint "")
    )
    (path
      (reference "R19") (unit 1) (value "4.7k") (footprint "")
    )
    (path
      (reference "R20") (unit 1) (value "4.7k") (footprint "")
    )
    (path
      (reference "RP1") (unit 1) (value "4.7k") (footprint "Resistor_THT:R_Array_SIP6")
    )
    (path
      (reference "TP1") (unit 1) (value "1") (footprint "")
    )
    (path
      (reference "TP2") (unit 1) (value "2") (footprint "")
    )
    (path
      (reference "TP3") (unit 1) (value "3") (footprint "")
    )
    (path
      (reference "TP4") (unit 1) (value "4") (footprint "")
    )
    (path
      (reference "U1") (unit 1) (value "SN75176AP") (footprint "Package_DIP:DIP-8_W7.62mm")
    )
    (path
      (reference "U2") (unit 1) (value "SN75176AP") (footprint "Package_DIP:DIP-8_W7.62mm")
    )
    (path
      (reference "U3") (unit 1) (value "8749") (footprint "")
    )
    (path
      (reference "U4") (unit 1) (value "7406") (footprint "")
    )
    (path
      (reference "U4") (unit 2) (value "7406") (footprint "")
    )
    (path
      (reference "U4") (unit 3) (value "7406") (footprint "")
    )
    (path
      (reference "U4") (unit 4) (value "7406") (footprint "")
    )
    (path
      (reference "U4") (unit 5) (value "7406") (footprint "")
    )
    (path
      (reference "U4") (unit 6) (value "7406") (footprint "")
    )
    (path
      (reference "U5") (unit 1) (value "Opamp_Dual") (footprint "")
    )
    (path
      (reference "U5") (unit 2) (value "Opamp_Dual") (footprint "")
    )
    (path
      (reference "U5") (unit 3) (value "Opamp_Dual") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "MC34064P") (footprint "Package_TO_SOT_THT:TO-92L_Inline")
    )
    (path
      (reference "X1") (unit 1) (value "11.3184") (footprint "")
    )
  )
)
