(kicad_sch (version 20211123) (generator eeschema)
  (paper "A0")
  (lib_symbols
    (symbol "4xxx:4050" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "4050" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "CMOS BUFFER" (id 5) (at 0 0 0))
      (property "ki_description" "Hex Buffer" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP?16*" (id 7) (at 0 0 0))
      (symbol "4050_1_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "4050_2_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
      )
      (symbol "4050_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "7")
        )
      )
      (symbol "4050_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "4050_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
      )
      (symbol "4050_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "14")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "15")
        )
      )
      (symbol "4050_7_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "1")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "VSS")
          (number "8")
        )
      )
      (symbol "4050_7_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74LS14" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "74LS14" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL not inverter" (id 5) (at 0 0 0))
      (property "ki_description" "Hex inverter schmitt trigger" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0))
      (symbol "74LS14_1_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74LS14_1_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_2_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74LS14_2_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS14_3_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS14_4_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74LS14_5_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS14_6_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74LS14_7_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS14_7_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74LS145" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 13.97 0))
      (property "Value" "74LS145" (id 1) (at -7.62 -16.51 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS145" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL DECOD10 OpenColl" (id 5) (at 0 0 0))
      (property "ki_description" "Decoder 1 to 10, Open Collector" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP?16*" (id 7) (at 0 0 0))
      (symbol "74LS145_1_0"
        (pin open_collector inverted (at 12.7 10.16 180) (length 5.08)
          (name "Q0")
          (number "1")
        )
        (pin open_collector inverted (at 12.7 -10.16 180) (length 5.08)
          (name "Q8")
          (number "10")
        )
        (pin open_collector inverted (at 12.7 -12.7 180) (length 5.08)
          (name "Q9")
          (number "11")
        )
        (pin input line (at -12.7 2.54 0) (length 5.08)
          (name "P3")
          (number "12")
        )
        (pin input line (at -12.7 5.08 0) (length 5.08)
          (name "P2")
          (number "13")
        )
        (pin input line (at -12.7 7.62 0) (length 5.08)
          (name "P1")
          (number "14")
        )
        (pin input line (at -12.7 10.16 0) (length 5.08)
          (name "P0")
          (number "15")
        )
        (pin power_in line (at 0 17.78 270) (length 5.08)
          (name "VCC")
          (number "16")
        )
        (pin open_collector inverted (at 12.7 7.62 180) (length 5.08)
          (name "Q1")
          (number "2")
        )
        (pin open_collector inverted (at 12.7 5.08 180) (length 5.08)
          (name "Q2")
          (number "3")
        )
        (pin open_collector inverted (at 12.7 2.54 180) (length 5.08)
          (name "Q3")
          (number "4")
        )
        (pin open_collector inverted (at 12.7 0 180) (length 5.08)
          (name "Q4")
          (number "5")
        )
        (pin open_collector inverted (at 12.7 -2.54 180) (length 5.08)
          (name "Q5")
          (number "6")
        )
        (pin open_collector inverted (at 12.7 -5.08 180) (length 5.08)
          (name "Q6")
          (number "7")
        )
        (pin power_in line (at 0 -20.32 90) (length 5.08)
          (name "GND")
          (number "8")
        )
        (pin open_collector inverted (at 12.7 -7.62 180) (length 5.08)
          (name "Q7")
          (number "9")
        )
      )
      (symbol "74LS145_1_1"
        (rectangle (start -7.62 12.7) (end 7.62 -15.24)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74LS38" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "74LS38" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL Nand2 OpenCol Buffer" (id 5) (at 0 0 0))
      (property "ki_description" "Quad Buffer 2-input NAND Open collector" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0))
      (symbol "74LS38_1_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS38_1_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "1")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "2")
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS38_2_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS38_2_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "4")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "5")
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS38_3_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS38_3_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "10")
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS38_4_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin open_collector inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS38_4_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin open_collector line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "12")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS38_5_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS38_5_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "74xx_IEEE:7407" (pin_names (offset 0.762)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 3.81 8.89 0))
      (property "Value" "7407" (id 1) (at 3.81 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "7407_0_1"
        (rectangle (start -6.35 6.35) (end 6.35 -6.35)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 -1.27)
            (xy -1.27 0)
            (xy -2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.048 1.016)
            (xy 4.064 2.032)
            (xy 2.54 3.556)
            (xy 1.016 2.032)
            (xy 2.032 1.016)
            (xy 1.016 1.016)
            (xy 4.064 1.016)
            (xy 4.064 1.016)
          )
          (fill (type none))
        )
        (pin power_in line (at 0 6.35 270) (length 0) hide
          (name "Vcc")
          (number "14")
        )
        (pin power_in line (at 0 -6.35 90) (length 0) hide
          (name "Gnd")
          (number "7")
        )
      )
      (symbol "7407_1_1"
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "1")
        )
        (pin open_collector line (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "2")
        )
      )
      (symbol "7407_2_1"
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "3")
        )
        (pin open_collector line (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "4")
        )
      )
      (symbol "7407_3_1"
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "5")
        )
        (pin open_collector line (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "6")
        )
      )
      (symbol "7407_4_1"
        (pin open_collector line (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "8")
        )
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "9")
        )
      )
      (symbol "7407_5_1"
        (pin open_collector line (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "10")
        )
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "11")
        )
      )
      (symbol "7407_6_1"
        (pin open_collector line (at 13.97 0 180) (length 7.62)
          (name "~")
          (number "12")
        )
        (pin input line (at -13.97 0 0) (length 7.62)
          (name "~")
          (number "13")
        )
      )
    )
    (symbol "Connector:DIN-8" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 3.175 5.715 0))
      (property "Value" "DIN-8" (id 1) (at 2.032 -5.842 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "circular DIN connector" (id 4) (at 0 0 0))
      (property "ki_description" "8-pin DIN connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIN*" (id 6) (at 0 0 0))
      (symbol "DIN-8_0_1"
        (arc (start -5.08 0) (mid -3.8609 -3.3364) (end -0.762 -5.08)
          (fill (type none))
        )
        (circle (center -3.048 -0.762) (radius 0.508)
          (fill (type none))
        )
        (circle (center -2.54 2.032) (radius 0.508)
          (fill (type none))
        )
        (circle (center -1.524 -2.794) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 0)
            (xy -3.556 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.508)
            (xy 0 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 0)
            (xy 3.556 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -4.318 -2.54)
            (xy -2.032 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.54)
            (xy -4.318 2.54)
            (xy -3.048 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 4.318 -2.54)
            (xy 2.032 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 2.54)
            (xy 4.318 2.54)
            (xy 3.048 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 -4.953)
            (xy -0.762 -4.191)
            (xy 0.762 -4.191)
            (xy 0.762 -4.953)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 0 3.302) (radius 0.508)
          (fill (type none))
        )
        (arc (start 0.762 -5.08) (mid 3.8685 -3.343) (end 5.08 0)
          (fill (type none))
        )
        (circle (center 1.524 -2.794) (radius 0.508)
          (fill (type none))
        )
        (circle (center 2.54 2.032) (radius 0.508)
          (fill (type none))
        )
        (circle (center 3.048 -0.762) (radius 0.508)
          (fill (type none))
        )
        (arc (start 5.08 0) (mid 0 5.08) (end -5.08 0)
          (fill (type none))
        )
      )
      (symbol "DIN-8_1_1"
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at -7.62 2.54 0) (length 2.54)
          (name "~")
          (number "4")
        )
        (pin passive line (at 7.62 2.54 180) (length 2.54)
          (name "~")
          (number "5")
        )
        (pin passive line (at -7.62 -2.54 0) (length 2.54)
          (name "~")
          (number "6")
        )
        (pin passive line (at 7.62 -2.54 180) (length 2.54)
          (name "~")
          (number "7")
        )
        (pin passive line (at 0 -7.62 90) (length 2.54)
          (name "~")
          (number "8")
        )
      )
    )
    (symbol "Device:Buzzer" (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BZ" (id 0) (at 3.81 1.27 0))
      (property "Value" "Buzzer" (id 1) (at 3.81 -1.27 0))
      (property "Footprint" "" (id 2) (at -0.635 2.54 90))
      (property "Datasheet" "~" (id 3) (at -0.635 2.54 90))
      (property "ki_keywords" "quartz resonator ceramic" (id 4) (at 0 0 0))
      (property "ki_description" "Buzzer, polarized" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "*Buzzer*" (id 6) (at 0 0 0))
      (symbol "Buzzer_0_1"
        (arc (start 0 -3.175) (mid 3.175 0) (end 0 3.175)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.651 1.905)
            (xy -1.143 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.397 2.159)
            (xy -1.397 1.651)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 3.175)
            (xy 0 -3.175)
          )
          (fill (type none))
        )
      )
      (symbol "Buzzer_1_1"
        (pin passive line (at -2.54 2.54 0) (length 2.54)
          (name "-")
          (number "1")
        )
        (pin passive line (at -2.54 -2.54 0) (length 2.54)
          (name "+")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0))
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Network08" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RN" (id 0) (at -12.7 0 90))
      (property "Value" "R_Network08" (id 1) (at 10.16 0 90))
      (property "Footprint" "Resistor_THT:R_Array_SIP9" (id 2) (at 12.065 0 90))
      (property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "R network star-topology" (id 4) (at 0 0 0))
      (property "ki_description" "8 resistor network, star topology, bussed resistors, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R?Array?SIP*" (id 6) (at 0 0 0))
      (symbol "R_Network08_0_1"
        (rectangle (start -11.43 -3.175) (end 8.89 3.175)
          (fill (type background))
        )
        (rectangle (start -10.922 1.524) (end -9.398 -2.54)
          (fill (type none))
        )
        (circle (center -10.16 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -8.382 1.524) (end -6.858 -2.54)
          (fill (type none))
        )
        (circle (center -7.62 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -5.842 1.524) (end -4.318 -2.54)
          (fill (type none))
        )
        (circle (center -5.08 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -3.302 1.524) (end -1.778 -2.54)
          (fill (type none))
        )
        (circle (center -2.54 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start -0.762 1.524) (end 0.762 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -10.16 -2.54)
            (xy -10.16 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 -2.54)
            (xy -7.62 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 -2.54)
            (xy 7.62 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -10.16 1.524)
            (xy -10.16 2.286)
            (xy -7.62 2.286)
            (xy -7.62 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 1.524)
            (xy -7.62 2.286)
            (xy -5.08 2.286)
            (xy -5.08 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.524)
            (xy -5.08 2.286)
            (xy -2.54 2.286)
            (xy -2.54 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.524)
            (xy -2.54 2.286)
            (xy 0 2.286)
            (xy 0 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.524)
            (xy 0 2.286)
            (xy 2.54 2.286)
            (xy 2.54 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.524)
            (xy 2.54 2.286)
            (xy 5.08 2.286)
            (xy 5.08 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 1.524)
            (xy 5.08 2.286)
            (xy 7.62 2.286)
            (xy 7.62 1.524)
          )
          (fill (type none))
        )
        (circle (center 0 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 1.778 1.524) (end 3.302 -2.54)
          (fill (type none))
        )
        (circle (center 2.54 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 4.318 1.524) (end 5.842 -2.54)
          (fill (type none))
        )
        (circle (center 5.08 2.286) (radius 0.254)
          (fill (type outline))
        )
        (rectangle (start 6.858 1.524) (end 8.382 -2.54)
          (fill (type none))
        )
      )
      (symbol "R_Network08_1_1"
        (pin passive line (at -10.16 5.08 270) (length 2.54)
          (name "common")
          (number "1")
        )
        (pin passive line (at -10.16 -5.08 90) (length 1.27)
          (name "R1")
          (number "2")
        )
        (pin passive line (at -7.62 -5.08 90) (length 1.27)
          (name "R2")
          (number "3")
        )
        (pin passive line (at -5.08 -5.08 90) (length 1.27)
          (name "R3")
          (number "4")
        )
        (pin passive line (at -2.54 -5.08 90) (length 1.27)
          (name "R4")
          (number "5")
        )
        (pin passive line (at 0 -5.08 90) (length 1.27)
          (name "R5")
          (number "6")
        )
        (pin passive line (at 2.54 -5.08 90) (length 1.27)
          (name "R6")
          (number "7")
        )
        (pin passive line (at 5.08 -5.08 90) (length 1.27)
          (name "R7")
          (number "8")
        )
        (pin passive line (at 7.62 -5.08 90) (length 1.27)
          (name "R8")
          (number "9")
        )
      )
    )
    (symbol "LED:LD271" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0.508 1.778 0))
      (property "Value" "LD271" (id 1) (at -1.016 -2.794 0))
      (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (id 2) (at 0 4.445 0))
      (property "Datasheet" "http://www.alliedelec.com/m/d/40788c34903a719969df15f1fbea1056.pdf" (id 3) (at -1.27 0 0))
      (property "ki_keywords" "IR LED" (id 4) (at 0 0 0))
      (property "ki_description" "940nm IR-LED, 5mm" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED*5.0mm*IRGrey*" (id 6) (at 0 0 0))
      (symbol "LD271_0_1"
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.381 3.175)
            (xy -0.127 3.175)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.143 1.651)
            (xy 0.381 3.175)
            (xy 0.381 2.667)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy -2.54 0)
            (xy 0 1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.413 1.651)
            (xy -0.889 3.175)
            (xy -0.889 2.667)
            (xy -0.889 3.175)
            (xy -1.397 3.175)
          )
          (fill (type none))
        )
      )
      (symbol "LD271_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "MCU_Intel:8049" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -13.97 35.56 0))
      (property "Value" "8049" (id 1) (at 8.89 35.56 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "MCS-48 uC Microcontroller" (id 4) (at 0 0 0))
      (property "ki_description" "MCS-48 8-bit Microcontroller, 2KB Mask ROM, 128B RAM, DIP-40" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP* PDIP*" (id 6) (at 0 0 0))
      (symbol "8049_1_1"
        (rectangle (start -13.97 -34.29) (end 13.97 34.29)
          (fill (type background))
        )
        (pin input line (at -17.78 -25.4 0) (length 3.81)
          (name "T0")
          (number "1")
        )
        (pin output output_low (at 17.78 -12.7 180) (length 3.81)
          (name "~{WR}")
          (number "10")
        )
        (pin output line (at 17.78 -2.54 180) (length 3.81)
          (name "ALE")
          (number "11")
        )
        (pin bidirectional line (at 17.78 20.32 180) (length 3.81)
          (name "DB.0")
          (number "12")
        )
        (pin bidirectional line (at 17.78 17.78 180) (length 3.81)
          (name "DB.1")
          (number "13")
        )
        (pin bidirectional line (at 17.78 15.24 180) (length 3.81)
          (name "DB.2")
          (number "14")
        )
        (pin bidirectional line (at 17.78 12.7 180) (length 3.81)
          (name "DB.3")
          (number "15")
        )
        (pin bidirectional line (at 17.78 10.16 180) (length 3.81)
          (name "DB.4")
          (number "16")
        )
        (pin bidirectional line (at 17.78 7.62 180) (length 3.81)
          (name "DB.5")
          (number "17")
        )
        (pin bidirectional line (at 17.78 5.08 180) (length 3.81)
          (name "DB.6")
          (number "18")
        )
        (pin bidirectional line (at 17.78 2.54 180) (length 3.81)
          (name "DB.7")
          (number "19")
        )
        (pin input line (at 17.78 -25.4 180) (length 3.81)
          (name "X1")
          (number "2")
        )
        (pin power_in line (at 0 -38.1 90) (length 3.81)
          (name "GND")
          (number "20")
        )
        (pin bidirectional line (at -17.78 2.54 0) (length 3.81)
          (name "P2.0")
          (number "21")
        )
        (pin bidirectional line (at -17.78 0 0) (length 3.81)
          (name "P2.1")
          (number "22")
        )
        (pin bidirectional line (at -17.78 -2.54 0) (length 3.81)
          (name "P2.2")
          (number "23")
        )
        (pin bidirectional line (at -17.78 -5.08 0) (length 3.81)
          (name "P2.3")
          (number "24")
        )
        (pin output line (at -17.78 -20.32 0) (length 3.81)
          (name "PROG")
          (number "25")
        )
        (pin power_in line (at 17.78 30.48 180) (length 3.81)
          (name "VDD")
          (number "26")
        )
        (pin bidirectional line (at -17.78 25.4 0) (length 3.81)
          (name "P1.0")
          (number "27")
        )
        (pin bidirectional line (at -17.78 22.86 0) (length 3.81)
          (name "P1.1")
          (number "28")
        )
        (pin bidirectional line (at -17.78 20.32 0) (length 3.81)
          (name "P1.2")
          (number "29")
        )
        (pin output line (at 17.78 -30.48 180) (length 3.81)
          (name "X2")
          (number "3")
        )
        (pin bidirectional line (at -17.78 17.78 0) (length 3.81)
          (name "P1.3")
          (number "30")
        )
        (pin bidirectional line (at -17.78 15.24 0) (length 3.81)
          (name "P1.4")
          (number "31")
        )
        (pin bidirectional line (at -17.78 12.7 0) (length 3.81)
          (name "P1.5")
          (number "32")
        )
        (pin bidirectional line (at -17.78 10.16 0) (length 3.81)
          (name "P1.6")
          (number "33")
        )
        (pin bidirectional line (at -17.78 7.62 0) (length 3.81)
          (name "P1.7")
          (number "34")
        )
        (pin bidirectional line (at -17.78 -7.62 0) (length 3.81)
          (name "P2.4")
          (number "35")
        )
        (pin bidirectional line (at -17.78 -10.16 0) (length 3.81)
          (name "P2.5")
          (number "36")
        )
        (pin bidirectional line (at -17.78 -12.7 0) (length 3.81)
          (name "P2.6")
          (number "37")
        )
        (pin bidirectional line (at -17.78 -15.24 0) (length 3.81)
          (name "P2.7")
          (number "38")
        )
        (pin input line (at -17.78 -27.94 0) (length 3.81)
          (name "T1")
          (number "39")
        )
        (pin input inverted (at -17.78 30.48 0) (length 3.81)
          (name "~{RESET}")
          (number "4")
        )
        (pin power_in line (at 0 38.1 270) (length 3.81)
          (name "VCC")
          (number "40")
        )
        (pin input inverted (at 17.78 -17.78 180) (length 3.81)
          (name "~{SS}")
          (number "5")
        )
        (pin input inverted (at -17.78 -30.48 0) (length 3.81)
          (name "~{INT}")
          (number "6")
        )
        (pin input line (at 17.78 25.4 180) (length 3.81)
          (name "EA")
          (number "7")
        )
        (pin output output_low (at 17.78 -10.16 180) (length 3.81)
          (name "~{RD}")
          (number "8")
        )
        (pin output output_low (at 17.78 -7.62 180) (length 3.81)
          (name "~{PSEN}")
          (number "9")
        )
      )
    )
    (symbol "Simulation_SPICE:DIODE" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "DIODE" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Spice_Netlist_Enabled" "Y" (id 4) (at 0 0 0))
      (property "Spice_Primitive" "D" (id 5) (at 0 0 0))
      (property "ki_keywords" "simulation" (id 6) (at 0 0 0))
      (property "ki_description" "Diode, anode on pin 1, for simulation only!" (id 7) (at 0 0 0))
      (symbol "DIODE_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
            (xy 1.27 0)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "DIODE_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "pspice:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "resistor simulation" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor symbol for simulation only" (id 5) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 3.81) (end 1.016 -3.81)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 6.35 270) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -6.35 90) (length 2.54)
          (name "~")
          (number "2")
        )
      )
    )
  )
  (junction (at 565.15 471.17) (diameter 0) (color 0 0 0 0))
  (junction (at 560.07 488.95) (diameter 0) (color 0 0 0 0))
  (junction (at 524.5922 363.22) (diameter 0) (color 0 0 0 0))
  (junction (at 497.84 355.6) (diameter 0) (color 0 0 0 0))
  (junction (at 391.16 459.74) (diameter 0) (color 0 0 0 0))
  (junction (at 542.29 447.04) (diameter 0) (color 0 0 0 0))
  (junction (at 435.61 340.36) (diameter 0) (color 0 0 0 0))
  (junction (at 542.29 449.58) (diameter 0) (color 0 0 0 0))
  (junction (at 457.2 322.58) (diameter 0) (color 0 0 0 0))
  (junction (at 396.24 464.82) (diameter 0) (color 0 0 0 0))
  (junction (at 457.2 314.96) (diameter 0) (color 0 0 0 0))
  (junction (at 542.29 454.66) (diameter 0) (color 0 0 0 0))
  (junction (at 554.99 506.73) (diameter 0) (color 0 0 0 0))
  (junction (at 549.91 524.51) (diameter 0) (color 0 0 0 0))
  (junction (at 497.84 325.12) (diameter 0) (color 0 0 0 0))
  (junction (at 557.53 497.84) (diameter 0) (color 0 0 0 0))
  (junction (at 393.7 462.28) (diameter 0) (color 0 0 0 0))
  (junction (at 497.84 340.36) (diameter 0) (color 0 0 0 0))
  (junction (at 567.69 463.55) (diameter 0) (color 0 0 0 0))
  (junction (at 552.45 515.62) (diameter 0) (color 0 0 0 0))
  (junction (at 542.29 452.12) (diameter 0) (color 0 0 0 0))
  (junction (at 542.29 444.5) (diameter 0) (color 0 0 0 0))
  (junction (at 435.61 323.85) (diameter 0) (color 0 0 0 0))
  (junction (at 388.62 457.2) (diameter 0) (color 0 0 0 0))
  (junction (at 562.61 480.06) (diameter 0) (color 0 0 0 0))
  (no_connect (at 441.96 520.7))
  (no_connect (at 441.96 518.16))
  (no_connect (at 441.96 480.06))
  (no_connect (at 441.96 477.52))
  (no_connect (at 542.29 420.37))
  (no_connect (at 542.29 417.83))
  (no_connect (at 542.29 415.29))
  (no_connect (at 542.29 410.21))
  (no_connect (at 506.73 427.99))
  (no_connect (at 542.29 425.45))
  (no_connect (at 506.73 433.07))
  (no_connect (at 506.73 435.61))
  (no_connect (at 543.56 289.56))
  (no_connect (at 506.73 384.81))
  (no_connect (at 506.73 387.35))
  (no_connect (at 506.73 389.89))
  (wire (pts (xy 358.14 375.92) (xy 453.39 375.92)))
  (wire (pts (xy 377.19 429.26) (xy 377.19 422.91)))
  (wire (pts (xy 542.29 430.53) (xy 548.64 430.53)))
  (wire (pts (xy 585.47 400.05) (xy 585.47 480.06)))
  (wire (pts (xy 546.1 524.51) (xy 549.91 524.51)))
  (wire (pts (xy 560.07 488.95) (xy 560.07 525.78)))
  (wire (pts (xy 506.73 415.29) (xy 382.27 415.29)))
  (wire (pts (xy 562.61 441.96) (xy 552.45 441.96)))
  (wire (pts (xy 542.29 433.07) (xy 542.29 430.53)))
  (wire (pts (xy 382.27 415.29) (xy 382.27 354.33)))
  (wire (pts (xy 596.9 392.43) (xy 596.9 506.73)))
  (wire (pts (xy 565.15 471.17) (xy 581.66 471.17)))
  (wire (pts (xy 412.75 326.39) (xy 412.75 323.85)))
  (wire (pts (xy 548.64 440.69) (xy 548.64 439.42)))
  (wire (pts (xy 391.16 459.74) (xy 416.56 459.74)))
  (wire (pts (xy 457.2 273.05) (xy 457.2 271.78)))
  (wire (pts (xy 506.73 394.97) (xy 369.57 394.97)))
  (wire (pts (xy 435.61 340.36) (xy 435.61 323.85)))
  (wire (pts (xy 506.73 377.19) (xy 506.73 309.88)))
  (wire (pts (xy 412.75 323.85) (xy 415.29 323.85)))
  (wire (pts (xy 546.1 497.84) (xy 557.53 497.84)))
  (wire (pts (xy 510.54 278.13) (xy 441.96 278.13)))
  (wire (pts (xy 542.29 447.04) (xy 542.29 449.58)))
  (wire (pts (xy 453.39 353.06) (xy 457.2 353.06)))
  (wire (pts (xy 554.99 449.58) (xy 554.99 506.73)))
  (wire (pts (xy 382.27 354.33) (xy 384.81 354.33)))
  (wire (pts (xy 552.45 515.62) (xy 570.23 515.62)))
  (wire (pts (xy 421.64 354.33) (xy 422.91 354.33)))
  (wire (pts (xy 604.52 387.35) (xy 604.52 524.51)))
  (wire (pts (xy 388.62 497.84) (xy 416.56 497.84)))
  (wire (pts (xy 497.84 340.36) (xy 497.84 355.6)))
  (wire (pts (xy 554.99 506.73) (xy 570.23 506.73)))
  (wire (pts (xy 567.69 535.94) (xy 580.39 535.94)))
  (wire (pts (xy 542.29 382.27) (xy 547.37 382.27)))
  (wire (pts (xy 542.29 438.15) (xy 542.29 440.69)))
  (wire (pts (xy 412.75 340.36) (xy 414.02 340.36)))
  (wire (pts (xy 457.2 360.68) (xy 497.84 360.68)))
  (wire (pts (xy 472.44 325.12) (xy 474.98 325.12)))
  (wire (pts (xy 379.73 417.83) (xy 379.73 340.36)))
  (wire (pts (xy 372.11 392.43) (xy 372.11 326.39)))
  (wire (pts (xy 501.65 322.58) (xy 501.65 325.12)))
  (wire (pts (xy 457.2 322.58) (xy 457.2 337.82)))
  (wire (pts (xy 542.29 452.12) (xy 542.29 454.66)))
  (wire (pts (xy 562.61 525.78) (xy 562.61 480.06)))
  (wire (pts (xy 565.15 471.17) (xy 565.15 525.78)))
  (wire (pts (xy 421.64 340.36) (xy 422.91 340.36)))
  (wire (pts (xy 393.7 502.92) (xy 393.7 462.28)))
  (wire (pts (xy 367.03 312.42) (xy 384.81 312.42)))
  (wire (pts (xy 457.2 358.14) (xy 457.2 360.68)))
  (wire (pts (xy 443.23 382.27) (xy 443.23 327.66)))
  (wire (pts (xy 552.45 452.12) (xy 552.45 515.62)))
  (wire (pts (xy 557.53 447.04) (xy 552.45 447.04)))
  (wire (pts (xy 396.24 412.75) (xy 506.73 412.75)))
  (wire (pts (xy 420.37 323.85) (xy 422.91 323.85)))
  (wire (pts (xy 358.14 429.26) (xy 358.14 375.92)))
  (wire (pts (xy 570.23 524.51) (xy 549.91 524.51)))
  (wire (pts (xy 367.03 400.05) (xy 367.03 312.42)))
  (wire (pts (xy 482.6 340.36) (xy 485.14 340.36)))
  (wire (pts (xy 549.91 449.58) (xy 554.99 449.58)))
  (wire (pts (xy 391.16 407.67) (xy 506.73 407.67)))
  (wire (pts (xy 549.91 524.51) (xy 549.91 457.2)))
  (wire (pts (xy 440.69 297.18) (xy 457.2 297.18)))
  (wire (pts (xy 472.44 309.88) (xy 506.73 309.88)))
  (wire (pts (xy 497.84 340.36) (xy 497.84 325.12)))
  (wire (pts (xy 593.09 497.84) (xy 585.47 497.84)))
  (wire (pts (xy 440.69 307.34) (xy 440.69 297.18)))
  (wire (pts (xy 391.16 500.38) (xy 391.16 459.74)))
  (wire (pts (xy 497.84 325.12) (xy 497.84 314.96)))
  (wire (pts (xy 457.2 312.42) (xy 457.2 314.96)))
  (wire (pts (xy 396.24 464.82) (xy 396.24 412.75)))
  (wire (pts (xy 546.1 463.55) (xy 567.69 463.55)))
  (wire (pts (xy 411.48 505.46) (xy 416.56 505.46)))
  (wire (pts (xy 384.81 397.51) (xy 384.81 368.3)))
  (wire (pts (xy 542.29 400.05) (xy 585.47 400.05)))
  (wire (pts (xy 410.21 273.05) (xy 426.72 273.05)))
  (wire (pts (xy 457.2 314.96) (xy 497.84 314.96)))
  (wire (pts (xy 560.07 444.5) (xy 552.45 444.5)))
  (wire (pts (xy 570.23 488.95) (xy 560.07 488.95)))
  (wire (pts (xy 542.29 397.51) (xy 589.28 397.51)))
  (wire (pts (xy 361.95 420.37) (xy 361.95 378.46)))
  (wire (pts (xy 435.61 314.96) (xy 457.2 314.96)))
  (wire (pts (xy 455.93 307.34) (xy 457.2 307.34)))
  (wire (pts (xy 542.29 441.96) (xy 542.29 444.5)))
  (wire (pts (xy 416.56 500.38) (xy 391.16 500.38)))
  (wire (pts (xy 412.75 368.3) (xy 510.54 368.3)))
  (wire (pts (xy 388.62 457.2) (xy 388.62 497.84)))
  (wire (pts (xy 379.73 340.36) (xy 384.81 340.36)))
  (wire (pts (xy 372.11 326.39) (xy 384.81 326.39)))
  (wire (pts (xy 482.6 325.12) (xy 485.14 325.12)))
  (wire (pts (xy 377.19 420.37) (xy 506.73 420.37)))
  (wire (pts (xy 435.61 340.36) (xy 435.61 354.33)))
  (wire (pts (xy 549.91 524.51) (xy 549.91 525.78)))
  (wire (pts (xy 560.07 488.95) (xy 560.07 444.5)))
  (wire (pts (xy 435.61 323.85) (xy 435.61 314.96)))
  (wire (pts (xy 393.7 462.28) (xy 393.7 410.21)))
  (wire (pts (xy 415.29 275.59) (xy 426.72 275.59)))
  (wire (pts (xy 562.61 480.06) (xy 570.23 480.06)))
  (wire (pts (xy 585.47 488.95) (xy 589.28 488.95)))
  (wire (pts (xy 600.71 389.89) (xy 600.71 515.62)))
  (wire (pts (xy 542.29 444.5) (xy 542.29 447.04)))
  (wire (pts (xy 354.33 278.13) (xy 426.72 278.13)))
  (wire (pts (xy 361.95 429.26) (xy 358.14 429.26)))
  (wire (pts (xy 552.45 515.62) (xy 552.45 525.78)))
  (wire (pts (xy 497.84 360.68) (xy 497.84 355.6)))
  (wire (pts (xy 542.29 405.13) (xy 577.85 405.13)))
  (wire (pts (xy 542.29 449.58) (xy 542.29 452.12)))
  (wire (pts (xy 546.1 480.06) (xy 562.61 480.06)))
  (wire (pts (xy 577.85 405.13) (xy 577.85 463.55)))
  (wire (pts (xy 396.24 464.82) (xy 396.24 490.22)))
  (wire (pts (xy 441.96 273.05) (xy 457.2 273.05)))
  (wire (pts (xy 472.44 340.36) (xy 474.98 340.36)))
  (wire (pts (xy 412.75 298.45) (xy 412.75 267.97)))
  (wire (pts (xy 412.75 312.42) (xy 415.29 312.42)))
  (wire (pts (xy 542.29 392.43) (xy 596.9 392.43)))
  (wire (pts (xy 441.96 457.2) (xy 542.29 457.2)))
  (wire (pts (xy 450.85 342.9) (xy 457.2 342.9)))
  (wire (pts (xy 567.69 463.55) (xy 567.69 525.78)))
  (wire (pts (xy 361.95 378.46) (xy 450.85 378.46)))
  (wire (pts (xy 570.23 497.84) (xy 557.53 497.84)))
  (wire (pts (xy 546.1 471.17) (xy 565.15 471.17)))
  (wire (pts (xy 604.52 524.51) (xy 585.47 524.51)))
  (wire (pts (xy 567.69 463.55) (xy 577.85 463.55)))
  (wire (pts (xy 581.66 402.59) (xy 581.66 471.17)))
  (wire (pts (xy 396.24 464.82) (xy 416.56 464.82)))
  (wire (pts (xy 412.75 354.33) (xy 414.02 354.33)))
  (wire (pts (xy 542.29 457.2) (xy 542.29 454.66)))
  (wire (pts (xy 369.57 298.45) (xy 384.81 298.45)))
  (wire (pts (xy 416.56 502.92) (xy 393.7 502.92)))
  (wire (pts (xy 557.53 497.84) (xy 557.53 525.78)))
  (wire (pts (xy 542.29 394.97) (xy 593.09 394.97)))
  (wire (pts (xy 482.6 355.6) (xy 485.14 355.6)))
  (wire (pts (xy 472.44 355.6) (xy 474.98 355.6)))
  (wire (pts (xy 557.53 497.84) (xy 557.53 447.04)))
  (wire (pts (xy 457.2 275.59) (xy 441.96 275.59)))
  (wire (pts (xy 450.85 378.46) (xy 450.85 342.9)))
  (wire (pts (xy 506.73 397.51) (xy 384.81 397.51)))
  (wire (pts (xy 524.51 363.22) (xy 524.51 369.57)))
  (wire (pts (xy 406.4 438.15) (xy 354.33 438.15)))
  (wire (pts (xy 457.2 297.18) (xy 457.2 275.59)))
  (wire (pts (xy 416.56 457.2) (xy 388.62 457.2)))
  (wire (pts (xy 548.64 430.53) (xy 548.64 431.8)))
  (wire (pts (xy 388.62 405.13) (xy 506.73 405.13)))
  (wire (pts (xy 453.39 375.92) (xy 453.39 353.06)))
  (wire (pts (xy 457.2 314.96) (xy 457.2 322.58)))
  (wire (pts (xy 412.75 267.97) (xy 434.34 267.97)))
  (wire (pts (xy 506.73 400.05) (xy 367.03 400.05)))
  (wire (pts (xy 542.29 389.89) (xy 600.71 389.89)))
  (wire (pts (xy 546.1 506.73) (xy 554.99 506.73)))
  (wire (pts (xy 443.23 327.66) (xy 457.2 327.66)))
  (wire (pts (xy 542.29 440.69) (xy 548.64 440.69)))
  (wire (pts (xy 542.29 402.59) (xy 581.66 402.59)))
  (wire (pts (xy 542.29 387.35) (xy 604.52 387.35)))
  (wire (pts (xy 391.16 459.74) (xy 391.16 407.67)))
  (wire (pts (xy 589.28 397.51) (xy 589.28 488.95)))
  (wire (pts (xy 377.19 422.91) (xy 506.73 422.91)))
  (wire (pts (xy 411.48 505.46) (xy 411.48 490.22)))
  (wire (pts (xy 501.65 325.12) (xy 497.84 325.12)))
  (wire (pts (xy 506.73 417.83) (xy 379.73 417.83)))
  (wire (pts (xy 438.15 438.15) (xy 506.73 438.15)))
  (wire (pts (xy 506.73 392.43) (xy 372.11 392.43)))
  (wire (pts (xy 524.5922 363.22) (xy 524.51 363.22)))
  (wire (pts (xy 388.62 405.13) (xy 388.62 457.2)))
  (wire (pts (xy 549.91 452.12) (xy 552.45 452.12)))
  (wire (pts (xy 600.71 515.62) (xy 585.47 515.62)))
  (wire (pts (xy 554.99 506.73) (xy 554.99 525.78)))
  (wire (pts (xy 415.29 312.42) (xy 415.29 275.59)))
  (wire (pts (xy 393.7 410.21) (xy 506.73 410.21)))
  (wire (pts (xy 546.1 488.95) (xy 560.07 488.95)))
  (wire (pts (xy 596.9 506.73) (xy 585.47 506.73)))
  (wire (pts (xy 421.64 438.15) (xy 422.91 438.15)))
  (wire (pts (xy 593.09 394.97) (xy 593.09 497.84)))
  (wire (pts (xy 369.57 394.97) (xy 369.57 298.45)))
  (wire (pts (xy 562.61 480.06) (xy 562.61 441.96)))
  (wire (pts (xy 393.7 462.28) (xy 416.56 462.28)))
  (wire (pts (xy 510.54 368.3) (xy 510.54 278.13)))
  (wire (pts (xy 354.33 438.15) (xy 354.33 278.13)))
  (wire (pts (xy 546.1 515.62) (xy 552.45 515.62)))
  (wire (pts (xy 443.23 382.27) (xy 506.73 382.27)))
  (label "CN1 blu" (at 405.13 309.88 0))
  (label "CN1 org" (at 440.69 295.91 0))
  (label "CN1 wht" (at 405.13 365.76 0))
  (label "DATA" (at 406.4 300.99 0))
  (label "CLOCK" (at 406.4 314.96 0))
  (label "CN1 yel" (at 405.13 295.91 0))
  (label "CN1 red" (at 459.74 270.51 0))
  (label "CN1 dgn" (at 400.05 435.61 0))
  (label "CN1 lgn" (at 400.05 274.32 0))
  (label "RESET" (at 438.15 309.88 0))
  (symbol (lib_id "74xx_IEEE:7407") (at 398.78 326.39 0) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "M4" (id 0) (at 398.78 328.93 0))
    (property "Value" "7407" (id 1) (at 398.78 331.47 0))
    (property "Footprint" "" (id 2) (at 398.78 326.39 0))
    (property "Datasheet" "" (id 3) (at 398.78 326.39 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "LED:LD271") (at 480.06 325.12 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 478.917 316.23 0))
    (property "Value" "HOLD" (id 1) (at 478.917 318.77 0))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (id 2) (at 480.06 320.675 0))
    (property "Datasheet" "http://www.alliedelec.com/m/d/40788c34903a719969df15f1fbea1056.pdf" (id 3) (at 478.79 325.12 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS145") (at 429.26 467.36 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M2" (id 0) (at 431.2794 449.58 0))
    (property "Value" "74LS145" (id 1) (at 431.2794 452.12 0))
    (property "Footprint" "" (id 2) (at 429.26 467.36 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS145" (id 3) (at 429.26 467.36 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "74xx_IEEE:7407") (at 398.78 312.42 0) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "M4" (id 0) (at 398.78 314.96 0))
    (property "Value" "7407" (id 1) (at 398.78 317.5 0))
    (property "Footprint" "" (id 2) (at 398.78 312.42 0))
    (property "Datasheet" "" (id 3) (at 398.78 312.42 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "pspice:R") (at 491.49 340.36 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 491.49 334.01 90))
    (property "Value" "R" (id 1) (at 491.49 336.55 90))
    (property "Footprint" "" (id 2) (at 491.49 340.36 0))
    (property "Datasheet" "~" (id 3) (at 491.49 340.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS14") (at 414.02 438.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M5" (id 0) (at 414.02 429.26 0))
    (property "Value" "74LS14" (id 1) (at 414.02 431.8 0))
    (property "Footprint" "" (id 2) (at 414.02 438.15 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 414.02 438.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS38") (at 464.82 325.12 0) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 464.82 316.23 0))
    (property "Value" "74LS38" (id 1) (at 464.82 318.77 0))
    (property "Footprint" "" (id 2) (at 464.82 325.12 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 464.82 325.12 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:GND") (at 547.37 382.27 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 553.72 382.27 0))
    (property "Value" "GND" (id 1) (at 551.18 382.2699 90))
    (property "Footprint" "" (id 2) (at 547.37 382.27 0))
    (property "Datasheet" "" (id 3) (at 547.37 382.27 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 457.2 271.78 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 457.2 275.59 0))
    (property "Value" "+5V" (id 1) (at 457.2 266.7 0))
    (property "Footprint" "" (id 2) (at 457.2 271.78 0))
    (property "Datasheet" "" (id 3) (at 457.2 271.78 0))
    (pin "1")
  )
  (symbol (lib_id "74xx_IEEE:7407") (at 398.78 368.3 0) (unit 6)
    (in_bom yes) (on_board yes)
    (property "Reference" "M4" (id 0) (at 398.78 370.84 0))
    (property "Value" "7407" (id 1) (at 398.78 373.38 0))
    (property "Footprint" "" (id 2) (at 398.78 368.3 0))
    (property "Datasheet" "" (id 3) (at 398.78 368.3 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "LED:LD271") (at 480.06 355.6 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 478.917 346.71 0))
    (property "Value" "Num Lock" (id 1) (at 478.917 349.25 0))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (id 2) (at 480.06 351.155 0))
    (property "Datasheet" "http://www.alliedelec.com/m/d/40788c34903a719969df15f1fbea1056.pdf" (id 3) (at 478.79 355.6 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS14") (at 448.31 307.34 0) (unit 3)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M5" (id 0) (at 448.31 298.45 0))
    (property "Value" "74LS14" (id 1) (at 448.31 300.99 0))
    (property "Footprint" "" (id 2) (at 448.31 307.34 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 448.31 307.34 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS38") (at 464.82 355.6 0) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 464.82 346.71 0))
    (property "Value" "74LS38" (id 1) (at 464.82 349.25 0))
    (property "Footprint" "" (id 2) (at 464.82 355.6 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 464.82 355.6 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "Device:Buzzer") (at 417.83 326.39 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "BZ" (id 0) (at 414.02 320.04 90))
    (property "Value" "Buzzer" (id 1) (at 414.02 322.58 90))
    (property "Footprint" "" (id 2) (at 420.37 325.755 90))
    (property "Datasheet" "~" (id 3) (at 420.37 325.755 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS145") (at 429.26 508 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M3" (id 0) (at 431.2794 490.22 0))
    (property "Value" "74LS145" (id 1) (at 431.2794 492.76 0))
    (property "Footprint" "" (id 2) (at 429.26 508 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS145" (id 3) (at 429.26 508 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Simulation_SPICE:DIODE") (at 546.1 452.12 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "W4" (id 0) (at 539.75 452.12 0))
    (property "Value" " " (id 1) (at 546.1 448.31 0))
    (property "Footprint" "" (id 2) (at 546.1 452.12 0))
    (property "Datasheet" "~" (id 3) (at 546.1 452.12 0))
    (property "Spice_Netlist_Enabled" "Y" (id 4) (at 546.1 452.12 0))
    (property "Spice_Primitive" "D" (id 5) (at 546.1 452.12 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74LS38") (at 464.82 309.88 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 464.82 300.99 0))
    (property "Value" "74LS38" (id 1) (at 464.82 303.53 0))
    (property "Footprint" "" (id 2) (at 464.82 309.88 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 464.82 309.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "pspice:R") (at 429.26 340.36 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 429.26 334.01 90))
    (property "Value" "R" (id 1) (at 429.26 336.55 90))
    (property "Footprint" "" (id 2) (at 429.26 340.36 0))
    (property "Datasheet" "~" (id 3) (at 429.26 340.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pspice:R") (at 491.49 325.12 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 491.49 318.77 90))
    (property "Value" "R" (id 1) (at 491.49 321.31 90))
    (property "Footprint" "" (id 2) (at 491.49 325.12 0))
    (property "Datasheet" "~" (id 3) (at 491.49 325.12 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 524.5922 363.22 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 524.5922 367.03 0))
    (property "Value" "+5V" (id 1) (at 524.5922 358.14 0))
    (property "Footprint" "" (id 2) (at 524.5922 363.22 0))
    (property "Datasheet" "" (id 3) (at 524.5922 363.22 0))
    (pin "1")
  )
  (symbol (lib_id "4xxx:4050") (at 577.85 515.62 0) (unit 5)
    (in_bom yes) (on_board yes)
    (property "Reference" "M7" (id 0) (at 576.58 514.35 0))
    (property "Value" "4050" (id 1) (at 576.58 516.89 0))
    (property "Footprint" "" (id 2) (at 577.85 515.62 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf" (id 3) (at 577.85 515.62 0))
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "14")
    (pin "15")
    (pin "1")
    (pin "8")
  )
  (symbol (lib_id "74xx:74LS38") (at 464.82 340.36 0) (unit 3)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M6" (id 0) (at 464.82 331.47 0))
    (property "Value" "74LS38" (id 1) (at 464.82 334.01 0))
    (property "Footprint" "" (id 2) (at 464.82 340.36 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS38" (id 3) (at 464.82 340.36 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "pspice:R") (at 491.49 355.6 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 491.49 349.25 90))
    (property "Value" "R" (id 1) (at 491.49 351.79 90))
    (property "Footprint" "" (id 2) (at 491.49 355.6 0))
    (property "Datasheet" "~" (id 3) (at 491.49 355.6 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "4xxx:4050") (at 577.85 497.84 0) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "M7" (id 0) (at 576.58 496.57 0))
    (property "Value" "4050" (id 1) (at 576.58 499.11 0))
    (property "Footprint" "" (id 2) (at 577.85 497.84 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf" (id 3) (at 577.85 497.84 0))
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "14")
    (pin "15")
    (pin "1")
    (pin "8")
  )
  (symbol (lib_id "Connector:DIN-8") (at 434.34 275.59 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J?" (id 0) (at 435.9911 265.43 0))
    (property "Value" "DIN-8" (id 1) (at 435.9911 267.97 0))
    (property "Footprint" "" (id 2) (at 434.34 275.59 0))
    (property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf" (id 3) (at 434.34 275.59 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:Crystal") (at 548.64 435.61 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "X1" (id 0) (at 552.45 434.3399 90))
    (property "Value" "Crystal" (id 1) (at 552.45 436.8799 90))
    (property "Footprint" "" (id 2) (at 548.64 435.61 0))
    (property "Datasheet" "~" (id 3) (at 548.64 435.61 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "LED:LD271") (at 480.06 340.36 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 478.917 331.47 0))
    (property "Value" "Alpha/Caps Lock" (id 1) (at 478.917 334.01 0))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (id 2) (at 480.06 335.915 0))
    (property "Datasheet" "http://www.alliedelec.com/m/d/40788c34903a719969df15f1fbea1056.pdf" (id 3) (at 478.79 340.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "4xxx:4050") (at 577.85 488.95 0) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "M7" (id 0) (at 576.58 487.68 0))
    (property "Value" "4050" (id 1) (at 576.58 490.22 0))
    (property "Footprint" "" (id 2) (at 577.85 488.95 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf" (id 3) (at 577.85 488.95 0))
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "14")
    (pin "15")
    (pin "1")
    (pin "8")
  )
  (symbol (lib_id "Simulation_SPICE:DIODE") (at 546.1 449.58 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "W3" (id 0) (at 539.75 449.58 0))
    (property "Value" " " (id 1) (at 546.1 445.77 0))
    (property "Footprint" "" (id 2) (at 546.1 449.58 0))
    (property "Datasheet" "~" (id 3) (at 546.1 449.58 0))
    (property "Spice_Netlist_Enabled" "Y" (id 4) (at 546.1 449.58 0))
    (property "Spice_Primitive" "D" (id 5) (at 546.1 449.58 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "4xxx:4050") (at 577.85 480.06 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "M7" (id 0) (at 576.58 478.79 0))
    (property "Value" "4050" (id 1) (at 576.58 481.33 0))
    (property "Footprint" "" (id 2) (at 577.85 480.06 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf" (id 3) (at 577.85 480.06 0))
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "14")
    (pin "15")
    (pin "1")
    (pin "8")
  )
  (symbol (lib_id "74xx:74LS14") (at 369.57 420.37 180) (unit 6)
    (in_bom yes) (on_board yes)
    (property "Reference" "M5" (id 0) (at 365.76 414.02 0))
    (property "Value" "74LS14" (id 1) (at 365.76 416.56 0))
    (property "Footprint" "" (id 2) (at 369.57 420.37 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 369.57 420.37 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "Device:R_Network08") (at 557.53 530.86 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "RN?" (id 0) (at 569.8613 529.3359 0))
    (property "Value" "4.7k" (id 1) (at 569.8613 531.8759 0))
    (property "Footprint" "Resistor_THT:R_Array_SIP9" (id 2) (at 545.465 530.86 90))
    (property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf" (id 3) (at 557.53 530.86 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Simulation_SPICE:DIODE") (at 546.1 447.04 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "W2" (id 0) (at 539.75 447.04 0))
    (property "Value" " " (id 1) (at 546.1 443.23 0))
    (property "Footprint" "" (id 2) (at 546.1 447.04 0))
    (property "Datasheet" "~" (id 3) (at 546.1 447.04 0))
    (property "Spice_Netlist_Enabled" "Y" (id 4) (at 546.1 447.04 0))
    (property "Spice_Primitive" "D" (id 5) (at 546.1 447.04 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx_IEEE:7407") (at 398.78 298.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "M4" (id 0) (at 398.78 300.99 0))
    (property "Value" "7407" (id 1) (at 398.78 303.53 0))
    (property "Footprint" "" (id 2) (at 398.78 298.45 0))
    (property "Datasheet" "" (id 3) (at 398.78 298.45 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "MCU_Intel:8049") (at 524.51 407.67 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M1" (id 0) (at 526.5294 368.3 0))
    (property "Value" "8049" (id 1) (at 526.5294 370.84 0))
    (property "Footprint" "" (id 2) (at 524.51 402.59 0))
    (property "Datasheet" "" (id 3) (at 524.51 402.59 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "pspice:R") (at 429.26 323.85 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 429.26 317.5 90))
    (property "Value" "R" (id 1) (at 429.26 320.04 90))
    (property "Footprint" "" (id 2) (at 429.26 323.85 0))
    (property "Datasheet" "~" (id 3) (at 429.26 323.85 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Simulation_SPICE:DIODE") (at 546.1 444.5 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "W1" (id 0) (at 539.75 444.5 0))
    (property "Value" " " (id 1) (at 546.1 440.69 0))
    (property "Footprint" "" (id 2) (at 546.1 444.5 0))
    (property "Datasheet" "~" (id 3) (at 546.1 444.5 0))
    (property "Spice_Netlist_Enabled" "Y" (id 4) (at 546.1 444.5 0))
    (property "Spice_Primitive" "D" (id 5) (at 546.1 444.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 410.21 273.05 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 410.21 279.4 0))
    (property "Value" "GND" (id 1) (at 410.21 278.13 0))
    (property "Footprint" "" (id 2) (at 410.21 273.05 0))
    (property "Datasheet" "" (id 3) (at 410.21 273.05 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 501.65 322.58 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 501.65 326.39 0))
    (property "Value" "+5V" (id 1) (at 501.65 317.5 0))
    (property "Footprint" "" (id 2) (at 501.65 322.58 0))
    (property "Datasheet" "" (id 3) (at 501.65 322.58 0))
    (pin "1")
  )
  (symbol (lib_id "LED:LD271") (at 419.1 340.36 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 417.957 331.47 0))
    (property "Value" "ON LINE" (id 1) (at 417.957 334.01 0))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (id 2) (at 419.1 335.915 0))
    (property "Datasheet" "http://www.alliedelec.com/m/d/40788c34903a719969df15f1fbea1056.pdf" (id 3) (at 417.83 340.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "4xxx:4050") (at 577.85 506.73 0) (unit 6)
    (in_bom yes) (on_board yes)
    (property "Reference" "M7" (id 0) (at 576.58 505.46 0))
    (property "Value" "4050" (id 1) (at 576.58 508 0))
    (property "Footprint" "" (id 2) (at 577.85 506.73 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf" (id 3) (at 577.85 506.73 0))
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "14")
    (pin "15")
    (pin "1")
    (pin "8")
  )
  (symbol (lib_id "Simulation_SPICE:DIODE") (at 546.1 441.96 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "W0" (id 0) (at 539.75 441.96 0))
    (property "Value" " " (id 1) (at 546.1 438.15 0))
    (property "Footprint" "" (id 2) (at 546.1 441.96 0))
    (property "Datasheet" "~" (id 3) (at 546.1 441.96 0))
    (property "Spice_Netlist_Enabled" "Y" (id 4) (at 546.1 441.96 0))
    (property "Spice_Primitive" "D" (id 5) (at 546.1 441.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Simulation_SPICE:DIODE") (at 546.1 454.66 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "W5" (id 0) (at 539.75 454.66 0))
    (property "Value" " " (id 1) (at 546.1 450.85 0))
    (property "Footprint" "" (id 2) (at 546.1 454.66 0))
    (property "Datasheet" "~" (id 3) (at 546.1 454.66 0))
    (property "Spice_Netlist_Enabled" "Y" (id 4) (at 546.1 454.66 0))
    (property "Spice_Primitive" "D" (id 5) (at 546.1 454.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "LED:LD271") (at 419.1 354.33 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 417.957 345.44 0))
    (property "Value" "Not Used" (id 1) (at 417.957 347.98 0))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (id 2) (at 419.1 349.885 0))
    (property "Datasheet" "http://www.alliedelec.com/m/d/40788c34903a719969df15f1fbea1056.pdf" (id 3) (at 417.83 354.33 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 580.39 535.94 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 580.39 539.75 0))
    (property "Value" "+5V" (id 1) (at 580.39 530.86 0))
    (property "Footprint" "" (id 2) (at 580.39 535.94 0))
    (property "Datasheet" "" (id 3) (at 580.39 535.94 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS14") (at 430.53 438.15 0) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "M5" (id 0) (at 430.53 429.26 0))
    (property "Value" "74LS14" (id 1) (at 430.53 431.8 0))
    (property "Footprint" "" (id 2) (at 430.53 438.15 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 430.53 438.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74LS14") (at 369.57 429.26 180) (unit 5)
    (in_bom yes) (on_board yes)
    (property "Reference" "M5" (id 0) (at 365.76 422.91 0))
    (property "Value" "74LS14" (id 1) (at 365.76 425.45 0))
    (property "Footprint" "" (id 2) (at 369.57 429.26 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 369.57 429.26 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx_IEEE:7407") (at 398.78 340.36 0) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "M4" (id 0) (at 398.78 342.9 0))
    (property "Value" "7407" (id 1) (at 398.78 345.44 0))
    (property "Footprint" "" (id 2) (at 398.78 340.36 0))
    (property "Datasheet" "" (id 3) (at 398.78 340.36 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "74xx:74LS14") (at 403.86 490.22 0) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "M5" (id 0) (at 403.86 481.33 0))
    (property "Value" "74LS14" (id 1) (at 403.86 483.87 0))
    (property "Footprint" "" (id 2) (at 403.86 490.22 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS14" (id 3) (at 403.86 490.22 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx_IEEE:7407") (at 398.78 354.33 0) (unit 5)
    (in_bom yes) (on_board yes)
    (property "Reference" "M4" (id 0) (at 398.78 356.87 0))
    (property "Value" "7407" (id 1) (at 398.78 359.41 0))
    (property "Footprint" "" (id 2) (at 398.78 354.33 0))
    (property "Datasheet" "" (id 3) (at 398.78 354.33 0))
    (pin "14")
    (pin "7")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
  )
  (symbol (lib_id "4xxx:4050") (at 577.85 524.51 0) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "M7" (id 0) (at 576.58 523.24 0))
    (property "Value" "4050" (id 1) (at 576.58 525.78 0))
    (property "Footprint" "" (id 2) (at 577.85 524.51 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/intersil/documents/cd40/cd4050bms.pdf" (id 3) (at 577.85 524.51 0))
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "14")
    (pin "15")
    (pin "1")
    (pin "8")
  )
  (symbol (lib_id "pspice:R") (at 429.26 354.33 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 429.26 347.98 90))
    (property "Value" "R" (id 1) (at 429.26 350.52 90))
    (property "Footprint" "" (id 2) (at 429.26 354.33 0))
    (property "Datasheet" "~" (id 3) (at 429.26 354.33 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "BZ") (unit 1) (value "Buzzer") (footprint "")
    )
    (path
      (reference "D?") (unit 1) (value "HOLD") (footprint "LED_THT:LED_D5.0mm_IRGrey")
    )
    (path
      (reference "D?") (unit 1) (value "Num Lock") (footprint "LED_THT:LED_D5.0mm_IRGrey")
    )
    (path
      (reference "D?") (unit 1) (value "Alpha/Caps Lock") (footprint "LED_THT:LED_D5.0mm_IRGrey")
    )
    (path
      (reference "D?") (unit 1) (value "ON LINE") (footprint "LED_THT:LED_D5.0mm_IRGrey")
    )
    (path
      (reference "D?") (unit 1) (value "Not Used") (footprint "LED_THT:LED_D5.0mm_IRGrey")
    )
    (path
      (reference "J?") (unit 1) (value "DIN-8") (footprint "")
    )
    (path
      (reference "M1") (unit 1) (value "8049") (footprint "")
    )
    (path
      (reference "M2") (unit 1) (value "74LS145") (footprint "")
    )
    (path
      (reference "M3") (unit 1) (value "74LS145") (footprint "")
    )
    (path
      (reference "M4") (unit 1) (value "7407") (footprint "")
    )
    (path
      (reference "M4") (unit 2) (value "7407") (footprint "")
    )
    (path
      (reference "M4") (unit 3) (value "7407") (footprint "")
    )
    (path
      (reference "M4") (unit 4) (value "7407") (footprint "")
    )
    (path
      (reference "M4") (unit 5) (value "7407") (footprint "")
    )
    (path
      (reference "M4") (unit 6) (value "7407") (footprint "")
    )
    (path
      (reference "M5") (unit 1) (value "74LS14") (footprint "")
    )
    (path
      (reference "M5") (unit 2) (value "74LS14") (footprint "")
    )
    (path
      (reference "M5") (unit 3) (value "74LS14") (footprint "")
    )
    (path
      (reference "M5") (unit 4) (value "74LS14") (footprint "")
    )
    (path
      (reference "M5") (unit 5) (value "74LS14") (footprint "")
    )
    (path
      (reference "M5") (unit 6) (value "74LS14") (footprint "")
    )
    (path
      (reference "M6") (unit 1) (value "74LS38") (footprint "")
    )
    (path
      (reference "M6") (unit 2) (value "74LS38") (footprint "")
    )
    (path
      (reference "M6") (unit 3) (value "74LS38") (footprint "")
    )
    (path
      (reference "M6") (unit 4) (value "74LS38") (footprint "")
    )
    (path
      (reference "M7") (unit 1) (value "4050") (footprint "")
    )
    (path
      (reference "M7") (unit 2) (value "4050") (footprint "")
    )
    (path
      (reference "M7") (unit 3) (value "4050") (footprint "")
    )
    (path
      (reference "M7") (unit 4) (value "4050") (footprint "")
    )
    (path
      (reference "M7") (unit 5) (value "4050") (footprint "")
    )
    (path
      (reference "M7") (unit 6) (value "4050") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "R") (footprint "")
    )
    (path
      (reference "RN?") (unit 1) (value "4.7k") (footprint "Resistor_THT:R_Array_SIP9")
    )
    (path
      (reference "W0") (unit 1) (value " ") (footprint "")
    )
    (path
      (reference "W1") (unit 1) (value " ") (footprint "")
    )
    (path
      (reference "W2") (unit 1) (value " ") (footprint "")
    )
    (path
      (reference "W3") (unit 1) (value " ") (footprint "")
    )
    (path
      (reference "W4") (unit 1) (value " ") (footprint "")
    )
    (path
      (reference "W5") (unit 1) (value " ") (footprint "")
    )
    (path
      (reference "X1") (unit 1) (value "Crystal") (footprint "")
    )
  )
)
